\section{aversive\_\-10-03-12/include/aversive/parts/ATmega406.h File Reference}
\label{ATmega406_8h}\index{aversive\_\-10-03-12/include/aversive/parts/ATmega406.h@{aversive\_\-10-03-12/include/aversive/parts/ATmega406.h}}
\subsection*{Defines}
\begin{CompactItemize}
\item 
\#define {\bf TIMER0\_\-PRESCALER\_\-DIV\_\-0}~0
\item 
\#define {\bf TIMER0\_\-PRESCALER\_\-DIV\_\-1}~1
\item 
\#define {\bf TIMER0\_\-PRESCALER\_\-DIV\_\-8}~2
\item 
\#define {\bf TIMER0\_\-PRESCALER\_\-DIV\_\-64}~3
\item 
\#define {\bf TIMER0\_\-PRESCALER\_\-DIV\_\-256}~4
\item 
\#define {\bf TIMER0\_\-PRESCALER\_\-DIV\_\-1024}~5
\item 
\#define {\bf TIMER0\_\-PRESCALER\_\-DIV\_\-FALL}~6
\item 
\#define {\bf TIMER0\_\-PRESCALER\_\-DIV\_\-RISE}~7
\item 
\#define {\bf TIMER0\_\-PRESCALER\_\-REG\_\-0}~0
\item 
\#define {\bf TIMER0\_\-PRESCALER\_\-REG\_\-1}~1
\item 
\#define {\bf TIMER0\_\-PRESCALER\_\-REG\_\-2}~8
\item 
\#define {\bf TIMER0\_\-PRESCALER\_\-REG\_\-3}~64
\item 
\#define {\bf TIMER0\_\-PRESCALER\_\-REG\_\-4}~256
\item 
\#define {\bf TIMER0\_\-PRESCALER\_\-REG\_\-5}~1024
\item 
\#define {\bf TIMER0\_\-PRESCALER\_\-REG\_\-6}~-1
\item 
\#define {\bf TIMER0\_\-PRESCALER\_\-REG\_\-7}~-2
\item 
\#define {\bf TIMER1\_\-PRESCALER\_\-DIV\_\-0}~0
\item 
\#define {\bf TIMER1\_\-PRESCALER\_\-DIV\_\-1}~1
\item 
\#define {\bf TIMER1\_\-PRESCALER\_\-DIV\_\-8}~2
\item 
\#define {\bf TIMER1\_\-PRESCALER\_\-DIV\_\-32}~3
\item 
\#define {\bf TIMER1\_\-PRESCALER\_\-DIV\_\-64}~4
\item 
\#define {\bf TIMER1\_\-PRESCALER\_\-DIV\_\-128}~5
\item 
\#define {\bf TIMER1\_\-PRESCALER\_\-DIV\_\-256}~6
\item 
\#define {\bf TIMER1\_\-PRESCALER\_\-DIV\_\-1024}~7
\item 
\#define {\bf TIMER1\_\-PRESCALER\_\-REG\_\-0}~0
\item 
\#define {\bf TIMER1\_\-PRESCALER\_\-REG\_\-1}~1
\item 
\#define {\bf TIMER1\_\-PRESCALER\_\-REG\_\-2}~8
\item 
\#define {\bf TIMER1\_\-PRESCALER\_\-REG\_\-3}~32
\item 
\#define {\bf TIMER1\_\-PRESCALER\_\-REG\_\-4}~64
\item 
\#define {\bf TIMER1\_\-PRESCALER\_\-REG\_\-5}~128
\item 
\#define {\bf TIMER1\_\-PRESCALER\_\-REG\_\-6}~256
\item 
\#define {\bf TIMER1\_\-PRESCALER\_\-REG\_\-7}~1024
\item 
\#define {\bf SIG\_\-OVERFLOW\_\-TOTAL\_\-NUM}~0
\item 
\#define {\bf SIG\_\-OUTPUT\_\-COMPARE\_\-TOTAL\_\-NUM}~0
\item 
\#define {\bf PWM\_\-TOTAL\_\-NUM}~0
\item 
\#define {\bf SIG\_\-INPUT\_\-CAPTURE\_\-TOTAL\_\-NUM}~0
\item 
\#define {\bf CADAC16\_\-REG}~CADAC2
\item 
\#define {\bf CADAC17\_\-REG}~CADAC2
\item 
\#define {\bf CADAC18\_\-REG}~CADAC2
\item 
\#define {\bf CADAC19\_\-REG}~CADAC2
\item 
\#define {\bf CADAC20\_\-REG}~CADAC2
\item 
\#define {\bf CADAC21\_\-REG}~CADAC2
\item 
\#define {\bf CADAC22\_\-REG}~CADAC2
\item 
\#define {\bf CADAC23\_\-REG}~CADAC2
\item 
\#define {\bf CADAC24\_\-REG}~CADAC3
\item 
\#define {\bf CADAC25\_\-REG}~CADAC3
\item 
\#define {\bf CADAC26\_\-REG}~CADAC3
\item 
\#define {\bf CADAC27\_\-REG}~CADAC3
\item 
\#define {\bf CADAC28\_\-REG}~CADAC3
\item 
\#define {\bf CADAC29\_\-REG}~CADAC3
\item 
\#define {\bf CADAC30\_\-REG}~CADAC3
\item 
\#define {\bf CADAC31\_\-REG}~CADAC3
\item 
\#define {\bf CADAC00\_\-REG}~CADAC0
\item 
\#define {\bf CADAC01\_\-REG}~CADAC0
\item 
\#define {\bf CADAC02\_\-REG}~CADAC0
\item 
\#define {\bf CADAC03\_\-REG}~CADAC0
\item 
\#define {\bf CADAC04\_\-REG}~CADAC0
\item 
\#define {\bf CADAC05\_\-REG}~CADAC0
\item 
\#define {\bf CADAC06\_\-REG}~CADAC0
\item 
\#define {\bf CADAC07\_\-REG}~CADAC0
\item 
\#define {\bf CADAC08\_\-REG}~CADAC1
\item 
\#define {\bf CADAC09\_\-REG}~CADAC1
\item 
\#define {\bf CADAC10\_\-REG}~CADAC1
\item 
\#define {\bf CADAC11\_\-REG}~CADAC1
\item 
\#define {\bf CADAC12\_\-REG}~CADAC1
\item 
\#define {\bf CADAC13\_\-REG}~CADAC1
\item 
\#define {\bf CADAC14\_\-REG}~CADAC1
\item 
\#define {\bf CADAC15\_\-REG}~CADAC1
\item 
\#define {\bf EERE\_\-REG}~EECR
\item 
\#define {\bf EEPE\_\-REG}~EECR
\item 
\#define {\bf EEMPE\_\-REG}~EECR
\item 
\#define {\bf EERIE\_\-REG}~EECR
\item 
\#define {\bf EEPM0\_\-REG}~EECR
\item 
\#define {\bf EEPM1\_\-REG}~EECR
\item 
\#define {\bf PCIF0\_\-REG}~PCIFR
\item 
\#define {\bf PCIF1\_\-REG}~PCIFR
\item 
\#define {\bf WUTP0\_\-REG}~WUTCSR
\item 
\#define {\bf WUTP1\_\-REG}~WUTCSR
\item 
\#define {\bf WUTP2\_\-REG}~WUTCSR
\item 
\#define {\bf WUTE\_\-REG}~WUTCSR
\item 
\#define {\bf WUTR\_\-REG}~WUTCSR
\item 
\#define {\bf WUTCF\_\-REG}~WUTCSR
\item 
\#define {\bf WUTIE\_\-REG}~WUTCSR
\item 
\#define {\bf WUTIF\_\-REG}~WUTCSR
\item 
\#define {\bf C\_\-REG}~SREG
\item 
\#define {\bf Z\_\-REG}~SREG
\item 
\#define {\bf N\_\-REG}~SREG
\item 
\#define {\bf V\_\-REG}~SREG
\item 
\#define {\bf S\_\-REG}~SREG
\item 
\#define {\bf H\_\-REG}~SREG
\item 
\#define {\bf T\_\-REG}~SREG
\item 
\#define {\bf I\_\-REG}~SREG
\item 
\#define {\bf PCIE0\_\-REG}~PCICR
\item 
\#define {\bf PCIE1\_\-REG}~PCICR
\item 
\#define {\bf DDB0\_\-REG}~DDRB
\item 
\#define {\bf DDB1\_\-REG}~DDRB
\item 
\#define {\bf DDB2\_\-REG}~DDRB
\item 
\#define {\bf DDB3\_\-REG}~DDRB
\item 
\#define {\bf DDB4\_\-REG}~DDRB
\item 
\#define {\bf DDB5\_\-REG}~DDRB
\item 
\#define {\bf DDB6\_\-REG}~DDRB
\item 
\#define {\bf DDB7\_\-REG}~DDRB
\item 
\#define {\bf CCD\_\-REG}~BPCR
\item 
\#define {\bf DCD\_\-REG}~BPCR
\item 
\#define {\bf SCD\_\-REG}~BPCR
\item 
\#define {\bf DUVD\_\-REG}~BPCR
\item 
\#define {\bf WDP0\_\-REG}~WDTCSR
\item 
\#define {\bf WDP1\_\-REG}~WDTCSR
\item 
\#define {\bf WDP2\_\-REG}~WDTCSR
\item 
\#define {\bf WDE\_\-REG}~WDTCSR
\item 
\#define {\bf WDCE\_\-REG}~WDTCSR
\item 
\#define {\bf WDP3\_\-REG}~WDTCSR
\item 
\#define {\bf WDIE\_\-REG}~WDTCSR
\item 
\#define {\bf WDIF\_\-REG}~WDTCSR
\item 
\#define {\bf EEDR0\_\-REG}~EEDR
\item 
\#define {\bf EEDR1\_\-REG}~EEDR
\item 
\#define {\bf EEDR2\_\-REG}~EEDR
\item 
\#define {\bf EEDR3\_\-REG}~EEDR
\item 
\#define {\bf EEDR4\_\-REG}~EEDR
\item 
\#define {\bf EEDR5\_\-REG}~EEDR
\item 
\#define {\bf EEDR6\_\-REG}~EEDR
\item 
\#define {\bf EEDR7\_\-REG}~EEDR
\item 
\#define {\bf TWD0\_\-REG}~TWDR
\item 
\#define {\bf TWD1\_\-REG}~TWDR
\item 
\#define {\bf TWD2\_\-REG}~TWDR
\item 
\#define {\bf TWD3\_\-REG}~TWDR
\item 
\#define {\bf TWD4\_\-REG}~TWDR
\item 
\#define {\bf TWD5\_\-REG}~TWDR
\item 
\#define {\bf TWD6\_\-REG}~TWDR
\item 
\#define {\bf TWD7\_\-REG}~TWDR
\item 
\#define {\bf PIND0\_\-REG}~PIND
\item 
\#define {\bf PIND1\_\-REG}~PIND
\item 
\#define {\bf PSRSYNC\_\-REG}~GTCCR
\item 
\#define {\bf TSM\_\-REG}~GTCCR
\item 
\#define {\bf TWBR0\_\-REG}~TWBR
\item 
\#define {\bf TWBR1\_\-REG}~TWBR
\item 
\#define {\bf TWBR2\_\-REG}~TWBR
\item 
\#define {\bf TWBR3\_\-REG}~TWBR
\item 
\#define {\bf TWBR4\_\-REG}~TWBR
\item 
\#define {\bf TWBR5\_\-REG}~TWBR
\item 
\#define {\bf TWBR6\_\-REG}~TWBR
\item 
\#define {\bf TWBR7\_\-REG}~TWBR
\item 
\#define {\bf BGCR0\_\-REG}~BGCRR
\item 
\#define {\bf BGCR1\_\-REG}~BGCRR
\item 
\#define {\bf BGCR2\_\-REG}~BGCRR
\item 
\#define {\bf BGCR3\_\-REG}~BGCRR
\item 
\#define {\bf BGCR4\_\-REG}~BGCRR
\item 
\#define {\bf BGCR5\_\-REG}~BGCRR
\item 
\#define {\bf BGCR6\_\-REG}~BGCRR
\item 
\#define {\bf BGCR7\_\-REG}~BGCRR
\item 
\#define {\bf DDA0\_\-REG}~DDRA
\item 
\#define {\bf DDA1\_\-REG}~DDRA
\item 
\#define {\bf DDA2\_\-REG}~DDRA
\item 
\#define {\bf DDA3\_\-REG}~DDRA
\item 
\#define {\bf DDA4\_\-REG}~DDRA
\item 
\#define {\bf DDA5\_\-REG}~DDRA
\item 
\#define {\bf DDA6\_\-REG}~DDRA
\item 
\#define {\bf DDA7\_\-REG}~DDRA
\item 
\#define {\bf INT0\_\-REG}~EIMSK
\item 
\#define {\bf INT1\_\-REG}~EIMSK
\item 
\#define {\bf INT2\_\-REG}~EIMSK
\item 
\#define {\bf INT3\_\-REG}~EIMSK
\item 
\#define {\bf PRVADC\_\-REG}~PRR0
\item 
\#define {\bf PRTIM0\_\-REG}~PRR0
\item 
\#define {\bf PRTIM1\_\-REG}~PRR0
\item 
\#define {\bf PRTWI\_\-REG}~PRR0
\item 
\#define {\bf PCINT8\_\-REG}~PCMSK1
\item 
\#define {\bf PCINT9\_\-REG}~PCMSK1
\item 
\#define {\bf PCINT10\_\-REG}~PCMSK1
\item 
\#define {\bf PCINT11\_\-REG}~PCMSK1
\item 
\#define {\bf PCINT12\_\-REG}~PCMSK1
\item 
\#define {\bf PCINT13\_\-REG}~PCMSK1
\item 
\#define {\bf PCINT14\_\-REG}~PCMSK1
\item 
\#define {\bf PCINT15\_\-REG}~PCMSK1
\item 
\#define {\bf OCR0A0\_\-REG}~OCR0A
\item 
\#define {\bf OCR0A1\_\-REG}~OCR0A
\item 
\#define {\bf OCR0A2\_\-REG}~OCR0A
\item 
\#define {\bf OCR0A3\_\-REG}~OCR0A
\item 
\#define {\bf OCR0A4\_\-REG}~OCR0A
\item 
\#define {\bf OCR0A5\_\-REG}~OCR0A
\item 
\#define {\bf OCR0A6\_\-REG}~OCR0A
\item 
\#define {\bf OCR0A7\_\-REG}~OCR0A
\item 
\#define {\bf CCDL0\_\-REG}~BPOCD
\item 
\#define {\bf CCDL1\_\-REG}~BPOCD
\item 
\#define {\bf CCDL2\_\-REG}~BPOCD
\item 
\#define {\bf CCDL3\_\-REG}~BPOCD
\item 
\#define {\bf DCDL0\_\-REG}~BPOCD
\item 
\#define {\bf DCDL1\_\-REG}~BPOCD
\item 
\#define {\bf DCDL2\_\-REG}~BPOCD
\item 
\#define {\bf DCDL3\_\-REG}~BPOCD
\item 
\#define {\bf DDD0\_\-REG}~DDRD
\item 
\#define {\bf DDD1\_\-REG}~DDRD
\item 
\#define {\bf OCR0B0\_\-REG}~OCR0B
\item 
\#define {\bf OCR0B1\_\-REG}~OCR0B
\item 
\#define {\bf OCR0B2\_\-REG}~OCR0B
\item 
\#define {\bf OCR0B3\_\-REG}~OCR0B
\item 
\#define {\bf OCR0B4\_\-REG}~OCR0B
\item 
\#define {\bf OCR0B5\_\-REG}~OCR0B
\item 
\#define {\bf OCR0B6\_\-REG}~OCR0B
\item 
\#define {\bf OCR0B7\_\-REG}~OCR0B
\item 
\#define {\bf SP8\_\-REG}~SPH
\item 
\#define {\bf SP9\_\-REG}~SPH
\item 
\#define {\bf SP10\_\-REG}~SPH
\item 
\#define {\bf SP11\_\-REG}~SPH
\item 
\#define {\bf SP12\_\-REG}~SPH
\item 
\#define {\bf SP13\_\-REG}~SPH
\item 
\#define {\bf SP14\_\-REG}~SPH
\item 
\#define {\bf SP15\_\-REG}~SPH
\item 
\#define {\bf ACS\_\-REG}~CCSR
\item 
\#define {\bf XOE\_\-REG}~CCSR
\item 
\#define {\bf CADICH0\_\-REG}~CADICH
\item 
\#define {\bf CADICH1\_\-REG}~CADICH
\item 
\#define {\bf CADICH2\_\-REG}~CADICH
\item 
\#define {\bf CADICH3\_\-REG}~CADICH
\item 
\#define {\bf CADICH4\_\-REG}~CADICH
\item 
\#define {\bf CADICH5\_\-REG}~CADICH
\item 
\#define {\bf CADICH6\_\-REG}~CADICH
\item 
\#define {\bf CADICH7\_\-REG}~CADICH
\item 
\#define {\bf PFD\_\-REG}~FCSR
\item 
\#define {\bf CFE\_\-REG}~FCSR
\item 
\#define {\bf DFE\_\-REG}~FCSR
\item 
\#define {\bf CPS\_\-REG}~FCSR
\item 
\#define {\bf PWMOPC\_\-REG}~FCSR
\item 
\#define {\bf PWMOC\_\-REG}~FCSR
\item 
\#define {\bf SP0\_\-REG}~SPL
\item 
\#define {\bf SP1\_\-REG}~SPL
\item 
\#define {\bf SP2\_\-REG}~SPL
\item 
\#define {\bf SP3\_\-REG}~SPL
\item 
\#define {\bf SP4\_\-REG}~SPL
\item 
\#define {\bf SP5\_\-REG}~SPL
\item 
\#define {\bf SP6\_\-REG}~SPL
\item 
\#define {\bf SP7\_\-REG}~SPL
\item 
\#define {\bf CADICIF\_\-REG}~CADCSRB
\item 
\#define {\bf CADRCIF\_\-REG}~CADCSRB
\item 
\#define {\bf CADACIF\_\-REG}~CADCSRB
\item 
\#define {\bf CADICIE\_\-REG}~CADCSRB
\item 
\#define {\bf CADRCIE\_\-REG}~CADCSRB
\item 
\#define {\bf CADACIE\_\-REG}~CADCSRB
\item 
\#define {\bf CADICL0\_\-REG}~CADICL
\item 
\#define {\bf CADICL1\_\-REG}~CADICL
\item 
\#define {\bf CADICL2\_\-REG}~CADICL
\item 
\#define {\bf CADICL3\_\-REG}~CADICL
\item 
\#define {\bf CADICL4\_\-REG}~CADICL
\item 
\#define {\bf CADICL5\_\-REG}~CADICL
\item 
\#define {\bf CADICL6\_\-REG}~CADICL
\item 
\#define {\bf CADICL7\_\-REG}~CADICL
\item 
\#define {\bf SCIE\_\-REG}~BPIR
\item 
\#define {\bf DOCIE\_\-REG}~BPIR
\item 
\#define {\bf COCIE\_\-REG}~BPIR
\item 
\#define {\bf DUVIE\_\-REG}~BPIR
\item 
\#define {\bf SCIF\_\-REG}~BPIR
\item 
\#define {\bf DOCIF\_\-REG}~BPIR
\item 
\#define {\bf COCIF\_\-REG}~BPIR
\item 
\#define {\bf DUVIF\_\-REG}~BPIR
\item 
\#define {\bf GPIOR10\_\-REG}~GPIOR1
\item 
\#define {\bf GPIOR11\_\-REG}~GPIOR1
\item 
\#define {\bf GPIOR12\_\-REG}~GPIOR1
\item 
\#define {\bf GPIOR13\_\-REG}~GPIOR1
\item 
\#define {\bf GPIOR14\_\-REG}~GPIOR1
\item 
\#define {\bf GPIOR15\_\-REG}~GPIOR1
\item 
\#define {\bf GPIOR16\_\-REG}~GPIOR1
\item 
\#define {\bf GPIOR17\_\-REG}~GPIOR1
\item 
\#define {\bf BPPL\_\-REG}~BPPLR
\item 
\#define {\bf BPPLE\_\-REG}~BPPLR
\item 
\#define {\bf CS10\_\-REG}~TCCR1B
\item 
\#define {\bf CS11\_\-REG}~TCCR1B
\item 
\#define {\bf CS12\_\-REG}~TCCR1B
\item 
\#define {\bf CTC1\_\-REG}~TCCR1B
\item 
\#define {\bf PORF\_\-REG}~MCUSR
\item 
\#define {\bf EXTRF\_\-REG}~MCUSR
\item 
\#define {\bf BODRF\_\-REG}~MCUSR
\item 
\#define {\bf WDRF\_\-REG}~MCUSR
\item 
\#define {\bf JTRF\_\-REG}~MCUSR
\item 
\#define {\bf EEAR8\_\-REG}~EEARH
\item 
\#define {\bf OCPT0\_\-REG}~CBPTR
\item 
\#define {\bf OCPT1\_\-REG}~CBPTR
\item 
\#define {\bf OCPT2\_\-REG}~CBPTR
\item 
\#define {\bf OCPT3\_\-REG}~CBPTR
\item 
\#define {\bf SCPT0\_\-REG}~CBPTR
\item 
\#define {\bf SCPT1\_\-REG}~CBPTR
\item 
\#define {\bf SCPT2\_\-REG}~CBPTR
\item 
\#define {\bf SCPT3\_\-REG}~CBPTR
\item 
\#define {\bf SPMEN\_\-REG}~SPMCSR
\item 
\#define {\bf PGERS\_\-REG}~SPMCSR
\item 
\#define {\bf PGWRT\_\-REG}~SPMCSR
\item 
\#define {\bf BLBSET\_\-REG}~SPMCSR
\item 
\#define {\bf RWWSRE\_\-REG}~SPMCSR
\item 
\#define {\bf SIGRD\_\-REG}~SPMCSR
\item 
\#define {\bf RWWSB\_\-REG}~SPMCSR
\item 
\#define {\bf SPMIE\_\-REG}~SPMCSR
\item 
\#define {\bf CADSE\_\-REG}~CADCSRA
\item 
\#define {\bf CADSI0\_\-REG}~CADCSRA
\item 
\#define {\bf CADSI1\_\-REG}~CADCSRA
\item 
\#define {\bf CADAS0\_\-REG}~CADCSRA
\item 
\#define {\bf CADAS1\_\-REG}~CADCSRA
\item 
\#define {\bf CADUB\_\-REG}~CADCSRA
\item 
\#define {\bf CADEN\_\-REG}~CADCSRA
\item 
\#define {\bf DUDL0\_\-REG}~BPDUV
\item 
\#define {\bf DUDL1\_\-REG}~BPDUV
\item 
\#define {\bf DUDL2\_\-REG}~BPDUV
\item 
\#define {\bf DUDL3\_\-REG}~BPDUV
\item 
\#define {\bf DUVT0\_\-REG}~BPDUV
\item 
\#define {\bf DUVT1\_\-REG}~BPDUV
\item 
\#define {\bf CADRDC0\_\-REG}~CADRDC
\item 
\#define {\bf CADRDC1\_\-REG}~CADRDC
\item 
\#define {\bf CADRDC2\_\-REG}~CADRDC
\item 
\#define {\bf CADRDC3\_\-REG}~CADRDC
\item 
\#define {\bf CADRDC4\_\-REG}~CADRDC
\item 
\#define {\bf CADRDC5\_\-REG}~CADRDC
\item 
\#define {\bf CADRDC6\_\-REG}~CADRDC
\item 
\#define {\bf CADRDC7\_\-REG}~CADRDC
\item 
\#define {\bf TCNT1L0\_\-REG}~TCNT1L
\item 
\#define {\bf TCNT1L1\_\-REG}~TCNT1L
\item 
\#define {\bf TCNT1L2\_\-REG}~TCNT1L
\item 
\#define {\bf TCNT1L3\_\-REG}~TCNT1L
\item 
\#define {\bf TCNT1L4\_\-REG}~TCNT1L
\item 
\#define {\bf TCNT1L5\_\-REG}~TCNT1L
\item 
\#define {\bf TCNT1L6\_\-REG}~TCNT1L
\item 
\#define {\bf TCNT1L7\_\-REG}~TCNT1L
\item 
\#define {\bf PORTB0\_\-REG}~PORTB
\item 
\#define {\bf PORTB1\_\-REG}~PORTB
\item 
\#define {\bf PORTB2\_\-REG}~PORTB
\item 
\#define {\bf PORTB3\_\-REG}~PORTB
\item 
\#define {\bf PORTB4\_\-REG}~PORTB
\item 
\#define {\bf PORTB5\_\-REG}~PORTB
\item 
\#define {\bf PORTB6\_\-REG}~PORTB
\item 
\#define {\bf PORTB7\_\-REG}~PORTB
\item 
\#define {\bf PORTD0\_\-REG}~PORTD
\item 
\#define {\bf PORTD1\_\-REG}~PORTD
\item 
\#define {\bf SE\_\-REG}~SMCR
\item 
\#define {\bf SM0\_\-REG}~SMCR
\item 
\#define {\bf SM1\_\-REG}~SMCR
\item 
\#define {\bf SM2\_\-REG}~SMCR
\item 
\#define {\bf TCNT1H0\_\-REG}~TCNT1H
\item 
\#define {\bf TCNT1H1\_\-REG}~TCNT1H
\item 
\#define {\bf TCNT1H2\_\-REG}~TCNT1H
\item 
\#define {\bf TCNT1H3\_\-REG}~TCNT1H
\item 
\#define {\bf TCNT1H4\_\-REG}~TCNT1H
\item 
\#define {\bf TCNT1H5\_\-REG}~TCNT1H
\item 
\#define {\bf TCNT1H6\_\-REG}~TCNT1H
\item 
\#define {\bf TCNT1H7\_\-REG}~TCNT1H
\item 
\#define {\bf PORTC0\_\-REG}~PORTC
\item 
\#define {\bf TWAM0\_\-REG}~TWAMR
\item 
\#define {\bf TWAM1\_\-REG}~TWAMR
\item 
\#define {\bf TWAM2\_\-REG}~TWAMR
\item 
\#define {\bf TWAM3\_\-REG}~TWAMR
\item 
\#define {\bf TWAM4\_\-REG}~TWAMR
\item 
\#define {\bf TWAM5\_\-REG}~TWAMR
\item 
\#define {\bf TWAM6\_\-REG}~TWAMR
\item 
\#define {\bf PORTA0\_\-REG}~PORTA
\item 
\#define {\bf PORTA1\_\-REG}~PORTA
\item 
\#define {\bf PORTA2\_\-REG}~PORTA
\item 
\#define {\bf PORTA3\_\-REG}~PORTA
\item 
\#define {\bf PORTA4\_\-REG}~PORTA
\item 
\#define {\bf PORTA5\_\-REG}~PORTA
\item 
\#define {\bf PORTA6\_\-REG}~PORTA
\item 
\#define {\bf PORTA7\_\-REG}~PORTA
\item 
\#define {\bf TWIE\_\-REG}~TWCR
\item 
\#define {\bf TWEN\_\-REG}~TWCR
\item 
\#define {\bf TWWC\_\-REG}~TWCR
\item 
\#define {\bf TWSTO\_\-REG}~TWCR
\item 
\#define {\bf TWSTA\_\-REG}~TWCR
\item 
\#define {\bf TWEA\_\-REG}~TWCR
\item 
\#define {\bf TWINT\_\-REG}~TWCR
\item 
\#define {\bf SCDL0\_\-REG}~BPSCD
\item 
\#define {\bf SCDL1\_\-REG}~BPSCD
\item 
\#define {\bf SCDL2\_\-REG}~BPSCD
\item 
\#define {\bf SCDL3\_\-REG}~BPSCD
\item 
\#define {\bf TCNT00\_\-REG}~TCNT0
\item 
\#define {\bf TCNT01\_\-REG}~TCNT0
\item 
\#define {\bf TCNT02\_\-REG}~TCNT0
\item 
\#define {\bf TCNT03\_\-REG}~TCNT0
\item 
\#define {\bf TCNT04\_\-REG}~TCNT0
\item 
\#define {\bf TCNT05\_\-REG}~TCNT0
\item 
\#define {\bf TCNT06\_\-REG}~TCNT0
\item 
\#define {\bf TCNT07\_\-REG}~TCNT0
\item 
\#define {\bf PINA0\_\-REG}~PINA
\item 
\#define {\bf PINA1\_\-REG}~PINA
\item 
\#define {\bf PINA2\_\-REG}~PINA
\item 
\#define {\bf PINA3\_\-REG}~PINA
\item 
\#define {\bf PINA4\_\-REG}~PINA
\item 
\#define {\bf PINA5\_\-REG}~PINA
\item 
\#define {\bf PINA6\_\-REG}~PINA
\item 
\#define {\bf PINA7\_\-REG}~PINA
\item 
\#define {\bf OCR1AH0\_\-REG}~OCR1AH
\item 
\#define {\bf OCR1AH1\_\-REG}~OCR1AH
\item 
\#define {\bf OCR1AH2\_\-REG}~OCR1AH
\item 
\#define {\bf OCR1AH3\_\-REG}~OCR1AH
\item 
\#define {\bf OCR1AH4\_\-REG}~OCR1AH
\item 
\#define {\bf OCR1AH5\_\-REG}~OCR1AH
\item 
\#define {\bf OCR1AH6\_\-REG}~OCR1AH
\item 
\#define {\bf OCR1AH7\_\-REG}~OCR1AH
\item 
\#define {\bf TWGCE\_\-REG}~TWAR
\item 
\#define {\bf TWA0\_\-REG}~TWAR
\item 
\#define {\bf TWA1\_\-REG}~TWAR
\item 
\#define {\bf TWA2\_\-REG}~TWAR
\item 
\#define {\bf TWA3\_\-REG}~TWAR
\item 
\#define {\bf TWA4\_\-REG}~TWAR
\item 
\#define {\bf TWA5\_\-REG}~TWAR
\item 
\#define {\bf TWA6\_\-REG}~TWAR
\item 
\#define {\bf GPIOR00\_\-REG}~GPIOR0
\item 
\#define {\bf GPIOR01\_\-REG}~GPIOR0
\item 
\#define {\bf GPIOR02\_\-REG}~GPIOR0
\item 
\#define {\bf GPIOR03\_\-REG}~GPIOR0
\item 
\#define {\bf GPIOR04\_\-REG}~GPIOR0
\item 
\#define {\bf GPIOR05\_\-REG}~GPIOR0
\item 
\#define {\bf GPIOR06\_\-REG}~GPIOR0
\item 
\#define {\bf GPIOR07\_\-REG}~GPIOR0
\item 
\#define {\bf EEAR0\_\-REG}~EEARL
\item 
\#define {\bf EEAR1\_\-REG}~EEARL
\item 
\#define {\bf EEAR2\_\-REG}~EEARL
\item 
\#define {\bf EEAR3\_\-REG}~EEARL
\item 
\#define {\bf EEAR4\_\-REG}~EEARL
\item 
\#define {\bf EEAR5\_\-REG}~EEARL
\item 
\#define {\bf EEAR6\_\-REG}~EEARL
\item 
\#define {\bf EEAR7\_\-REG}~EEARL
\item 
\#define {\bf TOIE0\_\-REG}~TIMSK0
\item 
\#define {\bf OCIE0A\_\-REG}~TIMSK0
\item 
\#define {\bf OCIE0B\_\-REG}~TIMSK0
\item 
\#define {\bf TOIE1\_\-REG}~TIMSK1
\item 
\#define {\bf OCIE1A\_\-REG}~TIMSK1
\item 
\#define {\bf CS00\_\-REG}~TCCR0B
\item 
\#define {\bf CS01\_\-REG}~TCCR0B
\item 
\#define {\bf CS02\_\-REG}~TCCR0B
\item 
\#define {\bf WGM02\_\-REG}~TCCR0B
\item 
\#define {\bf FOC0B\_\-REG}~TCCR0B
\item 
\#define {\bf FOC0A\_\-REG}~TCCR0B
\item 
\#define {\bf BGCC0\_\-REG}~BGCCR
\item 
\#define {\bf BGCC1\_\-REG}~BGCCR
\item 
\#define {\bf BGCC2\_\-REG}~BGCCR
\item 
\#define {\bf BGCC3\_\-REG}~BGCCR
\item 
\#define {\bf BGCC4\_\-REG}~BGCCR
\item 
\#define {\bf BGCC5\_\-REG}~BGCCR
\item 
\#define {\bf BGD\_\-REG}~BGCCR
\item 
\#define {\bf VADMUX0\_\-REG}~VADMUX
\item 
\#define {\bf VADMUX1\_\-REG}~VADMUX
\item 
\#define {\bf VADMUX2\_\-REG}~VADMUX
\item 
\#define {\bf VADMUX3\_\-REG}~VADMUX
\item 
\#define {\bf TWPS0\_\-REG}~TWSR
\item 
\#define {\bf TWPS1\_\-REG}~TWSR
\item 
\#define {\bf TWS3\_\-REG}~TWSR
\item 
\#define {\bf TWS4\_\-REG}~TWSR
\item 
\#define {\bf TWS5\_\-REG}~TWSR
\item 
\#define {\bf TWS6\_\-REG}~TWSR
\item 
\#define {\bf TWS7\_\-REG}~TWSR
\item 
\#define {\bf VADC8\_\-REG}~VADCH
\item 
\#define {\bf VADC9\_\-REG}~VADCH
\item 
\#define {\bf VADC10\_\-REG}~VADCH
\item 
\#define {\bf VADC11\_\-REG}~VADCH
\item 
\#define {\bf GPIOR20\_\-REG}~GPIOR2
\item 
\#define {\bf GPIOR21\_\-REG}~GPIOR2
\item 
\#define {\bf GPIOR22\_\-REG}~GPIOR2
\item 
\#define {\bf GPIOR23\_\-REG}~GPIOR2
\item 
\#define {\bf GPIOR24\_\-REG}~GPIOR2
\item 
\#define {\bf GPIOR25\_\-REG}~GPIOR2
\item 
\#define {\bf GPIOR26\_\-REG}~GPIOR2
\item 
\#define {\bf GPIOR27\_\-REG}~GPIOR2
\item 
\#define {\bf PCINT0\_\-REG}~PCMSK0
\item 
\#define {\bf PCINT1\_\-REG}~PCMSK0
\item 
\#define {\bf PCINT2\_\-REG}~PCMSK0
\item 
\#define {\bf PCINT3\_\-REG}~PCMSK0
\item 
\#define {\bf PCINT4\_\-REG}~PCMSK0
\item 
\#define {\bf PCINT5\_\-REG}~PCMSK0
\item 
\#define {\bf PCINT6\_\-REG}~PCMSK0
\item 
\#define {\bf PCINT7\_\-REG}~PCMSK0
\item 
\#define {\bf VADC0\_\-REG}~VADCL
\item 
\#define {\bf VADC1\_\-REG}~VADCL
\item 
\#define {\bf VADC2\_\-REG}~VADCL
\item 
\#define {\bf VADC3\_\-REG}~VADCL
\item 
\#define {\bf VADC4\_\-REG}~VADCL
\item 
\#define {\bf VADC5\_\-REG}~VADCL
\item 
\#define {\bf VADC6\_\-REG}~VADCL
\item 
\#define {\bf VADC7\_\-REG}~VADCL
\item 
\#define {\bf ISC00\_\-REG}~EICRA
\item 
\#define {\bf ISC01\_\-REG}~EICRA
\item 
\#define {\bf ISC10\_\-REG}~EICRA
\item 
\#define {\bf ISC11\_\-REG}~EICRA
\item 
\#define {\bf ISC20\_\-REG}~EICRA
\item 
\#define {\bf ISC21\_\-REG}~EICRA
\item 
\#define {\bf ISC30\_\-REG}~EICRA
\item 
\#define {\bf ISC31\_\-REG}~EICRA
\item 
\#define {\bf VADCCIE\_\-REG}~VADCSR
\item 
\#define {\bf VADCCIF\_\-REG}~VADCSR
\item 
\#define {\bf VADSC\_\-REG}~VADCSR
\item 
\#define {\bf VADEN\_\-REG}~VADCSR
\item 
\#define {\bf FCAL0\_\-REG}~FOSCCAL
\item 
\#define {\bf FCAL1\_\-REG}~FOSCCAL
\item 
\#define {\bf FCAL2\_\-REG}~FOSCCAL
\item 
\#define {\bf FCAL3\_\-REG}~FOSCCAL
\item 
\#define {\bf FCAL4\_\-REG}~FOSCCAL
\item 
\#define {\bf FCAL5\_\-REG}~FOSCCAL
\item 
\#define {\bf FCAL6\_\-REG}~FOSCCAL
\item 
\#define {\bf FCAL7\_\-REG}~FOSCCAL
\item 
\#define {\bf VADC0D\_\-REG}~DIDR0
\item 
\#define {\bf VADC1D\_\-REG}~DIDR0
\item 
\#define {\bf VADC2D\_\-REG}~DIDR0
\item 
\#define {\bf VADC3D\_\-REG}~DIDR0
\item 
\#define {\bf WGM00\_\-REG}~TCCR0A
\item 
\#define {\bf WGM01\_\-REG}~TCCR0A
\item 
\#define {\bf COM0B0\_\-REG}~TCCR0A
\item 
\#define {\bf COM0B1\_\-REG}~TCCR0A
\item 
\#define {\bf COM0A0\_\-REG}~TCCR0A
\item 
\#define {\bf COM0A1\_\-REG}~TCCR0A
\item 
\#define {\bf IVCE\_\-REG}~MCUCR
\item 
\#define {\bf IVSEL\_\-REG}~MCUCR
\item 
\#define {\bf PUD\_\-REG}~MCUCR
\item 
\#define {\bf JTD\_\-REG}~MCUCR
\item 
\#define {\bf CBE1\_\-REG}~CBCR
\item 
\#define {\bf CBE2\_\-REG}~CBCR
\item 
\#define {\bf CBE3\_\-REG}~CBCR
\item 
\#define {\bf CBE4\_\-REG}~CBCR
\item 
\#define {\bf TWBCIP\_\-REG}~TWBCSR
\item 
\#define {\bf TWBDT0\_\-REG}~TWBCSR
\item 
\#define {\bf TWBDT1\_\-REG}~TWBCSR
\item 
\#define {\bf TWBCIE\_\-REG}~TWBCSR
\item 
\#define {\bf TWBCIF\_\-REG}~TWBCSR
\item 
\#define {\bf OCR1AL0\_\-REG}~OCR1AL
\item 
\#define {\bf OCR1AL1\_\-REG}~OCR1AL
\item 
\#define {\bf OCR1AL2\_\-REG}~OCR1AL
\item 
\#define {\bf OCR1AL3\_\-REG}~OCR1AL
\item 
\#define {\bf OCR1AL4\_\-REG}~OCR1AL
\item 
\#define {\bf OCR1AL5\_\-REG}~OCR1AL
\item 
\#define {\bf OCR1AL6\_\-REG}~OCR1AL
\item 
\#define {\bf OCR1AL7\_\-REG}~OCR1AL
\item 
\#define {\bf CADRCC0\_\-REG}~CADRCC
\item 
\#define {\bf CADRCC1\_\-REG}~CADRCC
\item 
\#define {\bf CADRCC2\_\-REG}~CADRCC
\item 
\#define {\bf CADRCC3\_\-REG}~CADRCC
\item 
\#define {\bf CADRCC4\_\-REG}~CADRCC
\item 
\#define {\bf CADRCC5\_\-REG}~CADRCC
\item 
\#define {\bf CADRCC6\_\-REG}~CADRCC
\item 
\#define {\bf CADRCC7\_\-REG}~CADRCC
\item 
\#define {\bf PINB0\_\-REG}~PINB
\item 
\#define {\bf PINB1\_\-REG}~PINB
\item 
\#define {\bf PINB2\_\-REG}~PINB
\item 
\#define {\bf PINB3\_\-REG}~PINB
\item 
\#define {\bf PINB4\_\-REG}~PINB
\item 
\#define {\bf PINB5\_\-REG}~PINB
\item 
\#define {\bf PINB6\_\-REG}~PINB
\item 
\#define {\bf PINB7\_\-REG}~PINB
\item 
\#define {\bf INTF0\_\-REG}~EIFR
\item 
\#define {\bf INTF1\_\-REG}~EIFR
\item 
\#define {\bf INTF2\_\-REG}~EIFR
\item 
\#define {\bf INTF3\_\-REG}~EIFR
\item 
\#define {\bf TOV0\_\-REG}~TIFR0
\item 
\#define {\bf OCF0A\_\-REG}~TIFR0
\item 
\#define {\bf OCF0B\_\-REG}~TIFR0
\item 
\#define {\bf TOV1\_\-REG}~TIFR1
\item 
\#define {\bf OCF1A\_\-REG}~TIFR1
\item 
\#define {\bf ADC0\_\-PORT}~PORTA
\item 
\#define {\bf ADC0\_\-BIT}~0
\item 
\#define {\bf PCINT0\_\-PORT}~PORTA
\item 
\#define {\bf PCINT0\_\-BIT}~0
\item 
\#define {\bf ADC1\_\-PORT}~PORTA
\item 
\#define {\bf ADC1\_\-BIT}~1
\item 
\#define {\bf PCINT1\_\-PORT}~PORTA
\item 
\#define {\bf PCINT1\_\-BIT}~1
\item 
\#define {\bf ADC2\_\-PORT}~PORTA
\item 
\#define {\bf ADC2\_\-BIT}~2
\item 
\#define {\bf PCINT2\_\-PORT}~PORTA
\item 
\#define {\bf PCINT2\_\-BIT}~2
\item 
\#define {\bf ADC3\_\-PORT}~PORTA
\item 
\#define {\bf ADC3\_\-BIT}~3
\item 
\#define {\bf PCINT3\_\-PORT}~PORTA
\item 
\#define {\bf PCINT3\_\-BIT}~3
\item 
\#define {\bf ADC4\_\-PORT}~PORTA
\item 
\#define {\bf ADC4\_\-BIT}~4
\item 
\#define {\bf INT0\_\-PORT}~PORTA
\item 
\#define {\bf INT0\_\-BIT}~4
\item 
\#define {\bf PCINT4\_\-PORT}~PORTA
\item 
\#define {\bf PCINT4\_\-BIT}~4
\item 
\#define {\bf INT1\_\-PORT}~PORTA
\item 
\#define {\bf INT1\_\-BIT}~5
\item 
\#define {\bf PCINT5\_\-PORT}~PORTA
\item 
\#define {\bf PCINT5\_\-BIT}~5
\item 
\#define {\bf INT2\_\-PORT}~PORTA
\item 
\#define {\bf INT2\_\-BIT}~6
\item 
\#define {\bf PCINT6\_\-PORT}~PORTA
\item 
\#define {\bf PCINT6\_\-BIT}~6
\item 
\#define {\bf INT3\_\-PORT}~PORTA
\item 
\#define {\bf INT3\_\-BIT}~7
\item 
\#define {\bf PCINT7\_\-PORT}~PORTA
\item 
\#define {\bf PCINT7\_\-BIT}~7
\item 
\#define {\bf TDO\_\-PORT}~PORTB
\item 
\#define {\bf TDO\_\-BIT}~0
\item 
\#define {\bf PCINT8\_\-PORT}~PORTB
\item 
\#define {\bf PCINT8\_\-BIT}~0
\item 
\#define {\bf TDI\_\-PORT}~PORTB
\item 
\#define {\bf TDI\_\-BIT}~1
\item 
\#define {\bf PCINT9\_\-PORT}~PORTB
\item 
\#define {\bf PCINT9\_\-BIT}~1
\item 
\#define {\bf TMS\_\-PORT}~PORTB
\item 
\#define {\bf TMS\_\-BIT}~2
\item 
\#define {\bf PCINT10\_\-PORT}~PORTB
\item 
\#define {\bf PCINT10\_\-BIT}~2
\item 
\#define {\bf TCK\_\-PORT}~PORTB
\item 
\#define {\bf TCK\_\-BIT}~3
\item 
\#define {\bf PCINT11\_\-PORT}~PORTB
\item 
\#define {\bf PCINT11\_\-BIT}~3
\item 
\#define {\bf PCINT12\_\-PORT}~PORTB
\item 
\#define {\bf PCINT12\_\-BIT}~4
\item 
\#define {\bf PCINT13\_\-PORT}~PORTB
\item 
\#define {\bf PCINT13\_\-BIT}~5
\item 
\#define {\bf OC0A\_\-PORT}~PORTB
\item 
\#define {\bf OC0A\_\-BIT}~6
\item 
\#define {\bf PCINT14\_\-PORT}~PORTB
\item 
\#define {\bf PCINT14\_\-BIT}~6
\item 
\#define {\bf OC0B\_\-PORT}~PORTB
\item 
\#define {\bf OC0B\_\-BIT}~7
\item 
\#define {\bf PCINT15\_\-PORT}~PORTB
\item 
\#define {\bf PCINT15\_\-BIT}~7
\item 
\#define {\bf T0\_\-PORT}~PORTD
\item 
\#define {\bf T0\_\-BIT}~0
\end{CompactItemize}


\subsection{Define Documentation}
\index{ATmega406.h@{ATmega406.h}!ACS\_\-REG@{ACS\_\-REG}}
\index{ACS\_\-REG@{ACS\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[ACS\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define ACS\_\-REG~CCSR}\label{ATmega406_8h_bfe55dcfbd97fad5bf6082377b65260d}




Definition at line 308 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ADC0\_\-BIT@{ADC0\_\-BIT}}
\index{ADC0\_\-BIT@{ADC0\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[ADC0\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define ADC0\_\-BIT~0}\label{ATmega406_8h_7206c4bd8a6f4a826f3335983cd2f20a}




Definition at line 764 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ADC0\_\-PORT@{ADC0\_\-PORT}}
\index{ADC0\_\-PORT@{ADC0\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[ADC0\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define ADC0\_\-PORT~PORTA}\label{ATmega406_8h_030fbd74b964f9c0046a74f46a42276b}




Definition at line 763 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ADC1\_\-BIT@{ADC1\_\-BIT}}
\index{ADC1\_\-BIT@{ADC1\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[ADC1\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define ADC1\_\-BIT~1}\label{ATmega406_8h_e40ddcc3aacadf79ae2deb704f36a98e}




Definition at line 769 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ADC1\_\-PORT@{ADC1\_\-PORT}}
\index{ADC1\_\-PORT@{ADC1\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[ADC1\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define ADC1\_\-PORT~PORTA}\label{ATmega406_8h_a6c3631acac5f073bdc845e9163bc14e}




Definition at line 768 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ADC2\_\-BIT@{ADC2\_\-BIT}}
\index{ADC2\_\-BIT@{ADC2\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[ADC2\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define ADC2\_\-BIT~2}\label{ATmega406_8h_89fb449e9a1d85f77b89c966a0557fc0}




Definition at line 774 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ADC2\_\-PORT@{ADC2\_\-PORT}}
\index{ADC2\_\-PORT@{ADC2\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[ADC2\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define ADC2\_\-PORT~PORTA}\label{ATmega406_8h_e922961d5006c209ce0dc927418f3a8c}




Definition at line 773 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ADC3\_\-BIT@{ADC3\_\-BIT}}
\index{ADC3\_\-BIT@{ADC3\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[ADC3\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define ADC3\_\-BIT~3}\label{ATmega406_8h_402e4e450020f46ebfcacc50160229de}




Definition at line 779 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ADC3\_\-PORT@{ADC3\_\-PORT}}
\index{ADC3\_\-PORT@{ADC3\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[ADC3\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define ADC3\_\-PORT~PORTA}\label{ATmega406_8h_4dc2e1861decdb9984d788cdfce21363}




Definition at line 778 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ADC4\_\-BIT@{ADC4\_\-BIT}}
\index{ADC4\_\-BIT@{ADC4\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[ADC4\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define ADC4\_\-BIT~4}\label{ATmega406_8h_c9da02f14e6beba592e365d8f0d11e1c}




Definition at line 784 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ADC4\_\-PORT@{ADC4\_\-PORT}}
\index{ADC4\_\-PORT@{ADC4\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[ADC4\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define ADC4\_\-PORT~PORTA}\label{ATmega406_8h_1bd33c991b2d830d62695ab6d22f0b4d}




Definition at line 783 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BGCC0\_\-REG@{BGCC0\_\-REG}}
\index{BGCC0\_\-REG@{BGCC0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BGCC0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BGCC0\_\-REG~BGCCR}\label{ATmega406_8h_44dc2f012a6a4c44d21d6a2119c163de}




Definition at line 599 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BGCC1\_\-REG@{BGCC1\_\-REG}}
\index{BGCC1\_\-REG@{BGCC1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BGCC1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BGCC1\_\-REG~BGCCR}\label{ATmega406_8h_bee20f1580e4c0fa96f5bea11ea4c18a}




Definition at line 600 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BGCC2\_\-REG@{BGCC2\_\-REG}}
\index{BGCC2\_\-REG@{BGCC2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BGCC2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BGCC2\_\-REG~BGCCR}\label{ATmega406_8h_d55eb244e9edb9ef576cb731fa5b5df9}




Definition at line 601 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BGCC3\_\-REG@{BGCC3\_\-REG}}
\index{BGCC3\_\-REG@{BGCC3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BGCC3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BGCC3\_\-REG~BGCCR}\label{ATmega406_8h_32d38e1c50155c131e3102cbdcdcfab5}




Definition at line 602 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BGCC4\_\-REG@{BGCC4\_\-REG}}
\index{BGCC4\_\-REG@{BGCC4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BGCC4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BGCC4\_\-REG~BGCCR}\label{ATmega406_8h_3f025089210103140d05775167ed2958}




Definition at line 603 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BGCC5\_\-REG@{BGCC5\_\-REG}}
\index{BGCC5\_\-REG@{BGCC5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BGCC5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BGCC5\_\-REG~BGCCR}\label{ATmega406_8h_da3f350ca4efb74b9d8599d93eb09020}




Definition at line 604 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BGCR0\_\-REG@{BGCR0\_\-REG}}
\index{BGCR0\_\-REG@{BGCR0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BGCR0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BGCR0\_\-REG~BGCRR}\label{ATmega406_8h_6856612127bd51a1750370b861b61f4c}




Definition at line 222 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BGCR1\_\-REG@{BGCR1\_\-REG}}
\index{BGCR1\_\-REG@{BGCR1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BGCR1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BGCR1\_\-REG~BGCRR}\label{ATmega406_8h_62c23db1eedc975d5d10e537f339a97f}




Definition at line 223 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BGCR2\_\-REG@{BGCR2\_\-REG}}
\index{BGCR2\_\-REG@{BGCR2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BGCR2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BGCR2\_\-REG~BGCRR}\label{ATmega406_8h_5a2b96f1260fd6490f5a156de5319af5}




Definition at line 224 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BGCR3\_\-REG@{BGCR3\_\-REG}}
\index{BGCR3\_\-REG@{BGCR3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BGCR3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BGCR3\_\-REG~BGCRR}\label{ATmega406_8h_b87f25a21bfd000ec598024ae94e1a7e}




Definition at line 225 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BGCR4\_\-REG@{BGCR4\_\-REG}}
\index{BGCR4\_\-REG@{BGCR4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BGCR4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BGCR4\_\-REG~BGCRR}\label{ATmega406_8h_2d8f0ad1301e7b48ad6a5d9d4a4951ed}




Definition at line 226 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BGCR5\_\-REG@{BGCR5\_\-REG}}
\index{BGCR5\_\-REG@{BGCR5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BGCR5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BGCR5\_\-REG~BGCRR}\label{ATmega406_8h_18e68ba0eddeade9c2ca04b3cbcb9011}




Definition at line 227 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BGCR6\_\-REG@{BGCR6\_\-REG}}
\index{BGCR6\_\-REG@{BGCR6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BGCR6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BGCR6\_\-REG~BGCRR}\label{ATmega406_8h_53d007e81aabf42b3a11a4018cc6ca31}




Definition at line 228 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BGCR7\_\-REG@{BGCR7\_\-REG}}
\index{BGCR7\_\-REG@{BGCR7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BGCR7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BGCR7\_\-REG~BGCRR}\label{ATmega406_8h_d3e4fb39fb199713b9b06fbb1b8e500a}




Definition at line 229 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BGD\_\-REG@{BGD\_\-REG}}
\index{BGD\_\-REG@{BGD\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BGD\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BGD\_\-REG~BGCCR}\label{ATmega406_8h_d3010b5f4278168974702162b70abb45}




Definition at line 605 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BLBSET\_\-REG@{BLBSET\_\-REG}}
\index{BLBSET\_\-REG@{BLBSET\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BLBSET\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BLBSET\_\-REG~SPMCSR}\label{ATmega406_8h_7c8a500e5b966a8af0033b0bd9b3dd23}




Definition at line 411 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BODRF\_\-REG@{BODRF\_\-REG}}
\index{BODRF\_\-REG@{BODRF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BODRF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BODRF\_\-REG~MCUSR}\label{ATmega406_8h_c3568c9803c3b4fe985509273a9a880a}




Definition at line 390 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BPPL\_\-REG@{BPPL\_\-REG}}
\index{BPPL\_\-REG@{BPPL\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BPPL\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BPPL\_\-REG~BPPLR}\label{ATmega406_8h_dd67fa6591e8e4d72fa628d48aa2b4a6}




Definition at line 378 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!BPPLE\_\-REG@{BPPLE\_\-REG}}
\index{BPPLE\_\-REG@{BPPLE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[BPPLE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define BPPLE\_\-REG~BPPLR}\label{ATmega406_8h_f2aa8dfe03f0e7fec1db879223d96e76}




Definition at line 379 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!C\_\-REG@{C\_\-REG}}
\index{C\_\-REG@{C\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[C\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define C\_\-REG~SREG}\label{ATmega406_8h_5335949b52f31553bda075c17e0de4d8}




Definition at line 144 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC00\_\-REG@{CADAC00\_\-REG}}
\index{CADAC00\_\-REG@{CADAC00\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC00\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC00\_\-REG~CADAC0}\label{ATmega406_8h_5aafa50f4b50af5689d039bf661f0312}




Definition at line 102 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC01\_\-REG@{CADAC01\_\-REG}}
\index{CADAC01\_\-REG@{CADAC01\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC01\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC01\_\-REG~CADAC0}\label{ATmega406_8h_e87ce8993cdd5c0e84c3701e66a3863b}




Definition at line 103 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC02\_\-REG@{CADAC02\_\-REG}}
\index{CADAC02\_\-REG@{CADAC02\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC02\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC02\_\-REG~CADAC0}\label{ATmega406_8h_34adace11b7f56974c9248db5f7e799e}




Definition at line 104 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC03\_\-REG@{CADAC03\_\-REG}}
\index{CADAC03\_\-REG@{CADAC03\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC03\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC03\_\-REG~CADAC0}\label{ATmega406_8h_2203de9d8e17c9c0ebe9c705ce20eb99}




Definition at line 105 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC04\_\-REG@{CADAC04\_\-REG}}
\index{CADAC04\_\-REG@{CADAC04\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC04\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC04\_\-REG~CADAC0}\label{ATmega406_8h_ef5f92bc881f07d5cc09c94b6565a9f7}




Definition at line 106 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC05\_\-REG@{CADAC05\_\-REG}}
\index{CADAC05\_\-REG@{CADAC05\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC05\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC05\_\-REG~CADAC0}\label{ATmega406_8h_7fa8bd351c4641f937317d57787436b9}




Definition at line 107 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC06\_\-REG@{CADAC06\_\-REG}}
\index{CADAC06\_\-REG@{CADAC06\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC06\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC06\_\-REG~CADAC0}\label{ATmega406_8h_a2db263743269c904d09d06483aeac63}




Definition at line 108 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC07\_\-REG@{CADAC07\_\-REG}}
\index{CADAC07\_\-REG@{CADAC07\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC07\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC07\_\-REG~CADAC0}\label{ATmega406_8h_67b83d5816162d08fedc586c99a08954}




Definition at line 109 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC08\_\-REG@{CADAC08\_\-REG}}
\index{CADAC08\_\-REG@{CADAC08\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC08\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC08\_\-REG~CADAC1}\label{ATmega406_8h_78241e8866513442f2528fb011c3775f}




Definition at line 112 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC09\_\-REG@{CADAC09\_\-REG}}
\index{CADAC09\_\-REG@{CADAC09\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC09\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC09\_\-REG~CADAC1}\label{ATmega406_8h_73d23b1336b2d74cd5780d59e2404ec8}




Definition at line 113 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC10\_\-REG@{CADAC10\_\-REG}}
\index{CADAC10\_\-REG@{CADAC10\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC10\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC10\_\-REG~CADAC1}\label{ATmega406_8h_74fa69ee83a5a8a589196f3f95a1c839}




Definition at line 114 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC11\_\-REG@{CADAC11\_\-REG}}
\index{CADAC11\_\-REG@{CADAC11\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC11\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC11\_\-REG~CADAC1}\label{ATmega406_8h_a6d4752031ade4d1823fa6c9866e9483}




Definition at line 115 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC12\_\-REG@{CADAC12\_\-REG}}
\index{CADAC12\_\-REG@{CADAC12\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC12\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC12\_\-REG~CADAC1}\label{ATmega406_8h_e12d5c64b30c8e1b5dafb6cfc09666bd}




Definition at line 116 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC13\_\-REG@{CADAC13\_\-REG}}
\index{CADAC13\_\-REG@{CADAC13\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC13\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC13\_\-REG~CADAC1}\label{ATmega406_8h_14b7248c87cf0372e0324385e7e003f0}




Definition at line 117 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC14\_\-REG@{CADAC14\_\-REG}}
\index{CADAC14\_\-REG@{CADAC14\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC14\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC14\_\-REG~CADAC1}\label{ATmega406_8h_091c22ac7190c4425a08e72532332d99}




Definition at line 118 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC15\_\-REG@{CADAC15\_\-REG}}
\index{CADAC15\_\-REG@{CADAC15\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC15\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC15\_\-REG~CADAC1}\label{ATmega406_8h_d301045ac018af6672c4573e43db2269}




Definition at line 119 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC16\_\-REG@{CADAC16\_\-REG}}
\index{CADAC16\_\-REG@{CADAC16\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC16\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC16\_\-REG~CADAC2}\label{ATmega406_8h_ff2280e964b0fe32a1cf64eceede52b1}




Definition at line 82 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC17\_\-REG@{CADAC17\_\-REG}}
\index{CADAC17\_\-REG@{CADAC17\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC17\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC17\_\-REG~CADAC2}\label{ATmega406_8h_01a1599bbd80e65207de8f90cca7737c}




Definition at line 83 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC18\_\-REG@{CADAC18\_\-REG}}
\index{CADAC18\_\-REG@{CADAC18\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC18\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC18\_\-REG~CADAC2}\label{ATmega406_8h_ef7be483a4959d6c1c4671cf0101f336}




Definition at line 84 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC19\_\-REG@{CADAC19\_\-REG}}
\index{CADAC19\_\-REG@{CADAC19\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC19\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC19\_\-REG~CADAC2}\label{ATmega406_8h_9163cf03396eaf28e22feeac4fe81604}




Definition at line 85 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC20\_\-REG@{CADAC20\_\-REG}}
\index{CADAC20\_\-REG@{CADAC20\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC20\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC20\_\-REG~CADAC2}\label{ATmega406_8h_b4192fd04fe7ec8db57ba09fa9d61d50}




Definition at line 86 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC21\_\-REG@{CADAC21\_\-REG}}
\index{CADAC21\_\-REG@{CADAC21\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC21\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC21\_\-REG~CADAC2}\label{ATmega406_8h_5e442473ddb9a2e7990ff544fed9ef82}




Definition at line 87 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC22\_\-REG@{CADAC22\_\-REG}}
\index{CADAC22\_\-REG@{CADAC22\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC22\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC22\_\-REG~CADAC2}\label{ATmega406_8h_38bc44df8c28f95faea87185b7519a10}




Definition at line 88 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC23\_\-REG@{CADAC23\_\-REG}}
\index{CADAC23\_\-REG@{CADAC23\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC23\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC23\_\-REG~CADAC2}\label{ATmega406_8h_6db32352589389a2113b16a5171d29e5}




Definition at line 89 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC24\_\-REG@{CADAC24\_\-REG}}
\index{CADAC24\_\-REG@{CADAC24\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC24\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC24\_\-REG~CADAC3}\label{ATmega406_8h_9861bf645745e2ad1f82dffebf0488a0}




Definition at line 92 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC25\_\-REG@{CADAC25\_\-REG}}
\index{CADAC25\_\-REG@{CADAC25\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC25\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC25\_\-REG~CADAC3}\label{ATmega406_8h_09e60d378687a2b6220cf318bfb8850b}




Definition at line 93 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC26\_\-REG@{CADAC26\_\-REG}}
\index{CADAC26\_\-REG@{CADAC26\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC26\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC26\_\-REG~CADAC3}\label{ATmega406_8h_fd160114715dba2e7d650589a98d7788}




Definition at line 94 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC27\_\-REG@{CADAC27\_\-REG}}
\index{CADAC27\_\-REG@{CADAC27\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC27\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC27\_\-REG~CADAC3}\label{ATmega406_8h_ae7a5be99f0df7464c7f3484c428f316}




Definition at line 95 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC28\_\-REG@{CADAC28\_\-REG}}
\index{CADAC28\_\-REG@{CADAC28\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC28\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC28\_\-REG~CADAC3}\label{ATmega406_8h_363c3c2bfac62a72623d3b49da9b0354}




Definition at line 96 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC29\_\-REG@{CADAC29\_\-REG}}
\index{CADAC29\_\-REG@{CADAC29\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC29\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC29\_\-REG~CADAC3}\label{ATmega406_8h_5bed0e159a27197c71f52c0684e408fc}




Definition at line 97 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC30\_\-REG@{CADAC30\_\-REG}}
\index{CADAC30\_\-REG@{CADAC30\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC30\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC30\_\-REG~CADAC3}\label{ATmega406_8h_b4058d4fec5e85b1408454825535eafe}




Definition at line 98 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAC31\_\-REG@{CADAC31\_\-REG}}
\index{CADAC31\_\-REG@{CADAC31\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAC31\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAC31\_\-REG~CADAC3}\label{ATmega406_8h_6bc97f4215fcdd45afe8978155da76bc}




Definition at line 99 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADACIE\_\-REG@{CADACIE\_\-REG}}
\index{CADACIE\_\-REG@{CADACIE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADACIE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADACIE\_\-REG~CADCSRB}\label{ATmega406_8h_0396c768bc32fc9918c1ee4c0938eda2}




Definition at line 345 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADACIF\_\-REG@{CADACIF\_\-REG}}
\index{CADACIF\_\-REG@{CADACIF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADACIF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADACIF\_\-REG~CADCSRB}\label{ATmega406_8h_23adbb3a3e5a8c0091077fd591d58d92}




Definition at line 342 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAS0\_\-REG@{CADAS0\_\-REG}}
\index{CADAS0\_\-REG@{CADAS0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAS0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAS0\_\-REG~CADCSRA}\label{ATmega406_8h_287b4fd19d4e0ef569ab1d57f5692b7a}




Definition at line 421 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADAS1\_\-REG@{CADAS1\_\-REG}}
\index{CADAS1\_\-REG@{CADAS1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADAS1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADAS1\_\-REG~CADCSRA}\label{ATmega406_8h_22e7c556e080abe630919079a0bae292}




Definition at line 422 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADEN\_\-REG@{CADEN\_\-REG}}
\index{CADEN\_\-REG@{CADEN\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADEN\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADEN\_\-REG~CADCSRA}\label{ATmega406_8h_272d2083201292c81ef964d0ab061055}




Definition at line 424 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICH0\_\-REG@{CADICH0\_\-REG}}
\index{CADICH0\_\-REG@{CADICH0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICH0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICH0\_\-REG~CADICH}\label{ATmega406_8h_2fbd1122697e03236decd8625a4587cc}




Definition at line 312 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICH1\_\-REG@{CADICH1\_\-REG}}
\index{CADICH1\_\-REG@{CADICH1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICH1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICH1\_\-REG~CADICH}\label{ATmega406_8h_542c1c4ff7bf08b3e46bddd2b024a9fc}




Definition at line 313 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICH2\_\-REG@{CADICH2\_\-REG}}
\index{CADICH2\_\-REG@{CADICH2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICH2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICH2\_\-REG~CADICH}\label{ATmega406_8h_122504ee7dbbd246f4f58b70c7f1e637}




Definition at line 314 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICH3\_\-REG@{CADICH3\_\-REG}}
\index{CADICH3\_\-REG@{CADICH3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICH3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICH3\_\-REG~CADICH}\label{ATmega406_8h_fbd9f7ed343f9a477798a3b1228adf19}




Definition at line 315 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICH4\_\-REG@{CADICH4\_\-REG}}
\index{CADICH4\_\-REG@{CADICH4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICH4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICH4\_\-REG~CADICH}\label{ATmega406_8h_abedc1ff91cb17ef0f15aad2dc355708}




Definition at line 316 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICH5\_\-REG@{CADICH5\_\-REG}}
\index{CADICH5\_\-REG@{CADICH5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICH5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICH5\_\-REG~CADICH}\label{ATmega406_8h_4811f093fe48b21dc5fe35dd1a044047}




Definition at line 317 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICH6\_\-REG@{CADICH6\_\-REG}}
\index{CADICH6\_\-REG@{CADICH6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICH6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICH6\_\-REG~CADICH}\label{ATmega406_8h_cdfa9c7a359aa98f9ff06ca0f4377c99}




Definition at line 318 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICH7\_\-REG@{CADICH7\_\-REG}}
\index{CADICH7\_\-REG@{CADICH7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICH7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICH7\_\-REG~CADICH}\label{ATmega406_8h_0c46c44f15c0ceef8f2ae33c9ed4d90a}




Definition at line 319 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICIE\_\-REG@{CADICIE\_\-REG}}
\index{CADICIE\_\-REG@{CADICIE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICIE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICIE\_\-REG~CADCSRB}\label{ATmega406_8h_ba67aa539e3477c0d0a5b5e6361f33cd}




Definition at line 343 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICIF\_\-REG@{CADICIF\_\-REG}}
\index{CADICIF\_\-REG@{CADICIF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICIF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICIF\_\-REG~CADCSRB}\label{ATmega406_8h_34486796bcabc827a09054527d61775b}




Definition at line 340 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICL0\_\-REG@{CADICL0\_\-REG}}
\index{CADICL0\_\-REG@{CADICL0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICL0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICL0\_\-REG~CADICL}\label{ATmega406_8h_8e3387b5f045c3217b280bb77d61c484}




Definition at line 348 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICL1\_\-REG@{CADICL1\_\-REG}}
\index{CADICL1\_\-REG@{CADICL1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICL1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICL1\_\-REG~CADICL}\label{ATmega406_8h_bb762d1728745f22acc679079a70df7f}




Definition at line 349 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICL2\_\-REG@{CADICL2\_\-REG}}
\index{CADICL2\_\-REG@{CADICL2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICL2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICL2\_\-REG~CADICL}\label{ATmega406_8h_ea6f42a4756606708baa8e19f77ef078}




Definition at line 350 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICL3\_\-REG@{CADICL3\_\-REG}}
\index{CADICL3\_\-REG@{CADICL3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICL3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICL3\_\-REG~CADICL}\label{ATmega406_8h_718522cac75d9f702c76e748d1df49a5}




Definition at line 351 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICL4\_\-REG@{CADICL4\_\-REG}}
\index{CADICL4\_\-REG@{CADICL4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICL4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICL4\_\-REG~CADICL}\label{ATmega406_8h_e710aad7cd42af20f9848e38de55169d}




Definition at line 352 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICL5\_\-REG@{CADICL5\_\-REG}}
\index{CADICL5\_\-REG@{CADICL5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICL5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICL5\_\-REG~CADICL}\label{ATmega406_8h_57e3a6342ed95b2bb85496c6bb1b406b}




Definition at line 353 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICL6\_\-REG@{CADICL6\_\-REG}}
\index{CADICL6\_\-REG@{CADICL6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICL6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICL6\_\-REG~CADICL}\label{ATmega406_8h_302878ada15738a1d3796fd8a3ec77b0}




Definition at line 354 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADICL7\_\-REG@{CADICL7\_\-REG}}
\index{CADICL7\_\-REG@{CADICL7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADICL7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADICL7\_\-REG~CADICL}\label{ATmega406_8h_d3bda800993edad0865f3b4bba334d5d}




Definition at line 355 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRCC0\_\-REG@{CADRCC0\_\-REG}}
\index{CADRCC0\_\-REG@{CADRCC0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRCC0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRCC0\_\-REG~CADRCC}\label{ATmega406_8h_5526c9c9a7a18af99197ac458b0f820c}




Definition at line 728 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRCC1\_\-REG@{CADRCC1\_\-REG}}
\index{CADRCC1\_\-REG@{CADRCC1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRCC1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRCC1\_\-REG~CADRCC}\label{ATmega406_8h_66b3369e50cfbfce4a1ffb644b35cd00}




Definition at line 729 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRCC2\_\-REG@{CADRCC2\_\-REG}}
\index{CADRCC2\_\-REG@{CADRCC2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRCC2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRCC2\_\-REG~CADRCC}\label{ATmega406_8h_a9f3f39b1d5995dc5505150e338b89e0}




Definition at line 730 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRCC3\_\-REG@{CADRCC3\_\-REG}}
\index{CADRCC3\_\-REG@{CADRCC3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRCC3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRCC3\_\-REG~CADRCC}\label{ATmega406_8h_1fe016eb9edf81f28e4d43f109695673}




Definition at line 731 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRCC4\_\-REG@{CADRCC4\_\-REG}}
\index{CADRCC4\_\-REG@{CADRCC4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRCC4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRCC4\_\-REG~CADRCC}\label{ATmega406_8h_333b70a4861221b544e0496c7947beab}




Definition at line 732 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRCC5\_\-REG@{CADRCC5\_\-REG}}
\index{CADRCC5\_\-REG@{CADRCC5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRCC5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRCC5\_\-REG~CADRCC}\label{ATmega406_8h_7df76c4c14290afebd35a5103f62c7b3}




Definition at line 733 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRCC6\_\-REG@{CADRCC6\_\-REG}}
\index{CADRCC6\_\-REG@{CADRCC6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRCC6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRCC6\_\-REG~CADRCC}\label{ATmega406_8h_f74a82e09c9ab77eeb6cfa22d6922832}




Definition at line 734 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRCC7\_\-REG@{CADRCC7\_\-REG}}
\index{CADRCC7\_\-REG@{CADRCC7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRCC7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRCC7\_\-REG~CADRCC}\label{ATmega406_8h_11e6d6789eb6b97f86bbceedd2f453ad}




Definition at line 735 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRCIE\_\-REG@{CADRCIE\_\-REG}}
\index{CADRCIE\_\-REG@{CADRCIE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRCIE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRCIE\_\-REG~CADCSRB}\label{ATmega406_8h_61fe40606864c923461655303afab169}




Definition at line 344 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRCIF\_\-REG@{CADRCIF\_\-REG}}
\index{CADRCIF\_\-REG@{CADRCIF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRCIF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRCIF\_\-REG~CADCSRB}\label{ATmega406_8h_0bd1419c7d670643f32151e645f28090}




Definition at line 341 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRDC0\_\-REG@{CADRDC0\_\-REG}}
\index{CADRDC0\_\-REG@{CADRDC0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRDC0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRDC0\_\-REG~CADRDC}\label{ATmega406_8h_0fe5b047a32d9bc86f7fe0194df02687}




Definition at line 435 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRDC1\_\-REG@{CADRDC1\_\-REG}}
\index{CADRDC1\_\-REG@{CADRDC1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRDC1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRDC1\_\-REG~CADRDC}\label{ATmega406_8h_55ddb0159a9811a21963e857de037f19}




Definition at line 436 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRDC2\_\-REG@{CADRDC2\_\-REG}}
\index{CADRDC2\_\-REG@{CADRDC2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRDC2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRDC2\_\-REG~CADRDC}\label{ATmega406_8h_cd0ce8f85aca811995b9be2ab9a4850b}




Definition at line 437 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRDC3\_\-REG@{CADRDC3\_\-REG}}
\index{CADRDC3\_\-REG@{CADRDC3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRDC3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRDC3\_\-REG~CADRDC}\label{ATmega406_8h_c98df04e519349e10dd7684a9655716e}




Definition at line 438 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRDC4\_\-REG@{CADRDC4\_\-REG}}
\index{CADRDC4\_\-REG@{CADRDC4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRDC4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRDC4\_\-REG~CADRDC}\label{ATmega406_8h_9304d57a90c78af570d2114e42979622}




Definition at line 439 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRDC5\_\-REG@{CADRDC5\_\-REG}}
\index{CADRDC5\_\-REG@{CADRDC5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRDC5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRDC5\_\-REG~CADRDC}\label{ATmega406_8h_77d3ccd74ba63f940d54204c48cc015e}




Definition at line 440 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRDC6\_\-REG@{CADRDC6\_\-REG}}
\index{CADRDC6\_\-REG@{CADRDC6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRDC6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRDC6\_\-REG~CADRDC}\label{ATmega406_8h_b256e78d5bbfa85201079536198fabc8}




Definition at line 441 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADRDC7\_\-REG@{CADRDC7\_\-REG}}
\index{CADRDC7\_\-REG@{CADRDC7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADRDC7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADRDC7\_\-REG~CADRDC}\label{ATmega406_8h_693e42e07a3aa693ccab137865cf1d7e}




Definition at line 442 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADSE\_\-REG@{CADSE\_\-REG}}
\index{CADSE\_\-REG@{CADSE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADSE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADSE\_\-REG~CADCSRA}\label{ATmega406_8h_12f3eb61b9a683ca9a98b80d86b287b9}




Definition at line 418 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADSI0\_\-REG@{CADSI0\_\-REG}}
\index{CADSI0\_\-REG@{CADSI0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADSI0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADSI0\_\-REG~CADCSRA}\label{ATmega406_8h_56ee731ab70e24ece276c8db8d956951}




Definition at line 419 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADSI1\_\-REG@{CADSI1\_\-REG}}
\index{CADSI1\_\-REG@{CADSI1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADSI1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADSI1\_\-REG~CADCSRA}\label{ATmega406_8h_ac5c45950282ac18b3834de29c6cb251}




Definition at line 420 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CADUB\_\-REG@{CADUB\_\-REG}}
\index{CADUB\_\-REG@{CADUB\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CADUB\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CADUB\_\-REG~CADCSRA}\label{ATmega406_8h_1e49b74b2183654ca3de01fa8e8505cc}




Definition at line 423 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CBE1\_\-REG@{CBE1\_\-REG}}
\index{CBE1\_\-REG@{CBE1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CBE1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CBE1\_\-REG~CBCR}\label{ATmega406_8h_19722f1f39daaf8fddbd144d4dcf7e2d}




Definition at line 705 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CBE2\_\-REG@{CBE2\_\-REG}}
\index{CBE2\_\-REG@{CBE2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CBE2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CBE2\_\-REG~CBCR}\label{ATmega406_8h_ea17574ec9ea3a89baee455d9b6ec2aa}




Definition at line 706 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CBE3\_\-REG@{CBE3\_\-REG}}
\index{CBE3\_\-REG@{CBE3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CBE3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CBE3\_\-REG~CBCR}\label{ATmega406_8h_c011e1dfb600bfc0c103c71f09b5ef95}




Definition at line 707 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CBE4\_\-REG@{CBE4\_\-REG}}
\index{CBE4\_\-REG@{CBE4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CBE4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CBE4\_\-REG~CBCR}\label{ATmega406_8h_94ac4547bb126ae5e710d55e0a2b3723}




Definition at line 708 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CCD\_\-REG@{CCD\_\-REG}}
\index{CCD\_\-REG@{CCD\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CCD\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CCD\_\-REG~BPCR}\label{ATmega406_8h_d3be27a87c47bc478c6d14467b705883}




Definition at line 168 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CCDL0\_\-REG@{CCDL0\_\-REG}}
\index{CCDL0\_\-REG@{CCDL0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CCDL0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CCDL0\_\-REG~BPOCD}\label{ATmega406_8h_9cbfe15163d81644da9d0e4bab73c4c1}




Definition at line 274 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CCDL1\_\-REG@{CCDL1\_\-REG}}
\index{CCDL1\_\-REG@{CCDL1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CCDL1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CCDL1\_\-REG~BPOCD}\label{ATmega406_8h_227dda066c73599f346eea1e8c2d8078}




Definition at line 275 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CCDL2\_\-REG@{CCDL2\_\-REG}}
\index{CCDL2\_\-REG@{CCDL2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CCDL2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CCDL2\_\-REG~BPOCD}\label{ATmega406_8h_90bc03e9ccfadcd508083dc9968b6305}




Definition at line 276 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CCDL3\_\-REG@{CCDL3\_\-REG}}
\index{CCDL3\_\-REG@{CCDL3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CCDL3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CCDL3\_\-REG~BPOCD}\label{ATmega406_8h_01f9092a31ef78d9115d4471e435e7f0}




Definition at line 277 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CFE\_\-REG@{CFE\_\-REG}}
\index{CFE\_\-REG@{CFE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CFE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CFE\_\-REG~FCSR}\label{ATmega406_8h_57f33d59d1ba11cdc663350c39535190}




Definition at line 323 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!COCIE\_\-REG@{COCIE\_\-REG}}
\index{COCIE\_\-REG@{COCIE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[COCIE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define COCIE\_\-REG~BPIR}\label{ATmega406_8h_22d6fc816537362d337b285a3c5bd765}




Definition at line 360 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!COCIF\_\-REG@{COCIF\_\-REG}}
\index{COCIF\_\-REG@{COCIF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[COCIF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define COCIF\_\-REG~BPIR}\label{ATmega406_8h_67a2947aa6e1bce76f660df9cf5d5e55}




Definition at line 364 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!COM0A0\_\-REG@{COM0A0\_\-REG}}
\index{COM0A0\_\-REG@{COM0A0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[COM0A0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define COM0A0\_\-REG~TCCR0A}\label{ATmega406_8h_9c9465ff0fee821ed1763c20125f47a3}




Definition at line 695 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!COM0A1\_\-REG@{COM0A1\_\-REG}}
\index{COM0A1\_\-REG@{COM0A1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[COM0A1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define COM0A1\_\-REG~TCCR0A}\label{ATmega406_8h_3def34db20518881afd8dd086ffb398c}




Definition at line 696 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!COM0B0\_\-REG@{COM0B0\_\-REG}}
\index{COM0B0\_\-REG@{COM0B0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[COM0B0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define COM0B0\_\-REG~TCCR0A}\label{ATmega406_8h_9d23e2b8a3ebfce4226155d1ee5862a9}




Definition at line 693 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!COM0B1\_\-REG@{COM0B1\_\-REG}}
\index{COM0B1\_\-REG@{COM0B1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[COM0B1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define COM0B1\_\-REG~TCCR0A}\label{ATmega406_8h_2ce4faf67e1d6fe840938a8c4945b0eb}




Definition at line 694 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CPS\_\-REG@{CPS\_\-REG}}
\index{CPS\_\-REG@{CPS\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CPS\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CPS\_\-REG~FCSR}\label{ATmega406_8h_125d1b3d132434ed0a4c3667bc8455e8}




Definition at line 325 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CS00\_\-REG@{CS00\_\-REG}}
\index{CS00\_\-REG@{CS00\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CS00\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CS00\_\-REG~TCCR0B}\label{ATmega406_8h_d6fb22c4ce97d412dc37b55f4b35ee93}




Definition at line 591 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CS01\_\-REG@{CS01\_\-REG}}
\index{CS01\_\-REG@{CS01\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CS01\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CS01\_\-REG~TCCR0B}\label{ATmega406_8h_d7a4fa68797c75de6a1926be1cfec45c}




Definition at line 592 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CS02\_\-REG@{CS02\_\-REG}}
\index{CS02\_\-REG@{CS02\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CS02\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CS02\_\-REG~TCCR0B}\label{ATmega406_8h_1a9315fba28730441e7c82bb275bb9c3}




Definition at line 593 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CS10\_\-REG@{CS10\_\-REG}}
\index{CS10\_\-REG@{CS10\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CS10\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CS10\_\-REG~TCCR1B}\label{ATmega406_8h_4bccf13bfda930e64185bba13885c648}




Definition at line 382 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CS11\_\-REG@{CS11\_\-REG}}
\index{CS11\_\-REG@{CS11\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CS11\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CS11\_\-REG~TCCR1B}\label{ATmega406_8h_d99924dd14efce240828bab9be7449fe}




Definition at line 383 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CS12\_\-REG@{CS12\_\-REG}}
\index{CS12\_\-REG@{CS12\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CS12\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CS12\_\-REG~TCCR1B}\label{ATmega406_8h_e76fac75534b9165e7c6b5df064b14b5}




Definition at line 384 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!CTC1\_\-REG@{CTC1\_\-REG}}
\index{CTC1\_\-REG@{CTC1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[CTC1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define CTC1\_\-REG~TCCR1B}\label{ATmega406_8h_ce1a97e7116d8e7f1e128e56f1b7bc76}




Definition at line 385 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DCD\_\-REG@{DCD\_\-REG}}
\index{DCD\_\-REG@{DCD\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DCD\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DCD\_\-REG~BPCR}\label{ATmega406_8h_f12ac585320431be73af6a4095a3d95d}




Definition at line 169 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DCDL0\_\-REG@{DCDL0\_\-REG}}
\index{DCDL0\_\-REG@{DCDL0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DCDL0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DCDL0\_\-REG~BPOCD}\label{ATmega406_8h_c5e8c72ab3139c0c442f6baa00fdfea6}




Definition at line 278 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DCDL1\_\-REG@{DCDL1\_\-REG}}
\index{DCDL1\_\-REG@{DCDL1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DCDL1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DCDL1\_\-REG~BPOCD}\label{ATmega406_8h_21651a4ca8f6d0e87bc338816243b4aa}




Definition at line 279 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DCDL2\_\-REG@{DCDL2\_\-REG}}
\index{DCDL2\_\-REG@{DCDL2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DCDL2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DCDL2\_\-REG~BPOCD}\label{ATmega406_8h_941f0260f4cfe879645ce87ce1a487f0}




Definition at line 280 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DCDL3\_\-REG@{DCDL3\_\-REG}}
\index{DCDL3\_\-REG@{DCDL3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DCDL3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DCDL3\_\-REG~BPOCD}\label{ATmega406_8h_e5076bf249ca1aa0bb553705a66aac2f}




Definition at line 281 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDA0\_\-REG@{DDA0\_\-REG}}
\index{DDA0\_\-REG@{DDA0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDA0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDA0\_\-REG~DDRA}\label{ATmega406_8h_aef52c5aedb89ccabfc50839565390e2}




Definition at line 232 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDA1\_\-REG@{DDA1\_\-REG}}
\index{DDA1\_\-REG@{DDA1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDA1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDA1\_\-REG~DDRA}\label{ATmega406_8h_edf2c8fb8d1eb1c1e61262e344953b19}




Definition at line 233 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDA2\_\-REG@{DDA2\_\-REG}}
\index{DDA2\_\-REG@{DDA2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDA2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDA2\_\-REG~DDRA}\label{ATmega406_8h_f18acc40a827c632d2c6fad0906b4eba}




Definition at line 234 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDA3\_\-REG@{DDA3\_\-REG}}
\index{DDA3\_\-REG@{DDA3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDA3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDA3\_\-REG~DDRA}\label{ATmega406_8h_2a047ebfb566e37e3f620cbcce47048b}




Definition at line 235 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDA4\_\-REG@{DDA4\_\-REG}}
\index{DDA4\_\-REG@{DDA4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDA4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDA4\_\-REG~DDRA}\label{ATmega406_8h_d9298f6beb7643d24b31858390c2c7f8}




Definition at line 236 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDA5\_\-REG@{DDA5\_\-REG}}
\index{DDA5\_\-REG@{DDA5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDA5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDA5\_\-REG~DDRA}\label{ATmega406_8h_aeb34f94a11a2c485bfd0fa05ce22f3b}




Definition at line 237 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDA6\_\-REG@{DDA6\_\-REG}}
\index{DDA6\_\-REG@{DDA6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDA6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDA6\_\-REG~DDRA}\label{ATmega406_8h_d5846bc7ef66d84ad6d68fec402e2bd0}




Definition at line 238 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDA7\_\-REG@{DDA7\_\-REG}}
\index{DDA7\_\-REG@{DDA7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDA7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDA7\_\-REG~DDRA}\label{ATmega406_8h_bf262001da9c0b98276431dbb7f2c729}




Definition at line 239 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDB0\_\-REG@{DDB0\_\-REG}}
\index{DDB0\_\-REG@{DDB0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDB0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDB0\_\-REG~DDRB}\label{ATmega406_8h_7ab353495cd33f8c72f46e7d319c703a}




Definition at line 158 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDB1\_\-REG@{DDB1\_\-REG}}
\index{DDB1\_\-REG@{DDB1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDB1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDB1\_\-REG~DDRB}\label{ATmega406_8h_39058410287a0eeec43e291e018d01c1}




Definition at line 159 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDB2\_\-REG@{DDB2\_\-REG}}
\index{DDB2\_\-REG@{DDB2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDB2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDB2\_\-REG~DDRB}\label{ATmega406_8h_29d74f0664c454064897591d1919b293}




Definition at line 160 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDB3\_\-REG@{DDB3\_\-REG}}
\index{DDB3\_\-REG@{DDB3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDB3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDB3\_\-REG~DDRB}\label{ATmega406_8h_d8a09112abdf6f164c8a71f18e8c612a}




Definition at line 161 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDB4\_\-REG@{DDB4\_\-REG}}
\index{DDB4\_\-REG@{DDB4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDB4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDB4\_\-REG~DDRB}\label{ATmega406_8h_a15b3fe8b6fe58f7212e9c5d34aef6fb}




Definition at line 162 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDB5\_\-REG@{DDB5\_\-REG}}
\index{DDB5\_\-REG@{DDB5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDB5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDB5\_\-REG~DDRB}\label{ATmega406_8h_d67c06d800fb1f86170187f1a5aca74c}




Definition at line 163 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDB6\_\-REG@{DDB6\_\-REG}}
\index{DDB6\_\-REG@{DDB6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDB6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDB6\_\-REG~DDRB}\label{ATmega406_8h_319ef0c4c664b7b3242a2d4a39ecf8c8}




Definition at line 164 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDB7\_\-REG@{DDB7\_\-REG}}
\index{DDB7\_\-REG@{DDB7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDB7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDB7\_\-REG~DDRB}\label{ATmega406_8h_e4947913fc9208758819398510f06aee}




Definition at line 165 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDD0\_\-REG@{DDD0\_\-REG}}
\index{DDD0\_\-REG@{DDD0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDD0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDD0\_\-REG~DDRD}\label{ATmega406_8h_152c8fee78340e396d3024e7cea88433}




Definition at line 284 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DDD1\_\-REG@{DDD1\_\-REG}}
\index{DDD1\_\-REG@{DDD1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DDD1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DDD1\_\-REG~DDRD}\label{ATmega406_8h_be7032a0e18a85f4cd6d060a64802566}




Definition at line 285 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DFE\_\-REG@{DFE\_\-REG}}
\index{DFE\_\-REG@{DFE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DFE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DFE\_\-REG~FCSR}\label{ATmega406_8h_ce5392925ee20820dc62c8835bcca858}




Definition at line 324 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DOCIE\_\-REG@{DOCIE\_\-REG}}
\index{DOCIE\_\-REG@{DOCIE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DOCIE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DOCIE\_\-REG~BPIR}\label{ATmega406_8h_edb4695be1b474404e8db8d5735b3e66}




Definition at line 359 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DOCIF\_\-REG@{DOCIF\_\-REG}}
\index{DOCIF\_\-REG@{DOCIF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DOCIF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DOCIF\_\-REG~BPIR}\label{ATmega406_8h_cc165f999309b482ae3a77e5c1b55bd5}




Definition at line 363 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DUDL0\_\-REG@{DUDL0\_\-REG}}
\index{DUDL0\_\-REG@{DUDL0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DUDL0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DUDL0\_\-REG~BPDUV}\label{ATmega406_8h_5657151c0528007115dba1bfdb066f0f}




Definition at line 427 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DUDL1\_\-REG@{DUDL1\_\-REG}}
\index{DUDL1\_\-REG@{DUDL1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DUDL1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DUDL1\_\-REG~BPDUV}\label{ATmega406_8h_f087e8926fda4e394c005e8682fde280}




Definition at line 428 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DUDL2\_\-REG@{DUDL2\_\-REG}}
\index{DUDL2\_\-REG@{DUDL2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DUDL2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DUDL2\_\-REG~BPDUV}\label{ATmega406_8h_ea034e074f189362ae643b41469b99b2}




Definition at line 429 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DUDL3\_\-REG@{DUDL3\_\-REG}}
\index{DUDL3\_\-REG@{DUDL3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DUDL3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DUDL3\_\-REG~BPDUV}\label{ATmega406_8h_b45f3c1e4a99cf915672c2fbfe5de15e}




Definition at line 430 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DUVD\_\-REG@{DUVD\_\-REG}}
\index{DUVD\_\-REG@{DUVD\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DUVD\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DUVD\_\-REG~BPCR}\label{ATmega406_8h_01d6f856178286181ae0818584703032}




Definition at line 171 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DUVIE\_\-REG@{DUVIE\_\-REG}}
\index{DUVIE\_\-REG@{DUVIE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DUVIE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DUVIE\_\-REG~BPIR}\label{ATmega406_8h_1fa5ca567c04c82558ec4f1fca580cdd}




Definition at line 361 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DUVIF\_\-REG@{DUVIF\_\-REG}}
\index{DUVIF\_\-REG@{DUVIF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DUVIF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DUVIF\_\-REG~BPIR}\label{ATmega406_8h_399574a1147b8fcdbff3e33ed80264f2}




Definition at line 365 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DUVT0\_\-REG@{DUVT0\_\-REG}}
\index{DUVT0\_\-REG@{DUVT0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DUVT0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DUVT0\_\-REG~BPDUV}\label{ATmega406_8h_7d9f31f5e841b66bfd3033bf3f394c28}




Definition at line 431 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!DUVT1\_\-REG@{DUVT1\_\-REG}}
\index{DUVT1\_\-REG@{DUVT1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[DUVT1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define DUVT1\_\-REG~BPDUV}\label{ATmega406_8h_eeab7418cbac5ced8c2205b7b61c02c2}




Definition at line 432 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEAR0\_\-REG@{EEAR0\_\-REG}}
\index{EEAR0\_\-REG@{EEAR0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEAR0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEAR0\_\-REG~EEARL}\label{ATmega406_8h_e1187c7c4a9a2c9a94c52f960aea72b7}




Definition at line 572 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEAR1\_\-REG@{EEAR1\_\-REG}}
\index{EEAR1\_\-REG@{EEAR1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEAR1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEAR1\_\-REG~EEARL}\label{ATmega406_8h_3ecedc062008b7de245537691bab01a0}




Definition at line 573 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEAR2\_\-REG@{EEAR2\_\-REG}}
\index{EEAR2\_\-REG@{EEAR2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEAR2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEAR2\_\-REG~EEARL}\label{ATmega406_8h_d20f65b0b26eb04cfd85d58a61f1144c}




Definition at line 574 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEAR3\_\-REG@{EEAR3\_\-REG}}
\index{EEAR3\_\-REG@{EEAR3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEAR3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEAR3\_\-REG~EEARL}\label{ATmega406_8h_c62f3e15dcda82565987d6f2c5d085b7}




Definition at line 575 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEAR4\_\-REG@{EEAR4\_\-REG}}
\index{EEAR4\_\-REG@{EEAR4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEAR4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEAR4\_\-REG~EEARL}\label{ATmega406_8h_f5c808944940e03de96e4bc7b24c193e}




Definition at line 576 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEAR5\_\-REG@{EEAR5\_\-REG}}
\index{EEAR5\_\-REG@{EEAR5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEAR5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEAR5\_\-REG~EEARL}\label{ATmega406_8h_89176301c1e1a7567b527dd3125e644b}




Definition at line 577 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEAR6\_\-REG@{EEAR6\_\-REG}}
\index{EEAR6\_\-REG@{EEAR6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEAR6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEAR6\_\-REG~EEARL}\label{ATmega406_8h_8ef30328fa9ddb4fffdf336ef09c9e47}




Definition at line 578 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEAR7\_\-REG@{EEAR7\_\-REG}}
\index{EEAR7\_\-REG@{EEAR7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEAR7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEAR7\_\-REG~EEARL}\label{ATmega406_8h_c21ffe3cf613f29c03684fd7b88e0678}




Definition at line 579 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEAR8\_\-REG@{EEAR8\_\-REG}}
\index{EEAR8\_\-REG@{EEAR8\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEAR8\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEAR8\_\-REG~EEARH}\label{ATmega406_8h_f220aa494c268a9bccf6bd06bbdbd8b5}




Definition at line 395 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEDR0\_\-REG@{EEDR0\_\-REG}}
\index{EEDR0\_\-REG@{EEDR0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEDR0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEDR0\_\-REG~EEDR}\label{ATmega406_8h_8d216943a0cca47e19d07df2e094dd0c}




Definition at line 184 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEDR1\_\-REG@{EEDR1\_\-REG}}
\index{EEDR1\_\-REG@{EEDR1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEDR1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEDR1\_\-REG~EEDR}\label{ATmega406_8h_91207268cff90964d03fba66dcf40c9b}




Definition at line 185 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEDR2\_\-REG@{EEDR2\_\-REG}}
\index{EEDR2\_\-REG@{EEDR2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEDR2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEDR2\_\-REG~EEDR}\label{ATmega406_8h_381678d278d3388ee7402642d9356e89}




Definition at line 186 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEDR3\_\-REG@{EEDR3\_\-REG}}
\index{EEDR3\_\-REG@{EEDR3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEDR3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEDR3\_\-REG~EEDR}\label{ATmega406_8h_10c53e9f8101929b0c98c7b648adf7b2}




Definition at line 187 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEDR4\_\-REG@{EEDR4\_\-REG}}
\index{EEDR4\_\-REG@{EEDR4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEDR4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEDR4\_\-REG~EEDR}\label{ATmega406_8h_ec27ae2a8bbeab97b48f69d029778688}




Definition at line 188 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEDR5\_\-REG@{EEDR5\_\-REG}}
\index{EEDR5\_\-REG@{EEDR5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEDR5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEDR5\_\-REG~EEDR}\label{ATmega406_8h_4e36ce79337901ade900f6b39e0b5cbd}




Definition at line 189 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEDR6\_\-REG@{EEDR6\_\-REG}}
\index{EEDR6\_\-REG@{EEDR6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEDR6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEDR6\_\-REG~EEDR}\label{ATmega406_8h_7507ac912d4263b41db72ec4ea316e3d}




Definition at line 190 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEDR7\_\-REG@{EEDR7\_\-REG}}
\index{EEDR7\_\-REG@{EEDR7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEDR7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEDR7\_\-REG~EEDR}\label{ATmega406_8h_1f0ea61a10f28c018a87bd8c80b1d1d0}




Definition at line 191 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEMPE\_\-REG@{EEMPE\_\-REG}}
\index{EEMPE\_\-REG@{EEMPE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEMPE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEMPE\_\-REG~EECR}\label{ATmega406_8h_534c85dd5d47742d53180717f8432c58}




Definition at line 124 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEPE\_\-REG@{EEPE\_\-REG}}
\index{EEPE\_\-REG@{EEPE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEPE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEPE\_\-REG~EECR}\label{ATmega406_8h_c8a24aa10348737c092140618df9cc34}




Definition at line 123 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEPM0\_\-REG@{EEPM0\_\-REG}}
\index{EEPM0\_\-REG@{EEPM0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEPM0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEPM0\_\-REG~EECR}\label{ATmega406_8h_39008c85a0c5358e43b2b21db76547c5}




Definition at line 126 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EEPM1\_\-REG@{EEPM1\_\-REG}}
\index{EEPM1\_\-REG@{EEPM1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EEPM1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EEPM1\_\-REG~EECR}\label{ATmega406_8h_af8ab5d087a0eb2543074269e8a55611}




Definition at line 127 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EERE\_\-REG@{EERE\_\-REG}}
\index{EERE\_\-REG@{EERE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EERE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EERE\_\-REG~EECR}\label{ATmega406_8h_4b0a037ffc07086c66641e936e4ab391}




Definition at line 122 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EERIE\_\-REG@{EERIE\_\-REG}}
\index{EERIE\_\-REG@{EERIE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EERIE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EERIE\_\-REG~EECR}\label{ATmega406_8h_4807b87f52b0b2e793969557480bdb25}




Definition at line 125 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!EXTRF\_\-REG@{EXTRF\_\-REG}}
\index{EXTRF\_\-REG@{EXTRF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[EXTRF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define EXTRF\_\-REG~MCUSR}\label{ATmega406_8h_e620c15a439519ac2da939753266acc5}




Definition at line 389 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!FCAL0\_\-REG@{FCAL0\_\-REG}}
\index{FCAL0\_\-REG@{FCAL0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[FCAL0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define FCAL0\_\-REG~FOSCCAL}\label{ATmega406_8h_b2fc26ee670fe04b5bc6400389335a52}




Definition at line 675 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!FCAL1\_\-REG@{FCAL1\_\-REG}}
\index{FCAL1\_\-REG@{FCAL1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[FCAL1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define FCAL1\_\-REG~FOSCCAL}\label{ATmega406_8h_f96f5d08db5273825d421559844017c3}




Definition at line 676 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!FCAL2\_\-REG@{FCAL2\_\-REG}}
\index{FCAL2\_\-REG@{FCAL2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[FCAL2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define FCAL2\_\-REG~FOSCCAL}\label{ATmega406_8h_75604cd97d722a5a3f40fb5abd42d1b6}




Definition at line 677 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!FCAL3\_\-REG@{FCAL3\_\-REG}}
\index{FCAL3\_\-REG@{FCAL3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[FCAL3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define FCAL3\_\-REG~FOSCCAL}\label{ATmega406_8h_053be1f2da08a97bd329024029121c1b}




Definition at line 678 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!FCAL4\_\-REG@{FCAL4\_\-REG}}
\index{FCAL4\_\-REG@{FCAL4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[FCAL4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define FCAL4\_\-REG~FOSCCAL}\label{ATmega406_8h_5e89948cbdffb724c9e639a56cd13a4f}




Definition at line 679 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!FCAL5\_\-REG@{FCAL5\_\-REG}}
\index{FCAL5\_\-REG@{FCAL5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[FCAL5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define FCAL5\_\-REG~FOSCCAL}\label{ATmega406_8h_29e7e2212d3c2320ce23b40e9a394b63}




Definition at line 680 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!FCAL6\_\-REG@{FCAL6\_\-REG}}
\index{FCAL6\_\-REG@{FCAL6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[FCAL6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define FCAL6\_\-REG~FOSCCAL}\label{ATmega406_8h_6ff36496e10c3742a27e3e034d84b1ff}




Definition at line 681 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!FCAL7\_\-REG@{FCAL7\_\-REG}}
\index{FCAL7\_\-REG@{FCAL7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[FCAL7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define FCAL7\_\-REG~FOSCCAL}\label{ATmega406_8h_010a7954e1637d480501917132172261}




Definition at line 682 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!FOC0A\_\-REG@{FOC0A\_\-REG}}
\index{FOC0A\_\-REG@{FOC0A\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[FOC0A\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define FOC0A\_\-REG~TCCR0B}\label{ATmega406_8h_5273a16edbe72c0b173bcd9f63fcad5d}




Definition at line 596 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!FOC0B\_\-REG@{FOC0B\_\-REG}}
\index{FOC0B\_\-REG@{FOC0B\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[FOC0B\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define FOC0B\_\-REG~TCCR0B}\label{ATmega406_8h_70b0e0371adb056971724bd8729b2e32}




Definition at line 595 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR00\_\-REG@{GPIOR00\_\-REG}}
\index{GPIOR00\_\-REG@{GPIOR00\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR00\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR00\_\-REG~GPIOR0}\label{ATmega406_8h_b685813ba32bbaf4420521030d50c037}




Definition at line 562 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR01\_\-REG@{GPIOR01\_\-REG}}
\index{GPIOR01\_\-REG@{GPIOR01\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR01\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR01\_\-REG~GPIOR0}\label{ATmega406_8h_c706e7180a27bf80265fa991c48923da}




Definition at line 563 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR02\_\-REG@{GPIOR02\_\-REG}}
\index{GPIOR02\_\-REG@{GPIOR02\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR02\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR02\_\-REG~GPIOR0}\label{ATmega406_8h_e9a044500da3c8fd3b83ee57b753cf5a}




Definition at line 564 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR03\_\-REG@{GPIOR03\_\-REG}}
\index{GPIOR03\_\-REG@{GPIOR03\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR03\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR03\_\-REG~GPIOR0}\label{ATmega406_8h_7037df4b8ef967c60655040822116904}




Definition at line 565 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR04\_\-REG@{GPIOR04\_\-REG}}
\index{GPIOR04\_\-REG@{GPIOR04\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR04\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR04\_\-REG~GPIOR0}\label{ATmega406_8h_3bcd13cc46c1dad947f4a717886963bd}




Definition at line 566 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR05\_\-REG@{GPIOR05\_\-REG}}
\index{GPIOR05\_\-REG@{GPIOR05\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR05\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR05\_\-REG~GPIOR0}\label{ATmega406_8h_d17f1f3640c7c438450e1c6cd83dc416}




Definition at line 567 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR06\_\-REG@{GPIOR06\_\-REG}}
\index{GPIOR06\_\-REG@{GPIOR06\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR06\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR06\_\-REG~GPIOR0}\label{ATmega406_8h_34928f33c30d2778bcbd652d3bdc992e}




Definition at line 568 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR07\_\-REG@{GPIOR07\_\-REG}}
\index{GPIOR07\_\-REG@{GPIOR07\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR07\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR07\_\-REG~GPIOR0}\label{ATmega406_8h_80bf149d778a818c8b22d0e47d364f6c}




Definition at line 569 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR10\_\-REG@{GPIOR10\_\-REG}}
\index{GPIOR10\_\-REG@{GPIOR10\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR10\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR10\_\-REG~GPIOR1}\label{ATmega406_8h_0c74701f14e731ccfa7947080ec1fd9f}




Definition at line 368 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR11\_\-REG@{GPIOR11\_\-REG}}
\index{GPIOR11\_\-REG@{GPIOR11\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR11\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR11\_\-REG~GPIOR1}\label{ATmega406_8h_c89ae966cc5f650c67a4f64b533b972a}




Definition at line 369 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR12\_\-REG@{GPIOR12\_\-REG}}
\index{GPIOR12\_\-REG@{GPIOR12\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR12\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR12\_\-REG~GPIOR1}\label{ATmega406_8h_7f76dd7c79d2bc02264eddfb83e21f9c}




Definition at line 370 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR13\_\-REG@{GPIOR13\_\-REG}}
\index{GPIOR13\_\-REG@{GPIOR13\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR13\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR13\_\-REG~GPIOR1}\label{ATmega406_8h_59613cf26325e7193f38349c9172edb2}




Definition at line 371 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR14\_\-REG@{GPIOR14\_\-REG}}
\index{GPIOR14\_\-REG@{GPIOR14\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR14\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR14\_\-REG~GPIOR1}\label{ATmega406_8h_f6c932c67c1239f8920bea53eefbccd2}




Definition at line 372 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR15\_\-REG@{GPIOR15\_\-REG}}
\index{GPIOR15\_\-REG@{GPIOR15\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR15\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR15\_\-REG~GPIOR1}\label{ATmega406_8h_30ca1225d7607c42928f4cad3d965283}




Definition at line 373 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR16\_\-REG@{GPIOR16\_\-REG}}
\index{GPIOR16\_\-REG@{GPIOR16\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR16\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR16\_\-REG~GPIOR1}\label{ATmega406_8h_86b974ae70cbc0717a8f7515c3a458c5}




Definition at line 374 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR17\_\-REG@{GPIOR17\_\-REG}}
\index{GPIOR17\_\-REG@{GPIOR17\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR17\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR17\_\-REG~GPIOR1}\label{ATmega406_8h_0e49370d23d38b5a3390c338b26209fc}




Definition at line 375 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR20\_\-REG@{GPIOR20\_\-REG}}
\index{GPIOR20\_\-REG@{GPIOR20\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR20\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR20\_\-REG~GPIOR2}\label{ATmega406_8h_3790087c426bd43e2adddb6ecd73e386}




Definition at line 629 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR21\_\-REG@{GPIOR21\_\-REG}}
\index{GPIOR21\_\-REG@{GPIOR21\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR21\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR21\_\-REG~GPIOR2}\label{ATmega406_8h_940062f35eee1065c6303ac7235f559a}




Definition at line 630 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR22\_\-REG@{GPIOR22\_\-REG}}
\index{GPIOR22\_\-REG@{GPIOR22\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR22\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR22\_\-REG~GPIOR2}\label{ATmega406_8h_7c436e7420ded2f0613e6641d95b0c52}




Definition at line 631 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR23\_\-REG@{GPIOR23\_\-REG}}
\index{GPIOR23\_\-REG@{GPIOR23\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR23\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR23\_\-REG~GPIOR2}\label{ATmega406_8h_df1117d309a043e9c04be45c1b4b77a9}




Definition at line 632 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR24\_\-REG@{GPIOR24\_\-REG}}
\index{GPIOR24\_\-REG@{GPIOR24\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR24\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR24\_\-REG~GPIOR2}\label{ATmega406_8h_d44d09cf80aa143ae8524daf27bb7a61}




Definition at line 633 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR25\_\-REG@{GPIOR25\_\-REG}}
\index{GPIOR25\_\-REG@{GPIOR25\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR25\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR25\_\-REG~GPIOR2}\label{ATmega406_8h_665dd9b34b86dfda15def8fe104848cc}




Definition at line 634 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR26\_\-REG@{GPIOR26\_\-REG}}
\index{GPIOR26\_\-REG@{GPIOR26\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR26\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR26\_\-REG~GPIOR2}\label{ATmega406_8h_b2de6daa35a101d8ce7d3796cf633eed}




Definition at line 635 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!GPIOR27\_\-REG@{GPIOR27\_\-REG}}
\index{GPIOR27\_\-REG@{GPIOR27\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[GPIOR27\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define GPIOR27\_\-REG~GPIOR2}\label{ATmega406_8h_104cb3d89f026f59dfb8859ca0208116}




Definition at line 636 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!H\_\-REG@{H\_\-REG}}
\index{H\_\-REG@{H\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[H\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define H\_\-REG~SREG}\label{ATmega406_8h_9e7762cfa71109c938bdda8ccfd7a7e8}




Definition at line 149 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!I\_\-REG@{I\_\-REG}}
\index{I\_\-REG@{I\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[I\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define I\_\-REG~SREG}\label{ATmega406_8h_856b2402264352968c67d30cff7b75ea}




Definition at line 151 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!INT0\_\-BIT@{INT0\_\-BIT}}
\index{INT0\_\-BIT@{INT0\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[INT0\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define INT0\_\-BIT~4}\label{ATmega406_8h_5d004e5a830a09b875a030e98a40a55b}




Definition at line 786 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!INT0\_\-PORT@{INT0\_\-PORT}}
\index{INT0\_\-PORT@{INT0\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[INT0\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define INT0\_\-PORT~PORTA}\label{ATmega406_8h_dc981fa047fd68da334581984c22269f}




Definition at line 785 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!INT0\_\-REG@{INT0\_\-REG}}
\index{INT0\_\-REG@{INT0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[INT0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define INT0\_\-REG~EIMSK}\label{ATmega406_8h_ef41b7ee03276d4f5fcd2255aba0dce4}




Definition at line 242 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!INT1\_\-BIT@{INT1\_\-BIT}}
\index{INT1\_\-BIT@{INT1\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[INT1\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define INT1\_\-BIT~5}\label{ATmega406_8h_087cf0a65af1e5b32ce8c2a7104f97bd}




Definition at line 791 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!INT1\_\-PORT@{INT1\_\-PORT}}
\index{INT1\_\-PORT@{INT1\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[INT1\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define INT1\_\-PORT~PORTA}\label{ATmega406_8h_f96062a0df1453b55f3925974436e531}




Definition at line 790 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!INT1\_\-REG@{INT1\_\-REG}}
\index{INT1\_\-REG@{INT1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[INT1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define INT1\_\-REG~EIMSK}\label{ATmega406_8h_ed8a95911748ccc51f86338edd2a850c}




Definition at line 243 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!INT2\_\-BIT@{INT2\_\-BIT}}
\index{INT2\_\-BIT@{INT2\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[INT2\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define INT2\_\-BIT~6}\label{ATmega406_8h_76e97c2312ea89a01323b87eb5258ee7}




Definition at line 796 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!INT2\_\-PORT@{INT2\_\-PORT}}
\index{INT2\_\-PORT@{INT2\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[INT2\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define INT2\_\-PORT~PORTA}\label{ATmega406_8h_9b2ca3d6eabbe1d6e038dc0c983b0460}




Definition at line 795 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!INT2\_\-REG@{INT2\_\-REG}}
\index{INT2\_\-REG@{INT2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[INT2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define INT2\_\-REG~EIMSK}\label{ATmega406_8h_ea735ad7d48b20943b32340fa26a4073}




Definition at line 244 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!INT3\_\-BIT@{INT3\_\-BIT}}
\index{INT3\_\-BIT@{INT3\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[INT3\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define INT3\_\-BIT~7}\label{ATmega406_8h_4e013943ba14f67e49e123947b93df62}




Definition at line 801 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!INT3\_\-PORT@{INT3\_\-PORT}}
\index{INT3\_\-PORT@{INT3\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[INT3\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define INT3\_\-PORT~PORTA}\label{ATmega406_8h_638c53e478ed12e1f201297c6d307243}




Definition at line 800 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!INT3\_\-REG@{INT3\_\-REG}}
\index{INT3\_\-REG@{INT3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[INT3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define INT3\_\-REG~EIMSK}\label{ATmega406_8h_f47858a0ab6e747d696d3d34b2f8b657}




Definition at line 245 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!INTF0\_\-REG@{INTF0\_\-REG}}
\index{INTF0\_\-REG@{INTF0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[INTF0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define INTF0\_\-REG~EIFR}\label{ATmega406_8h_c8eea570a562240195a8d71daa36a15a}




Definition at line 748 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!INTF1\_\-REG@{INTF1\_\-REG}}
\index{INTF1\_\-REG@{INTF1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[INTF1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define INTF1\_\-REG~EIFR}\label{ATmega406_8h_18326e0f6547e43792de1ed122ee4382}




Definition at line 749 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!INTF2\_\-REG@{INTF2\_\-REG}}
\index{INTF2\_\-REG@{INTF2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[INTF2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define INTF2\_\-REG~EIFR}\label{ATmega406_8h_05ff50f0cf4c490f7b45a9506f07c116}




Definition at line 750 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!INTF3\_\-REG@{INTF3\_\-REG}}
\index{INTF3\_\-REG@{INTF3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[INTF3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define INTF3\_\-REG~EIFR}\label{ATmega406_8h_2bc3a324ee02d7ebeb0767ded371bd6b}




Definition at line 751 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ISC00\_\-REG@{ISC00\_\-REG}}
\index{ISC00\_\-REG@{ISC00\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[ISC00\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define ISC00\_\-REG~EICRA}\label{ATmega406_8h_21c52d8f7ccc0b73261c2871950dec5f}




Definition at line 659 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ISC01\_\-REG@{ISC01\_\-REG}}
\index{ISC01\_\-REG@{ISC01\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[ISC01\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define ISC01\_\-REG~EICRA}\label{ATmega406_8h_1d3247e568986e0a910394086a1aa8a8}




Definition at line 660 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ISC10\_\-REG@{ISC10\_\-REG}}
\index{ISC10\_\-REG@{ISC10\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[ISC10\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define ISC10\_\-REG~EICRA}\label{ATmega406_8h_d8fcec19bf04f6c2fdd03b92511928b8}




Definition at line 661 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ISC11\_\-REG@{ISC11\_\-REG}}
\index{ISC11\_\-REG@{ISC11\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[ISC11\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define ISC11\_\-REG~EICRA}\label{ATmega406_8h_dcec47801cf8ca8953ebc068cfa097c8}




Definition at line 662 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ISC20\_\-REG@{ISC20\_\-REG}}
\index{ISC20\_\-REG@{ISC20\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[ISC20\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define ISC20\_\-REG~EICRA}\label{ATmega406_8h_07ddc6fbbaea79b0d8e327399ace7343}




Definition at line 663 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ISC21\_\-REG@{ISC21\_\-REG}}
\index{ISC21\_\-REG@{ISC21\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[ISC21\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define ISC21\_\-REG~EICRA}\label{ATmega406_8h_1c4f80e5ee5e9ff648be2f1378827af4}




Definition at line 664 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ISC30\_\-REG@{ISC30\_\-REG}}
\index{ISC30\_\-REG@{ISC30\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[ISC30\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define ISC30\_\-REG~EICRA}\label{ATmega406_8h_708c40b174145e7a0bdbf82c42413426}




Definition at line 665 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!ISC31\_\-REG@{ISC31\_\-REG}}
\index{ISC31\_\-REG@{ISC31\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[ISC31\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define ISC31\_\-REG~EICRA}\label{ATmega406_8h_3947671fbfd87c7b6fe0372940cdccd0}




Definition at line 666 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!IVCE\_\-REG@{IVCE\_\-REG}}
\index{IVCE\_\-REG@{IVCE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[IVCE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define IVCE\_\-REG~MCUCR}\label{ATmega406_8h_a2d0b2fab1e834745137c45cdc990652}




Definition at line 699 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!IVSEL\_\-REG@{IVSEL\_\-REG}}
\index{IVSEL\_\-REG@{IVSEL\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[IVSEL\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define IVSEL\_\-REG~MCUCR}\label{ATmega406_8h_4b1c656675f122c04630fd0059be6a42}




Definition at line 700 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!JTD\_\-REG@{JTD\_\-REG}}
\index{JTD\_\-REG@{JTD\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[JTD\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define JTD\_\-REG~MCUCR}\label{ATmega406_8h_2dceb15d0c659678824af95799179951}




Definition at line 702 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!JTRF\_\-REG@{JTRF\_\-REG}}
\index{JTRF\_\-REG@{JTRF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[JTRF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define JTRF\_\-REG~MCUSR}\label{ATmega406_8h_ccd93f42b9845213793482a88a7d1e9a}




Definition at line 392 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!N\_\-REG@{N\_\-REG}}
\index{N\_\-REG@{N\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[N\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define N\_\-REG~SREG}\label{ATmega406_8h_22560b62179eb57d9a1f102291689234}




Definition at line 146 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OC0A\_\-BIT@{OC0A\_\-BIT}}
\index{OC0A\_\-BIT@{OC0A\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[OC0A\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define OC0A\_\-BIT~6}\label{ATmega406_8h_0ad390da135913247403e8652024f03d}




Definition at line 832 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OC0A\_\-PORT@{OC0A\_\-PORT}}
\index{OC0A\_\-PORT@{OC0A\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[OC0A\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define OC0A\_\-PORT~PORTB}\label{ATmega406_8h_8709b42aa8a925818f664ef4b2cc0ac9}




Definition at line 831 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OC0B\_\-BIT@{OC0B\_\-BIT}}
\index{OC0B\_\-BIT@{OC0B\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[OC0B\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define OC0B\_\-BIT~7}\label{ATmega406_8h_21274478f5f4bad3636de29945a2be9d}




Definition at line 837 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OC0B\_\-PORT@{OC0B\_\-PORT}}
\index{OC0B\_\-PORT@{OC0B\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[OC0B\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define OC0B\_\-PORT~PORTB}\label{ATmega406_8h_5224aff8eb24cefcb135075432349b26}




Definition at line 836 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCF0A\_\-REG@{OCF0A\_\-REG}}
\index{OCF0A\_\-REG@{OCF0A\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCF0A\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCF0A\_\-REG~TIFR0}\label{ATmega406_8h_3f48357e922f77b8fd07213ee72f6569}




Definition at line 755 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCF0B\_\-REG@{OCF0B\_\-REG}}
\index{OCF0B\_\-REG@{OCF0B\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCF0B\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCF0B\_\-REG~TIFR0}\label{ATmega406_8h_f5f73cadcda2b3b40e99b59ac99e27a6}




Definition at line 756 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCF1A\_\-REG@{OCF1A\_\-REG}}
\index{OCF1A\_\-REG@{OCF1A\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCF1A\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCF1A\_\-REG~TIFR1}\label{ATmega406_8h_e5a9fd43ec78b0c6e7539d83dd7926d0}




Definition at line 760 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCIE0A\_\-REG@{OCIE0A\_\-REG}}
\index{OCIE0A\_\-REG@{OCIE0A\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCIE0A\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCIE0A\_\-REG~TIMSK0}\label{ATmega406_8h_b5623e5597e7929772a52ce8a5e35294}




Definition at line 583 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCIE0B\_\-REG@{OCIE0B\_\-REG}}
\index{OCIE0B\_\-REG@{OCIE0B\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCIE0B\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCIE0B\_\-REG~TIMSK0}\label{ATmega406_8h_04c1067deee0b48f3d9e21fcaa364107}




Definition at line 584 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCIE1A\_\-REG@{OCIE1A\_\-REG}}
\index{OCIE1A\_\-REG@{OCIE1A\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCIE1A\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCIE1A\_\-REG~TIMSK1}\label{ATmega406_8h_6854b762f72186a69a1dd3f894dba314}




Definition at line 588 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCPT0\_\-REG@{OCPT0\_\-REG}}
\index{OCPT0\_\-REG@{OCPT0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCPT0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCPT0\_\-REG~CBPTR}\label{ATmega406_8h_a4da79a671c630617e460e8964d38441}




Definition at line 398 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCPT1\_\-REG@{OCPT1\_\-REG}}
\index{OCPT1\_\-REG@{OCPT1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCPT1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCPT1\_\-REG~CBPTR}\label{ATmega406_8h_571702f11c91405b5bcb00a267893c39}




Definition at line 399 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCPT2\_\-REG@{OCPT2\_\-REG}}
\index{OCPT2\_\-REG@{OCPT2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCPT2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCPT2\_\-REG~CBPTR}\label{ATmega406_8h_e39460779f086379df8de4b08ec199d4}




Definition at line 400 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCPT3\_\-REG@{OCPT3\_\-REG}}
\index{OCPT3\_\-REG@{OCPT3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCPT3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCPT3\_\-REG~CBPTR}\label{ATmega406_8h_bf1df8c554ca978415c3f8926c246bb2}




Definition at line 401 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR0A0\_\-REG@{OCR0A0\_\-REG}}
\index{OCR0A0\_\-REG@{OCR0A0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR0A0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR0A0\_\-REG~OCR0A}\label{ATmega406_8h_c3e3a5ca6a79a1cef8e399dd498236ea}




Definition at line 264 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR0A1\_\-REG@{OCR0A1\_\-REG}}
\index{OCR0A1\_\-REG@{OCR0A1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR0A1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR0A1\_\-REG~OCR0A}\label{ATmega406_8h_0535fa9ac6149b4979dbfb42c77480e3}




Definition at line 265 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR0A2\_\-REG@{OCR0A2\_\-REG}}
\index{OCR0A2\_\-REG@{OCR0A2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR0A2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR0A2\_\-REG~OCR0A}\label{ATmega406_8h_3abcaf6f1308ead01ad2ad2dbdcecad5}




Definition at line 266 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR0A3\_\-REG@{OCR0A3\_\-REG}}
\index{OCR0A3\_\-REG@{OCR0A3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR0A3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR0A3\_\-REG~OCR0A}\label{ATmega406_8h_81a196d593e97042fc76fb2644bc3113}




Definition at line 267 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR0A4\_\-REG@{OCR0A4\_\-REG}}
\index{OCR0A4\_\-REG@{OCR0A4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR0A4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR0A4\_\-REG~OCR0A}\label{ATmega406_8h_4da05012933232075f01cf28739ae350}




Definition at line 268 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR0A5\_\-REG@{OCR0A5\_\-REG}}
\index{OCR0A5\_\-REG@{OCR0A5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR0A5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR0A5\_\-REG~OCR0A}\label{ATmega406_8h_efce6d13999dfae7c7e2505d9a60eb95}




Definition at line 269 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR0A6\_\-REG@{OCR0A6\_\-REG}}
\index{OCR0A6\_\-REG@{OCR0A6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR0A6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR0A6\_\-REG~OCR0A}\label{ATmega406_8h_6b473a1eff0c0f06986d8187d4c5ede6}




Definition at line 270 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR0A7\_\-REG@{OCR0A7\_\-REG}}
\index{OCR0A7\_\-REG@{OCR0A7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR0A7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR0A7\_\-REG~OCR0A}\label{ATmega406_8h_024f5a2f048a683599bfceef3669c729}




Definition at line 271 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR0B0\_\-REG@{OCR0B0\_\-REG}}
\index{OCR0B0\_\-REG@{OCR0B0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR0B0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR0B0\_\-REG~OCR0B}\label{ATmega406_8h_abb295c023e235ec6ce4ea21750fd2f2}




Definition at line 288 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR0B1\_\-REG@{OCR0B1\_\-REG}}
\index{OCR0B1\_\-REG@{OCR0B1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR0B1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR0B1\_\-REG~OCR0B}\label{ATmega406_8h_b3004cd016933951f49676e9eb867272}




Definition at line 289 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR0B2\_\-REG@{OCR0B2\_\-REG}}
\index{OCR0B2\_\-REG@{OCR0B2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR0B2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR0B2\_\-REG~OCR0B}\label{ATmega406_8h_27f50a55b23aa1130345bc66dfe93537}




Definition at line 290 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR0B3\_\-REG@{OCR0B3\_\-REG}}
\index{OCR0B3\_\-REG@{OCR0B3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR0B3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR0B3\_\-REG~OCR0B}\label{ATmega406_8h_efaf996b78ded92e38ff8d050dda7014}




Definition at line 291 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR0B4\_\-REG@{OCR0B4\_\-REG}}
\index{OCR0B4\_\-REG@{OCR0B4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR0B4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR0B4\_\-REG~OCR0B}\label{ATmega406_8h_d30372e5f9ad21478cdd4970a1f49436}




Definition at line 292 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR0B5\_\-REG@{OCR0B5\_\-REG}}
\index{OCR0B5\_\-REG@{OCR0B5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR0B5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR0B5\_\-REG~OCR0B}\label{ATmega406_8h_d9b95a8e0afa4e2b979067abce9a5422}




Definition at line 293 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR0B6\_\-REG@{OCR0B6\_\-REG}}
\index{OCR0B6\_\-REG@{OCR0B6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR0B6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR0B6\_\-REG~OCR0B}\label{ATmega406_8h_e01dfec13055b6bcff758d5250fa9a2c}




Definition at line 294 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR0B7\_\-REG@{OCR0B7\_\-REG}}
\index{OCR0B7\_\-REG@{OCR0B7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR0B7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR0B7\_\-REG~OCR0B}\label{ATmega406_8h_569b84760567cd4cb09a686a74ae32e3}




Definition at line 295 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR1AH0\_\-REG@{OCR1AH0\_\-REG}}
\index{OCR1AH0\_\-REG@{OCR1AH0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR1AH0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR1AH0\_\-REG~OCR1AH}\label{ATmega406_8h_76cffc78592a8684b6ad766495c67b97}




Definition at line 542 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR1AH1\_\-REG@{OCR1AH1\_\-REG}}
\index{OCR1AH1\_\-REG@{OCR1AH1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR1AH1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR1AH1\_\-REG~OCR1AH}\label{ATmega406_8h_6ff71710a669c3a301f09038c2656ffc}




Definition at line 543 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR1AH2\_\-REG@{OCR1AH2\_\-REG}}
\index{OCR1AH2\_\-REG@{OCR1AH2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR1AH2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR1AH2\_\-REG~OCR1AH}\label{ATmega406_8h_664d0221d7d1b04e8de8a7c0a570d72a}




Definition at line 544 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR1AH3\_\-REG@{OCR1AH3\_\-REG}}
\index{OCR1AH3\_\-REG@{OCR1AH3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR1AH3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR1AH3\_\-REG~OCR1AH}\label{ATmega406_8h_9ae7117bbdff1b73881565ffa935d23c}




Definition at line 545 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR1AH4\_\-REG@{OCR1AH4\_\-REG}}
\index{OCR1AH4\_\-REG@{OCR1AH4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR1AH4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR1AH4\_\-REG~OCR1AH}\label{ATmega406_8h_8b9575a62855f2b00b42c86d2b8fe219}




Definition at line 546 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR1AH5\_\-REG@{OCR1AH5\_\-REG}}
\index{OCR1AH5\_\-REG@{OCR1AH5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR1AH5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR1AH5\_\-REG~OCR1AH}\label{ATmega406_8h_86de588f6310ed6535f319930d6b8769}




Definition at line 547 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR1AH6\_\-REG@{OCR1AH6\_\-REG}}
\index{OCR1AH6\_\-REG@{OCR1AH6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR1AH6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR1AH6\_\-REG~OCR1AH}\label{ATmega406_8h_de644871a6cf22e4afa55e62d129c76d}




Definition at line 548 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR1AH7\_\-REG@{OCR1AH7\_\-REG}}
\index{OCR1AH7\_\-REG@{OCR1AH7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR1AH7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR1AH7\_\-REG~OCR1AH}\label{ATmega406_8h_9175672c5137d382cb7caf6f420dcb95}




Definition at line 549 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR1AL0\_\-REG@{OCR1AL0\_\-REG}}
\index{OCR1AL0\_\-REG@{OCR1AL0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR1AL0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR1AL0\_\-REG~OCR1AL}\label{ATmega406_8h_b7156a04d6b271949b7089575b073e77}




Definition at line 718 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR1AL1\_\-REG@{OCR1AL1\_\-REG}}
\index{OCR1AL1\_\-REG@{OCR1AL1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR1AL1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR1AL1\_\-REG~OCR1AL}\label{ATmega406_8h_804cba0f39f492d7288da3e1f6493b10}




Definition at line 719 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR1AL2\_\-REG@{OCR1AL2\_\-REG}}
\index{OCR1AL2\_\-REG@{OCR1AL2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR1AL2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR1AL2\_\-REG~OCR1AL}\label{ATmega406_8h_602b5d751df6f8a1ce0f5884c8b2d5bf}




Definition at line 720 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR1AL3\_\-REG@{OCR1AL3\_\-REG}}
\index{OCR1AL3\_\-REG@{OCR1AL3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR1AL3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR1AL3\_\-REG~OCR1AL}\label{ATmega406_8h_c9878f7beec4913a6b24ec1e7508808b}




Definition at line 721 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR1AL4\_\-REG@{OCR1AL4\_\-REG}}
\index{OCR1AL4\_\-REG@{OCR1AL4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR1AL4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR1AL4\_\-REG~OCR1AL}\label{ATmega406_8h_9be063575a85da6c6db243a5b6ac5206}




Definition at line 722 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR1AL5\_\-REG@{OCR1AL5\_\-REG}}
\index{OCR1AL5\_\-REG@{OCR1AL5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR1AL5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR1AL5\_\-REG~OCR1AL}\label{ATmega406_8h_e36d5d702dbe5b043976c0000b45ae68}




Definition at line 723 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR1AL6\_\-REG@{OCR1AL6\_\-REG}}
\index{OCR1AL6\_\-REG@{OCR1AL6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR1AL6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR1AL6\_\-REG~OCR1AL}\label{ATmega406_8h_9f0194a166ce44212f4d6440922e59c9}




Definition at line 724 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!OCR1AL7\_\-REG@{OCR1AL7\_\-REG}}
\index{OCR1AL7\_\-REG@{OCR1AL7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[OCR1AL7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define OCR1AL7\_\-REG~OCR1AL}\label{ATmega406_8h_0de9246b2f818d409d6993151145fc2a}




Definition at line 725 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCIE0\_\-REG@{PCIE0\_\-REG}}
\index{PCIE0\_\-REG@{PCIE0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCIE0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCIE0\_\-REG~PCICR}\label{ATmega406_8h_cc36a3d829c10e1ba4aa71009041b1f1}




Definition at line 154 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCIE1\_\-REG@{PCIE1\_\-REG}}
\index{PCIE1\_\-REG@{PCIE1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCIE1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCIE1\_\-REG~PCICR}\label{ATmega406_8h_fd57d01796fa506dea12b2cda35765ee}




Definition at line 155 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCIF0\_\-REG@{PCIF0\_\-REG}}
\index{PCIF0\_\-REG@{PCIF0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCIF0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCIF0\_\-REG~PCIFR}\label{ATmega406_8h_84ad580ef98d182b06ddfe9266c1ea93}




Definition at line 130 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCIF1\_\-REG@{PCIF1\_\-REG}}
\index{PCIF1\_\-REG@{PCIF1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCIF1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCIF1\_\-REG~PCIFR}\label{ATmega406_8h_600943af3d98c3c7ba13ac0f6e2fe6ce}




Definition at line 131 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT0\_\-BIT@{PCINT0\_\-BIT}}
\index{PCINT0\_\-BIT@{PCINT0\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT0\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT0\_\-BIT~0}\label{ATmega406_8h_6343b0a3cda1861529245574df547615}




Definition at line 766 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT0\_\-PORT@{PCINT0\_\-PORT}}
\index{PCINT0\_\-PORT@{PCINT0\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT0\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT0\_\-PORT~PORTA}\label{ATmega406_8h_b1de4465aa9d7a044fff09cd97ef13a6}




Definition at line 765 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT0\_\-REG@{PCINT0\_\-REG}}
\index{PCINT0\_\-REG@{PCINT0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT0\_\-REG~PCMSK0}\label{ATmega406_8h_1fc8de5bdf89aa2195c98f52d21f7ba1}




Definition at line 639 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT10\_\-BIT@{PCINT10\_\-BIT}}
\index{PCINT10\_\-BIT@{PCINT10\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT10\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT10\_\-BIT~2}\label{ATmega406_8h_0a73af10fa857337d63feff8567a2880}




Definition at line 818 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT10\_\-PORT@{PCINT10\_\-PORT}}
\index{PCINT10\_\-PORT@{PCINT10\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT10\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT10\_\-PORT~PORTB}\label{ATmega406_8h_255681d931b2685b01a842d2772e41dc}




Definition at line 817 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT10\_\-REG@{PCINT10\_\-REG}}
\index{PCINT10\_\-REG@{PCINT10\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT10\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT10\_\-REG~PCMSK1}\label{ATmega406_8h_9e49252fb3f8c92bfaf3814031cc919f}




Definition at line 256 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT11\_\-BIT@{PCINT11\_\-BIT}}
\index{PCINT11\_\-BIT@{PCINT11\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT11\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT11\_\-BIT~3}\label{ATmega406_8h_c84fb45b3701f222d1b0ccb32afc0821}




Definition at line 823 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT11\_\-PORT@{PCINT11\_\-PORT}}
\index{PCINT11\_\-PORT@{PCINT11\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT11\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT11\_\-PORT~PORTB}\label{ATmega406_8h_ad00eea33f59e9f7bf3f62eb0a8ee289}




Definition at line 822 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT11\_\-REG@{PCINT11\_\-REG}}
\index{PCINT11\_\-REG@{PCINT11\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT11\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT11\_\-REG~PCMSK1}\label{ATmega406_8h_fcbb1e0e89a9e5a26cccf46dafaf3fd8}




Definition at line 257 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT12\_\-BIT@{PCINT12\_\-BIT}}
\index{PCINT12\_\-BIT@{PCINT12\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT12\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT12\_\-BIT~4}\label{ATmega406_8h_9295f935895b92e56d558bcda39f40fb}




Definition at line 826 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT12\_\-PORT@{PCINT12\_\-PORT}}
\index{PCINT12\_\-PORT@{PCINT12\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT12\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT12\_\-PORT~PORTB}\label{ATmega406_8h_04b0a08cf28d3c3e7f8cfc422b933718}




Definition at line 825 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT12\_\-REG@{PCINT12\_\-REG}}
\index{PCINT12\_\-REG@{PCINT12\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT12\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT12\_\-REG~PCMSK1}\label{ATmega406_8h_29aa9a90bda96d18e17809b76a53ce91}




Definition at line 258 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT13\_\-BIT@{PCINT13\_\-BIT}}
\index{PCINT13\_\-BIT@{PCINT13\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT13\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT13\_\-BIT~5}\label{ATmega406_8h_a90caf5b501df32853960ab522a622a2}




Definition at line 829 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT13\_\-PORT@{PCINT13\_\-PORT}}
\index{PCINT13\_\-PORT@{PCINT13\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT13\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT13\_\-PORT~PORTB}\label{ATmega406_8h_72b8e0cd92b6e206bce9b2a30e5adbf9}




Definition at line 828 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT13\_\-REG@{PCINT13\_\-REG}}
\index{PCINT13\_\-REG@{PCINT13\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT13\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT13\_\-REG~PCMSK1}\label{ATmega406_8h_ebf531a77c3a584910f781592d70dc02}




Definition at line 259 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT14\_\-BIT@{PCINT14\_\-BIT}}
\index{PCINT14\_\-BIT@{PCINT14\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT14\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT14\_\-BIT~6}\label{ATmega406_8h_20800c19dfed6d6009e47fd102d954e8}




Definition at line 834 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT14\_\-PORT@{PCINT14\_\-PORT}}
\index{PCINT14\_\-PORT@{PCINT14\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT14\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT14\_\-PORT~PORTB}\label{ATmega406_8h_6b14a9bb14e86341079f8b9687581088}




Definition at line 833 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT14\_\-REG@{PCINT14\_\-REG}}
\index{PCINT14\_\-REG@{PCINT14\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT14\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT14\_\-REG~PCMSK1}\label{ATmega406_8h_f2e7bf7f3dc1971468e01e03c1f520de}




Definition at line 260 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT15\_\-BIT@{PCINT15\_\-BIT}}
\index{PCINT15\_\-BIT@{PCINT15\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT15\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT15\_\-BIT~7}\label{ATmega406_8h_9e0b6363cf5fa860edca1a9d676abf33}




Definition at line 839 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT15\_\-PORT@{PCINT15\_\-PORT}}
\index{PCINT15\_\-PORT@{PCINT15\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT15\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT15\_\-PORT~PORTB}\label{ATmega406_8h_3f140ca45181c62dc09d56065bfe1014}




Definition at line 838 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT15\_\-REG@{PCINT15\_\-REG}}
\index{PCINT15\_\-REG@{PCINT15\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT15\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT15\_\-REG~PCMSK1}\label{ATmega406_8h_dda3fd70fb83520df2b5ce893f28b5e1}




Definition at line 261 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT1\_\-BIT@{PCINT1\_\-BIT}}
\index{PCINT1\_\-BIT@{PCINT1\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT1\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT1\_\-BIT~1}\label{ATmega406_8h_21ec77de7608babe865d1919de82464b}




Definition at line 771 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT1\_\-PORT@{PCINT1\_\-PORT}}
\index{PCINT1\_\-PORT@{PCINT1\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT1\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT1\_\-PORT~PORTA}\label{ATmega406_8h_8c69086f27273ba63e5a57c547d976f2}




Definition at line 770 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT1\_\-REG@{PCINT1\_\-REG}}
\index{PCINT1\_\-REG@{PCINT1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT1\_\-REG~PCMSK0}\label{ATmega406_8h_26779181002e7ea2d1b1671cde829992}




Definition at line 640 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT2\_\-BIT@{PCINT2\_\-BIT}}
\index{PCINT2\_\-BIT@{PCINT2\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT2\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT2\_\-BIT~2}\label{ATmega406_8h_2b66add4059fd601c26fe3294c796523}




Definition at line 776 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT2\_\-PORT@{PCINT2\_\-PORT}}
\index{PCINT2\_\-PORT@{PCINT2\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT2\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT2\_\-PORT~PORTA}\label{ATmega406_8h_10edcff04cefc04d6fed3a93defa81cd}




Definition at line 775 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT2\_\-REG@{PCINT2\_\-REG}}
\index{PCINT2\_\-REG@{PCINT2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT2\_\-REG~PCMSK0}\label{ATmega406_8h_44afccf44b76d9f61fa5bab7738f7e99}




Definition at line 641 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT3\_\-BIT@{PCINT3\_\-BIT}}
\index{PCINT3\_\-BIT@{PCINT3\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT3\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT3\_\-BIT~3}\label{ATmega406_8h_396bf5081b19670b6359887a3a444d01}




Definition at line 781 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT3\_\-PORT@{PCINT3\_\-PORT}}
\index{PCINT3\_\-PORT@{PCINT3\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT3\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT3\_\-PORT~PORTA}\label{ATmega406_8h_ddbb79db12851a8f87875e653550eab2}




Definition at line 780 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT3\_\-REG@{PCINT3\_\-REG}}
\index{PCINT3\_\-REG@{PCINT3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT3\_\-REG~PCMSK0}\label{ATmega406_8h_ad92aed06b38cc34ccb0e3aac10ab4fa}




Definition at line 642 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT4\_\-BIT@{PCINT4\_\-BIT}}
\index{PCINT4\_\-BIT@{PCINT4\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT4\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT4\_\-BIT~4}\label{ATmega406_8h_bb9ad6e6592b88daee39ab22ce9c527e}




Definition at line 788 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT4\_\-PORT@{PCINT4\_\-PORT}}
\index{PCINT4\_\-PORT@{PCINT4\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT4\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT4\_\-PORT~PORTA}\label{ATmega406_8h_a1251765304df676b79d1c30413bf8e8}




Definition at line 787 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT4\_\-REG@{PCINT4\_\-REG}}
\index{PCINT4\_\-REG@{PCINT4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT4\_\-REG~PCMSK0}\label{ATmega406_8h_493d06113c3fbb3742899a614534ae01}




Definition at line 643 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT5\_\-BIT@{PCINT5\_\-BIT}}
\index{PCINT5\_\-BIT@{PCINT5\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT5\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT5\_\-BIT~5}\label{ATmega406_8h_204ad527a04b554131e812fab2871026}




Definition at line 793 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT5\_\-PORT@{PCINT5\_\-PORT}}
\index{PCINT5\_\-PORT@{PCINT5\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT5\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT5\_\-PORT~PORTA}\label{ATmega406_8h_d1ad035a0efaa1ef9f67d6a5c359c80f}




Definition at line 792 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT5\_\-REG@{PCINT5\_\-REG}}
\index{PCINT5\_\-REG@{PCINT5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT5\_\-REG~PCMSK0}\label{ATmega406_8h_c297aacfe6169d64a6bf5ab747518b14}




Definition at line 644 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT6\_\-BIT@{PCINT6\_\-BIT}}
\index{PCINT6\_\-BIT@{PCINT6\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT6\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT6\_\-BIT~6}\label{ATmega406_8h_a9de0b658c86105fd69c302e77326ad8}




Definition at line 798 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT6\_\-PORT@{PCINT6\_\-PORT}}
\index{PCINT6\_\-PORT@{PCINT6\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT6\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT6\_\-PORT~PORTA}\label{ATmega406_8h_86962228dadea234942d02d9c225d0db}




Definition at line 797 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT6\_\-REG@{PCINT6\_\-REG}}
\index{PCINT6\_\-REG@{PCINT6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT6\_\-REG~PCMSK0}\label{ATmega406_8h_1bc3b580d9f16a4a296d306edd493175}




Definition at line 645 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT7\_\-BIT@{PCINT7\_\-BIT}}
\index{PCINT7\_\-BIT@{PCINT7\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT7\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT7\_\-BIT~7}\label{ATmega406_8h_6dc4e799e523eec1e4f7656e25c4990d}




Definition at line 803 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT7\_\-PORT@{PCINT7\_\-PORT}}
\index{PCINT7\_\-PORT@{PCINT7\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT7\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT7\_\-PORT~PORTA}\label{ATmega406_8h_fd0a2ab6a4540e83edc2c5b0e643eb48}




Definition at line 802 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT7\_\-REG@{PCINT7\_\-REG}}
\index{PCINT7\_\-REG@{PCINT7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT7\_\-REG~PCMSK0}\label{ATmega406_8h_328583e3ab557eaaf35c0d1d28c57356}




Definition at line 646 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT8\_\-BIT@{PCINT8\_\-BIT}}
\index{PCINT8\_\-BIT@{PCINT8\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT8\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT8\_\-BIT~0}\label{ATmega406_8h_8d797cc448266b873f1be177195f5ea7}




Definition at line 808 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT8\_\-PORT@{PCINT8\_\-PORT}}
\index{PCINT8\_\-PORT@{PCINT8\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT8\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT8\_\-PORT~PORTB}\label{ATmega406_8h_ce2e7eeb5f08ed840ecc4039eb257878}




Definition at line 807 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT8\_\-REG@{PCINT8\_\-REG}}
\index{PCINT8\_\-REG@{PCINT8\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT8\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT8\_\-REG~PCMSK1}\label{ATmega406_8h_14d972f3e5b6be4d07dd2ae24aef01ec}




Definition at line 254 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT9\_\-BIT@{PCINT9\_\-BIT}}
\index{PCINT9\_\-BIT@{PCINT9\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT9\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT9\_\-BIT~1}\label{ATmega406_8h_4cdd3ace79b4689fc5f632fe351aa819}




Definition at line 813 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT9\_\-PORT@{PCINT9\_\-PORT}}
\index{PCINT9\_\-PORT@{PCINT9\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT9\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT9\_\-PORT~PORTB}\label{ATmega406_8h_827ff9585812b881142a51eb14919455}




Definition at line 812 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PCINT9\_\-REG@{PCINT9\_\-REG}}
\index{PCINT9\_\-REG@{PCINT9\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PCINT9\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PCINT9\_\-REG~PCMSK1}\label{ATmega406_8h_36ba853a00599ea9182d2e51c9da91ae}




Definition at line 255 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PFD\_\-REG@{PFD\_\-REG}}
\index{PFD\_\-REG@{PFD\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PFD\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PFD\_\-REG~FCSR}\label{ATmega406_8h_40a3200d55031324df1f1e2a5a6aba3d}




Definition at line 322 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PGERS\_\-REG@{PGERS\_\-REG}}
\index{PGERS\_\-REG@{PGERS\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PGERS\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PGERS\_\-REG~SPMCSR}\label{ATmega406_8h_82d438bd58be8d9b45211cc6b0448c80}




Definition at line 409 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PGWRT\_\-REG@{PGWRT\_\-REG}}
\index{PGWRT\_\-REG@{PGWRT\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PGWRT\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PGWRT\_\-REG~SPMCSR}\label{ATmega406_8h_baa71acc8944bcb1f49f429b64858848}




Definition at line 410 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PINA0\_\-REG@{PINA0\_\-REG}}
\index{PINA0\_\-REG@{PINA0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PINA0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PINA0\_\-REG~PINA}\label{ATmega406_8h_87349a516bad6c685f2d9ff9bb4ab515}




Definition at line 532 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PINA1\_\-REG@{PINA1\_\-REG}}
\index{PINA1\_\-REG@{PINA1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PINA1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PINA1\_\-REG~PINA}\label{ATmega406_8h_bd8ae178cf4ac0a74bc9459af700f983}




Definition at line 533 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PINA2\_\-REG@{PINA2\_\-REG}}
\index{PINA2\_\-REG@{PINA2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PINA2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PINA2\_\-REG~PINA}\label{ATmega406_8h_4dbb93d8f28d534ca550384d7f39331d}




Definition at line 534 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PINA3\_\-REG@{PINA3\_\-REG}}
\index{PINA3\_\-REG@{PINA3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PINA3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PINA3\_\-REG~PINA}\label{ATmega406_8h_eefe274ba938dcf7469743718b0f36ff}




Definition at line 535 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PINA4\_\-REG@{PINA4\_\-REG}}
\index{PINA4\_\-REG@{PINA4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PINA4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PINA4\_\-REG~PINA}\label{ATmega406_8h_459069978dae75fa518d619380b77b95}




Definition at line 536 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PINA5\_\-REG@{PINA5\_\-REG}}
\index{PINA5\_\-REG@{PINA5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PINA5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PINA5\_\-REG~PINA}\label{ATmega406_8h_16cb456ecc3f246c1c98f59af4c4f1da}




Definition at line 537 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PINA6\_\-REG@{PINA6\_\-REG}}
\index{PINA6\_\-REG@{PINA6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PINA6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PINA6\_\-REG~PINA}\label{ATmega406_8h_a0589540c6bd28b4cf195196a88d6425}




Definition at line 538 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PINA7\_\-REG@{PINA7\_\-REG}}
\index{PINA7\_\-REG@{PINA7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PINA7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PINA7\_\-REG~PINA}\label{ATmega406_8h_3f67696541bb9a66c09eb4604a68ad30}




Definition at line 539 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PINB0\_\-REG@{PINB0\_\-REG}}
\index{PINB0\_\-REG@{PINB0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PINB0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PINB0\_\-REG~PINB}\label{ATmega406_8h_887fe46ced810578885cd2f9576233fb}




Definition at line 738 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PINB1\_\-REG@{PINB1\_\-REG}}
\index{PINB1\_\-REG@{PINB1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PINB1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PINB1\_\-REG~PINB}\label{ATmega406_8h_96950156307fa8076767279ccb521a6d}




Definition at line 739 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PINB2\_\-REG@{PINB2\_\-REG}}
\index{PINB2\_\-REG@{PINB2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PINB2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PINB2\_\-REG~PINB}\label{ATmega406_8h_d5bd17b842b338d4383087c675a3a4f3}




Definition at line 740 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PINB3\_\-REG@{PINB3\_\-REG}}
\index{PINB3\_\-REG@{PINB3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PINB3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PINB3\_\-REG~PINB}\label{ATmega406_8h_f127a9d3187d4d3886ec120fa904d239}




Definition at line 741 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PINB4\_\-REG@{PINB4\_\-REG}}
\index{PINB4\_\-REG@{PINB4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PINB4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PINB4\_\-REG~PINB}\label{ATmega406_8h_33bd7788e70872f9c27adc27fd324222}




Definition at line 742 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PINB5\_\-REG@{PINB5\_\-REG}}
\index{PINB5\_\-REG@{PINB5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PINB5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PINB5\_\-REG~PINB}\label{ATmega406_8h_18e2c7ec2497f5b8511ef2ddf50c457f}




Definition at line 743 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PINB6\_\-REG@{PINB6\_\-REG}}
\index{PINB6\_\-REG@{PINB6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PINB6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PINB6\_\-REG~PINB}\label{ATmega406_8h_8f1d15c22912ea93248edbdb38c57613}




Definition at line 744 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PINB7\_\-REG@{PINB7\_\-REG}}
\index{PINB7\_\-REG@{PINB7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PINB7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PINB7\_\-REG~PINB}\label{ATmega406_8h_1d86f584aa520ed5ccb77ce75c9eae18}




Definition at line 745 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PIND0\_\-REG@{PIND0\_\-REG}}
\index{PIND0\_\-REG@{PIND0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PIND0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PIND0\_\-REG~PIND}\label{ATmega406_8h_a609777bfcce6a82df13bce5f936098d}




Definition at line 204 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PIND1\_\-REG@{PIND1\_\-REG}}
\index{PIND1\_\-REG@{PIND1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PIND1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PIND1\_\-REG~PIND}\label{ATmega406_8h_1ad1507c23c6cf423b3025d4a39562d3}




Definition at line 205 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORF\_\-REG@{PORF\_\-REG}}
\index{PORF\_\-REG@{PORF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORF\_\-REG~MCUSR}\label{ATmega406_8h_4793c8733c88789e4b47f72f77323fee}




Definition at line 388 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTA0\_\-REG@{PORTA0\_\-REG}}
\index{PORTA0\_\-REG@{PORTA0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTA0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTA0\_\-REG~PORTA}\label{ATmega406_8h_475de0053a32e046102c0f210b4e255e}




Definition at line 497 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTA1\_\-REG@{PORTA1\_\-REG}}
\index{PORTA1\_\-REG@{PORTA1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTA1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTA1\_\-REG~PORTA}\label{ATmega406_8h_87b55483461028deb8d509268ae94b94}




Definition at line 498 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTA2\_\-REG@{PORTA2\_\-REG}}
\index{PORTA2\_\-REG@{PORTA2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTA2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTA2\_\-REG~PORTA}\label{ATmega406_8h_7e25eccb55e4007a78a3bbeaec680868}




Definition at line 499 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTA3\_\-REG@{PORTA3\_\-REG}}
\index{PORTA3\_\-REG@{PORTA3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTA3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTA3\_\-REG~PORTA}\label{ATmega406_8h_80ae0ee68636f546d1f2c36364633a9f}




Definition at line 500 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTA4\_\-REG@{PORTA4\_\-REG}}
\index{PORTA4\_\-REG@{PORTA4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTA4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTA4\_\-REG~PORTA}\label{ATmega406_8h_118186f069a85a80ba9b607252f7b872}




Definition at line 501 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTA5\_\-REG@{PORTA5\_\-REG}}
\index{PORTA5\_\-REG@{PORTA5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTA5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTA5\_\-REG~PORTA}\label{ATmega406_8h_ae7c16aa4d53dcbc8efedddb46302ec6}




Definition at line 502 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTA6\_\-REG@{PORTA6\_\-REG}}
\index{PORTA6\_\-REG@{PORTA6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTA6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTA6\_\-REG~PORTA}\label{ATmega406_8h_4f10d602cb1f8040562ce0740de40071}




Definition at line 503 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTA7\_\-REG@{PORTA7\_\-REG}}
\index{PORTA7\_\-REG@{PORTA7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTA7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTA7\_\-REG~PORTA}\label{ATmega406_8h_e898aab8094633737f7f93d8270e9984}




Definition at line 504 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTB0\_\-REG@{PORTB0\_\-REG}}
\index{PORTB0\_\-REG@{PORTB0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTB0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTB0\_\-REG~PORTB}\label{ATmega406_8h_814e08d4ce55f8ef9f191bf2d2bb2242}




Definition at line 455 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTB1\_\-REG@{PORTB1\_\-REG}}
\index{PORTB1\_\-REG@{PORTB1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTB1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTB1\_\-REG~PORTB}\label{ATmega406_8h_3eadaad1e12b199a95c7b50317ed4a74}




Definition at line 456 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTB2\_\-REG@{PORTB2\_\-REG}}
\index{PORTB2\_\-REG@{PORTB2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTB2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTB2\_\-REG~PORTB}\label{ATmega406_8h_ea22c0fcf453c2cfed4b484d7dbdd012}




Definition at line 457 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTB3\_\-REG@{PORTB3\_\-REG}}
\index{PORTB3\_\-REG@{PORTB3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTB3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTB3\_\-REG~PORTB}\label{ATmega406_8h_3f3db80ab2df6227b50dcc9167dde63b}




Definition at line 458 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTB4\_\-REG@{PORTB4\_\-REG}}
\index{PORTB4\_\-REG@{PORTB4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTB4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTB4\_\-REG~PORTB}\label{ATmega406_8h_4d2fae120a0ebd695b8ffc6a18abf574}




Definition at line 459 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTB5\_\-REG@{PORTB5\_\-REG}}
\index{PORTB5\_\-REG@{PORTB5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTB5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTB5\_\-REG~PORTB}\label{ATmega406_8h_cbf5541cd8cce15b3d335ec1bb9c6674}




Definition at line 460 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTB6\_\-REG@{PORTB6\_\-REG}}
\index{PORTB6\_\-REG@{PORTB6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTB6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTB6\_\-REG~PORTB}\label{ATmega406_8h_ed9d497eb6d695e499fc490bbc9149fc}




Definition at line 461 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTB7\_\-REG@{PORTB7\_\-REG}}
\index{PORTB7\_\-REG@{PORTB7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTB7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTB7\_\-REG~PORTB}\label{ATmega406_8h_c83c2727ee2a47574b83f215c21be623}




Definition at line 462 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTC0\_\-REG@{PORTC0\_\-REG}}
\index{PORTC0\_\-REG@{PORTC0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTC0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTC0\_\-REG~PORTC}\label{ATmega406_8h_5d396cb8a677196f22e78ed6e10b9a84}




Definition at line 485 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTD0\_\-REG@{PORTD0\_\-REG}}
\index{PORTD0\_\-REG@{PORTD0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTD0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTD0\_\-REG~PORTD}\label{ATmega406_8h_2952ce2f503b50c06170b7b28e69ea6e}




Definition at line 465 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PORTD1\_\-REG@{PORTD1\_\-REG}}
\index{PORTD1\_\-REG@{PORTD1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PORTD1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PORTD1\_\-REG~PORTD}\label{ATmega406_8h_1f188cc9d7fdd39ba485f47f778927db}




Definition at line 466 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PRTIM0\_\-REG@{PRTIM0\_\-REG}}
\index{PRTIM0\_\-REG@{PRTIM0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PRTIM0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PRTIM0\_\-REG~PRR0}\label{ATmega406_8h_383cbcdc57f174082da252908e8d8b7e}




Definition at line 249 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PRTIM1\_\-REG@{PRTIM1\_\-REG}}
\index{PRTIM1\_\-REG@{PRTIM1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PRTIM1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PRTIM1\_\-REG~PRR0}\label{ATmega406_8h_e6b05a19b01448d75b81c43eafa77f7b}




Definition at line 250 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PRTWI\_\-REG@{PRTWI\_\-REG}}
\index{PRTWI\_\-REG@{PRTWI\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PRTWI\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PRTWI\_\-REG~PRR0}\label{ATmega406_8h_552a46f3daa707ecc2d40ec31341321f}




Definition at line 251 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PRVADC\_\-REG@{PRVADC\_\-REG}}
\index{PRVADC\_\-REG@{PRVADC\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PRVADC\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PRVADC\_\-REG~PRR0}\label{ATmega406_8h_58536ebaaf80110d7412e7bf488045ce}




Definition at line 248 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PSRSYNC\_\-REG@{PSRSYNC\_\-REG}}
\index{PSRSYNC\_\-REG@{PSRSYNC\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PSRSYNC\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PSRSYNC\_\-REG~GTCCR}\label{ATmega406_8h_628a64a640746546004768242b9a2144}




Definition at line 208 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PUD\_\-REG@{PUD\_\-REG}}
\index{PUD\_\-REG@{PUD\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PUD\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PUD\_\-REG~MCUCR}\label{ATmega406_8h_4695ce5358406651354ca4f021d1d2d6}




Definition at line 701 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PWM\_\-TOTAL\_\-NUM@{PWM\_\-TOTAL\_\-NUM}}
\index{PWM\_\-TOTAL\_\-NUM@{PWM\_\-TOTAL\_\-NUM}!ATmega406.h@{ATmega406.h}}
\subsubsection[PWM\_\-TOTAL\_\-NUM]{\setlength{\rightskip}{0pt plus 5cm}\#define PWM\_\-TOTAL\_\-NUM~0}\label{ATmega406_8h_7cb4da096f48116b7ab3d837e16dd1e1}




Definition at line 75 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PWMOC\_\-REG@{PWMOC\_\-REG}}
\index{PWMOC\_\-REG@{PWMOC\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PWMOC\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PWMOC\_\-REG~FCSR}\label{ATmega406_8h_7c51dff52466f51931491dd7ba83ce6a}




Definition at line 327 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!PWMOPC\_\-REG@{PWMOPC\_\-REG}}
\index{PWMOPC\_\-REG@{PWMOPC\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[PWMOPC\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define PWMOPC\_\-REG~FCSR}\label{ATmega406_8h_430c54734e2997ff21a065645c25092d}




Definition at line 326 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!RWWSB\_\-REG@{RWWSB\_\-REG}}
\index{RWWSB\_\-REG@{RWWSB\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[RWWSB\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define RWWSB\_\-REG~SPMCSR}\label{ATmega406_8h_a49c40927ba6e250afac9c32118398d9}




Definition at line 414 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!RWWSRE\_\-REG@{RWWSRE\_\-REG}}
\index{RWWSRE\_\-REG@{RWWSRE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[RWWSRE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define RWWSRE\_\-REG~SPMCSR}\label{ATmega406_8h_5a79ba3615229f283e1e74d46b6800a3}




Definition at line 412 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!S\_\-REG@{S\_\-REG}}
\index{S\_\-REG@{S\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[S\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define S\_\-REG~SREG}\label{ATmega406_8h_d5c67a4893fa78c73eb10898d520766a}




Definition at line 148 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SCD\_\-REG@{SCD\_\-REG}}
\index{SCD\_\-REG@{SCD\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SCD\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SCD\_\-REG~BPCR}\label{ATmega406_8h_e3cc92921de560a1939c1e9c4a762294}




Definition at line 170 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SCDL0\_\-REG@{SCDL0\_\-REG}}
\index{SCDL0\_\-REG@{SCDL0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SCDL0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SCDL0\_\-REG~BPSCD}\label{ATmega406_8h_3e8198489e256066d84912971967e0d3}




Definition at line 516 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SCDL1\_\-REG@{SCDL1\_\-REG}}
\index{SCDL1\_\-REG@{SCDL1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SCDL1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SCDL1\_\-REG~BPSCD}\label{ATmega406_8h_6827a30dfa496ae299ce8941f6094118}




Definition at line 517 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SCDL2\_\-REG@{SCDL2\_\-REG}}
\index{SCDL2\_\-REG@{SCDL2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SCDL2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SCDL2\_\-REG~BPSCD}\label{ATmega406_8h_6176b6394e794049e8ae075fb077f3bf}




Definition at line 518 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SCDL3\_\-REG@{SCDL3\_\-REG}}
\index{SCDL3\_\-REG@{SCDL3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SCDL3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SCDL3\_\-REG~BPSCD}\label{ATmega406_8h_93e40beaf2b179a47a50c5b3c1d8f776}




Definition at line 519 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SCIE\_\-REG@{SCIE\_\-REG}}
\index{SCIE\_\-REG@{SCIE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SCIE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SCIE\_\-REG~BPIR}\label{ATmega406_8h_6f09d0d3a1f69da5a5e522749921ca85}




Definition at line 358 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SCIF\_\-REG@{SCIF\_\-REG}}
\index{SCIF\_\-REG@{SCIF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SCIF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SCIF\_\-REG~BPIR}\label{ATmega406_8h_44ce15569beb6b96080432b2ddda5df7}




Definition at line 362 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SCPT0\_\-REG@{SCPT0\_\-REG}}
\index{SCPT0\_\-REG@{SCPT0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SCPT0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SCPT0\_\-REG~CBPTR}\label{ATmega406_8h_0d4afdff57659f36d1dca010f550c818}




Definition at line 402 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SCPT1\_\-REG@{SCPT1\_\-REG}}
\index{SCPT1\_\-REG@{SCPT1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SCPT1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SCPT1\_\-REG~CBPTR}\label{ATmega406_8h_7d9476c4a85dd669c5c53f30bdcdf6a7}




Definition at line 403 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SCPT2\_\-REG@{SCPT2\_\-REG}}
\index{SCPT2\_\-REG@{SCPT2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SCPT2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SCPT2\_\-REG~CBPTR}\label{ATmega406_8h_f29c622cd97dcb0482e71101c9bebfcb}




Definition at line 404 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SCPT3\_\-REG@{SCPT3\_\-REG}}
\index{SCPT3\_\-REG@{SCPT3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SCPT3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SCPT3\_\-REG~CBPTR}\label{ATmega406_8h_be618a3487fa161c22425baa81fe2713}




Definition at line 405 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SE\_\-REG@{SE\_\-REG}}
\index{SE\_\-REG@{SE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SE\_\-REG~SMCR}\label{ATmega406_8h_3753fa832d100be472ba02984bafbb97}




Definition at line 469 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SIG\_\-INPUT\_\-CAPTURE\_\-TOTAL\_\-NUM@{SIG\_\-INPUT\_\-CAPTURE\_\-TOTAL\_\-NUM}}
\index{SIG\_\-INPUT\_\-CAPTURE\_\-TOTAL\_\-NUM@{SIG\_\-INPUT\_\-CAPTURE\_\-TOTAL\_\-NUM}!ATmega406.h@{ATmega406.h}}
\subsubsection[SIG\_\-INPUT\_\-CAPTURE\_\-TOTAL\_\-NUM]{\setlength{\rightskip}{0pt plus 5cm}\#define SIG\_\-INPUT\_\-CAPTURE\_\-TOTAL\_\-NUM~0}\label{ATmega406_8h_c42ea58970ddffa0fa9ee4be1fed0f2e}




Definition at line 78 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SIG\_\-OUTPUT\_\-COMPARE\_\-TOTAL\_\-NUM@{SIG\_\-OUTPUT\_\-COMPARE\_\-TOTAL\_\-NUM}}
\index{SIG\_\-OUTPUT\_\-COMPARE\_\-TOTAL\_\-NUM@{SIG\_\-OUTPUT\_\-COMPARE\_\-TOTAL\_\-NUM}!ATmega406.h@{ATmega406.h}}
\subsubsection[SIG\_\-OUTPUT\_\-COMPARE\_\-TOTAL\_\-NUM]{\setlength{\rightskip}{0pt plus 5cm}\#define SIG\_\-OUTPUT\_\-COMPARE\_\-TOTAL\_\-NUM~0}\label{ATmega406_8h_b79e450e7a2efdb68b3284986e261eb6}




Definition at line 72 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SIG\_\-OVERFLOW\_\-TOTAL\_\-NUM@{SIG\_\-OVERFLOW\_\-TOTAL\_\-NUM}}
\index{SIG\_\-OVERFLOW\_\-TOTAL\_\-NUM@{SIG\_\-OVERFLOW\_\-TOTAL\_\-NUM}!ATmega406.h@{ATmega406.h}}
\subsubsection[SIG\_\-OVERFLOW\_\-TOTAL\_\-NUM]{\setlength{\rightskip}{0pt plus 5cm}\#define SIG\_\-OVERFLOW\_\-TOTAL\_\-NUM~0}\label{ATmega406_8h_2d8b8ff307d3ab929cbfe927dcb4dedb}




Definition at line 69 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SIGRD\_\-REG@{SIGRD\_\-REG}}
\index{SIGRD\_\-REG@{SIGRD\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SIGRD\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SIGRD\_\-REG~SPMCSR}\label{ATmega406_8h_073b29aae3c3f2175ad89495285d0839}




Definition at line 413 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SM0\_\-REG@{SM0\_\-REG}}
\index{SM0\_\-REG@{SM0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SM0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SM0\_\-REG~SMCR}\label{ATmega406_8h_ecdc6672d1da1703528bb4c6a175cccd}




Definition at line 470 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SM1\_\-REG@{SM1\_\-REG}}
\index{SM1\_\-REG@{SM1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SM1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SM1\_\-REG~SMCR}\label{ATmega406_8h_cf3ed9d8a05266beda14d174c478aafe}




Definition at line 471 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SM2\_\-REG@{SM2\_\-REG}}
\index{SM2\_\-REG@{SM2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SM2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SM2\_\-REG~SMCR}\label{ATmega406_8h_518ceb13930595fb924655cf11ca929f}




Definition at line 472 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SP0\_\-REG@{SP0\_\-REG}}
\index{SP0\_\-REG@{SP0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SP0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SP0\_\-REG~SPL}\label{ATmega406_8h_5608c5fb647d16f5100e81ba32d53321}




Definition at line 330 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SP10\_\-REG@{SP10\_\-REG}}
\index{SP10\_\-REG@{SP10\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SP10\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SP10\_\-REG~SPH}\label{ATmega406_8h_82b9e11bea11d7278380f73ebd8b3e65}




Definition at line 300 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SP11\_\-REG@{SP11\_\-REG}}
\index{SP11\_\-REG@{SP11\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SP11\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SP11\_\-REG~SPH}\label{ATmega406_8h_83a324a8dfc1aefa1ecf888731fb8038}




Definition at line 301 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SP12\_\-REG@{SP12\_\-REG}}
\index{SP12\_\-REG@{SP12\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SP12\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SP12\_\-REG~SPH}\label{ATmega406_8h_0507d8ec64852e32084acbb2a1f02c73}




Definition at line 302 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SP13\_\-REG@{SP13\_\-REG}}
\index{SP13\_\-REG@{SP13\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SP13\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SP13\_\-REG~SPH}\label{ATmega406_8h_7cd2a6caf6bc98d15733f3392ce831fe}




Definition at line 303 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SP14\_\-REG@{SP14\_\-REG}}
\index{SP14\_\-REG@{SP14\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SP14\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SP14\_\-REG~SPH}\label{ATmega406_8h_20f5e9c3debe0298791627de76aa4d02}




Definition at line 304 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SP15\_\-REG@{SP15\_\-REG}}
\index{SP15\_\-REG@{SP15\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SP15\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SP15\_\-REG~SPH}\label{ATmega406_8h_97fdf98f15cbbfebbb2d0bb9ad8bda2d}




Definition at line 305 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SP1\_\-REG@{SP1\_\-REG}}
\index{SP1\_\-REG@{SP1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SP1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SP1\_\-REG~SPL}\label{ATmega406_8h_dcc9607ff34ab7b4442d36474ff4e64f}




Definition at line 331 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SP2\_\-REG@{SP2\_\-REG}}
\index{SP2\_\-REG@{SP2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SP2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SP2\_\-REG~SPL}\label{ATmega406_8h_1c046e06f5d6f64e29defa4a461881f6}




Definition at line 332 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SP3\_\-REG@{SP3\_\-REG}}
\index{SP3\_\-REG@{SP3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SP3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SP3\_\-REG~SPL}\label{ATmega406_8h_51ab7d3611a5aac013930eed859dc8dd}




Definition at line 333 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SP4\_\-REG@{SP4\_\-REG}}
\index{SP4\_\-REG@{SP4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SP4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SP4\_\-REG~SPL}\label{ATmega406_8h_6b1c6fa1974ceeef4a00a305a06e7196}




Definition at line 334 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SP5\_\-REG@{SP5\_\-REG}}
\index{SP5\_\-REG@{SP5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SP5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SP5\_\-REG~SPL}\label{ATmega406_8h_5fbfd4d58925f91318ad6134055bef03}




Definition at line 335 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SP6\_\-REG@{SP6\_\-REG}}
\index{SP6\_\-REG@{SP6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SP6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SP6\_\-REG~SPL}\label{ATmega406_8h_c0f324075c96f94eee13eb815e489011}




Definition at line 336 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SP7\_\-REG@{SP7\_\-REG}}
\index{SP7\_\-REG@{SP7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SP7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SP7\_\-REG~SPL}\label{ATmega406_8h_02c78d91b95bbb40b4b353bef14004b1}




Definition at line 337 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SP8\_\-REG@{SP8\_\-REG}}
\index{SP8\_\-REG@{SP8\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SP8\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SP8\_\-REG~SPH}\label{ATmega406_8h_604be5836f953abd148459e518e6da83}




Definition at line 298 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SP9\_\-REG@{SP9\_\-REG}}
\index{SP9\_\-REG@{SP9\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SP9\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SP9\_\-REG~SPH}\label{ATmega406_8h_947920343c0f3c53df283bd7dc6415a8}




Definition at line 299 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SPMEN\_\-REG@{SPMEN\_\-REG}}
\index{SPMEN\_\-REG@{SPMEN\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SPMEN\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SPMEN\_\-REG~SPMCSR}\label{ATmega406_8h_4de612ee44ba85f90ac3cf6e3c3afed9}




Definition at line 408 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!SPMIE\_\-REG@{SPMIE\_\-REG}}
\index{SPMIE\_\-REG@{SPMIE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[SPMIE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define SPMIE\_\-REG~SPMCSR}\label{ATmega406_8h_5da07c9aab4947a615b084b35617d357}




Definition at line 415 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!T0\_\-BIT@{T0\_\-BIT}}
\index{T0\_\-BIT@{T0\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[T0\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define T0\_\-BIT~0}\label{ATmega406_8h_adb4f7772697cd095ae5fb90aeec659f}




Definition at line 843 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!T0\_\-PORT@{T0\_\-PORT}}
\index{T0\_\-PORT@{T0\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[T0\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define T0\_\-PORT~PORTD}\label{ATmega406_8h_217613f31ebd791655795b26f7344827}




Definition at line 842 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!T\_\-REG@{T\_\-REG}}
\index{T\_\-REG@{T\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[T\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define T\_\-REG~SREG}\label{ATmega406_8h_109aeb5473f651bba0263dbf92c97221}




Definition at line 150 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCK\_\-BIT@{TCK\_\-BIT}}
\index{TCK\_\-BIT@{TCK\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCK\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define TCK\_\-BIT~3}\label{ATmega406_8h_eabdd3d190f93493ddd6c24d2c9f1e42}




Definition at line 821 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCK\_\-PORT@{TCK\_\-PORT}}
\index{TCK\_\-PORT@{TCK\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCK\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define TCK\_\-PORT~PORTB}\label{ATmega406_8h_3c9ea2886017851574d28a6a4b1d17bc}




Definition at line 820 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT00\_\-REG@{TCNT00\_\-REG}}
\index{TCNT00\_\-REG@{TCNT00\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT00\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT00\_\-REG~TCNT0}\label{ATmega406_8h_9127d2f865133ffabd991da175ecd586}




Definition at line 522 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT01\_\-REG@{TCNT01\_\-REG}}
\index{TCNT01\_\-REG@{TCNT01\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT01\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT01\_\-REG~TCNT0}\label{ATmega406_8h_c532980be61a57a37d9c6c55ec019f54}




Definition at line 523 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT02\_\-REG@{TCNT02\_\-REG}}
\index{TCNT02\_\-REG@{TCNT02\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT02\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT02\_\-REG~TCNT0}\label{ATmega406_8h_e6d4e46a963b050c2ec6c1251a74c325}




Definition at line 524 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT03\_\-REG@{TCNT03\_\-REG}}
\index{TCNT03\_\-REG@{TCNT03\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT03\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT03\_\-REG~TCNT0}\label{ATmega406_8h_d951b9b59a68391883abc6f8dec42878}




Definition at line 525 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT04\_\-REG@{TCNT04\_\-REG}}
\index{TCNT04\_\-REG@{TCNT04\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT04\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT04\_\-REG~TCNT0}\label{ATmega406_8h_93154558aa471f041498d5059d642db0}




Definition at line 526 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT05\_\-REG@{TCNT05\_\-REG}}
\index{TCNT05\_\-REG@{TCNT05\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT05\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT05\_\-REG~TCNT0}\label{ATmega406_8h_040cf51192eb15a6e32e67a52986616e}




Definition at line 527 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT06\_\-REG@{TCNT06\_\-REG}}
\index{TCNT06\_\-REG@{TCNT06\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT06\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT06\_\-REG~TCNT0}\label{ATmega406_8h_25751be7558b74a2ac1d7a1307268778}




Definition at line 528 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT07\_\-REG@{TCNT07\_\-REG}}
\index{TCNT07\_\-REG@{TCNT07\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT07\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT07\_\-REG~TCNT0}\label{ATmega406_8h_d58b3778d28983c5d604edb26315536f}




Definition at line 529 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT1H0\_\-REG@{TCNT1H0\_\-REG}}
\index{TCNT1H0\_\-REG@{TCNT1H0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT1H0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT1H0\_\-REG~TCNT1H}\label{ATmega406_8h_a25ece3bdccc712500a9fb51af5fe557}




Definition at line 475 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT1H1\_\-REG@{TCNT1H1\_\-REG}}
\index{TCNT1H1\_\-REG@{TCNT1H1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT1H1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT1H1\_\-REG~TCNT1H}\label{ATmega406_8h_d97ed8249b922cc19cecc021c12ea783}




Definition at line 476 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT1H2\_\-REG@{TCNT1H2\_\-REG}}
\index{TCNT1H2\_\-REG@{TCNT1H2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT1H2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT1H2\_\-REG~TCNT1H}\label{ATmega406_8h_f578b228d973cb4d616eb51d37765697}




Definition at line 477 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT1H3\_\-REG@{TCNT1H3\_\-REG}}
\index{TCNT1H3\_\-REG@{TCNT1H3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT1H3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT1H3\_\-REG~TCNT1H}\label{ATmega406_8h_5627b674239b3c237b3327a6fe72bbbd}




Definition at line 478 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT1H4\_\-REG@{TCNT1H4\_\-REG}}
\index{TCNT1H4\_\-REG@{TCNT1H4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT1H4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT1H4\_\-REG~TCNT1H}\label{ATmega406_8h_23dc0075885d6a295d9b2044f65170d0}




Definition at line 479 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT1H5\_\-REG@{TCNT1H5\_\-REG}}
\index{TCNT1H5\_\-REG@{TCNT1H5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT1H5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT1H5\_\-REG~TCNT1H}\label{ATmega406_8h_93aa52885a457f46936c4501fdad82ff}




Definition at line 480 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT1H6\_\-REG@{TCNT1H6\_\-REG}}
\index{TCNT1H6\_\-REG@{TCNT1H6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT1H6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT1H6\_\-REG~TCNT1H}\label{ATmega406_8h_4d94dde3b93ff056ff7ceb0774907803}




Definition at line 481 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT1H7\_\-REG@{TCNT1H7\_\-REG}}
\index{TCNT1H7\_\-REG@{TCNT1H7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT1H7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT1H7\_\-REG~TCNT1H}\label{ATmega406_8h_94072c2c6d4a730d86ad0a3d91375e44}




Definition at line 482 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT1L0\_\-REG@{TCNT1L0\_\-REG}}
\index{TCNT1L0\_\-REG@{TCNT1L0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT1L0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT1L0\_\-REG~TCNT1L}\label{ATmega406_8h_188d60f8d09fc037b9c5a8cb850f620d}




Definition at line 445 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT1L1\_\-REG@{TCNT1L1\_\-REG}}
\index{TCNT1L1\_\-REG@{TCNT1L1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT1L1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT1L1\_\-REG~TCNT1L}\label{ATmega406_8h_7ae20ef3144cb261ffbc188904aa6fc8}




Definition at line 446 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT1L2\_\-REG@{TCNT1L2\_\-REG}}
\index{TCNT1L2\_\-REG@{TCNT1L2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT1L2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT1L2\_\-REG~TCNT1L}\label{ATmega406_8h_9d359e3c9797388743e07f62cd6a7f69}




Definition at line 447 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT1L3\_\-REG@{TCNT1L3\_\-REG}}
\index{TCNT1L3\_\-REG@{TCNT1L3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT1L3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT1L3\_\-REG~TCNT1L}\label{ATmega406_8h_60acfda9c5f3665a29d7fc035cc14e9f}




Definition at line 448 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT1L4\_\-REG@{TCNT1L4\_\-REG}}
\index{TCNT1L4\_\-REG@{TCNT1L4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT1L4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT1L4\_\-REG~TCNT1L}\label{ATmega406_8h_3372b7f2a7af05e0763489f98de9acbb}




Definition at line 449 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT1L5\_\-REG@{TCNT1L5\_\-REG}}
\index{TCNT1L5\_\-REG@{TCNT1L5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT1L5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT1L5\_\-REG~TCNT1L}\label{ATmega406_8h_b799b9cca3dc49d5eeccb878498a54d6}




Definition at line 450 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT1L6\_\-REG@{TCNT1L6\_\-REG}}
\index{TCNT1L6\_\-REG@{TCNT1L6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT1L6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT1L6\_\-REG~TCNT1L}\label{ATmega406_8h_0b9c322bd0d2e05fba2d599682f68577}




Definition at line 451 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TCNT1L7\_\-REG@{TCNT1L7\_\-REG}}
\index{TCNT1L7\_\-REG@{TCNT1L7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TCNT1L7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TCNT1L7\_\-REG~TCNT1L}\label{ATmega406_8h_d79699eade7a8ffaa386919f3b7495df}




Definition at line 452 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TDI\_\-BIT@{TDI\_\-BIT}}
\index{TDI\_\-BIT@{TDI\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[TDI\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define TDI\_\-BIT~1}\label{ATmega406_8h_767c6ea12bdc0ab3e9738626470caef9}




Definition at line 811 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TDI\_\-PORT@{TDI\_\-PORT}}
\index{TDI\_\-PORT@{TDI\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[TDI\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define TDI\_\-PORT~PORTB}\label{ATmega406_8h_698f4d257e96c22ffa82dd891e83f05e}




Definition at line 810 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TDO\_\-BIT@{TDO\_\-BIT}}
\index{TDO\_\-BIT@{TDO\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[TDO\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define TDO\_\-BIT~0}\label{ATmega406_8h_b455ca827f4e2795d4ba9eb4c58fa69c}




Definition at line 806 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TDO\_\-PORT@{TDO\_\-PORT}}
\index{TDO\_\-PORT@{TDO\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[TDO\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define TDO\_\-PORT~PORTB}\label{ATmega406_8h_c8159a00d7a31eb94b3fd5aadd90dd39}




Definition at line 805 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER0\_\-PRESCALER\_\-DIV\_\-0@{TIMER0\_\-PRESCALER\_\-DIV\_\-0}}
\index{TIMER0\_\-PRESCALER\_\-DIV\_\-0@{TIMER0\_\-PRESCALER\_\-DIV\_\-0}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER0\_\-PRESCALER\_\-DIV\_\-0]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER0\_\-PRESCALER\_\-DIV\_\-0~0}\label{ATmega406_8h_c66ec013fa597474117c127351bedced}




Definition at line 28 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER0\_\-PRESCALER\_\-DIV\_\-1@{TIMER0\_\-PRESCALER\_\-DIV\_\-1}}
\index{TIMER0\_\-PRESCALER\_\-DIV\_\-1@{TIMER0\_\-PRESCALER\_\-DIV\_\-1}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER0\_\-PRESCALER\_\-DIV\_\-1]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER0\_\-PRESCALER\_\-DIV\_\-1~1}\label{ATmega406_8h_d60a9603ee404b402b1b7652b419614a}




Definition at line 29 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER0\_\-PRESCALER\_\-DIV\_\-1024@{TIMER0\_\-PRESCALER\_\-DIV\_\-1024}}
\index{TIMER0\_\-PRESCALER\_\-DIV\_\-1024@{TIMER0\_\-PRESCALER\_\-DIV\_\-1024}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER0\_\-PRESCALER\_\-DIV\_\-1024]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER0\_\-PRESCALER\_\-DIV\_\-1024~5}\label{ATmega406_8h_972da851dcc6b09922511e1284edc36e}




Definition at line 33 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER0\_\-PRESCALER\_\-DIV\_\-256@{TIMER0\_\-PRESCALER\_\-DIV\_\-256}}
\index{TIMER0\_\-PRESCALER\_\-DIV\_\-256@{TIMER0\_\-PRESCALER\_\-DIV\_\-256}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER0\_\-PRESCALER\_\-DIV\_\-256]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER0\_\-PRESCALER\_\-DIV\_\-256~4}\label{ATmega406_8h_668e89427212bdd50a9fc22780627bdd}




Definition at line 32 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER0\_\-PRESCALER\_\-DIV\_\-64@{TIMER0\_\-PRESCALER\_\-DIV\_\-64}}
\index{TIMER0\_\-PRESCALER\_\-DIV\_\-64@{TIMER0\_\-PRESCALER\_\-DIV\_\-64}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER0\_\-PRESCALER\_\-DIV\_\-64]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER0\_\-PRESCALER\_\-DIV\_\-64~3}\label{ATmega406_8h_1ff030cae6ddd509d1dc8a34ef020a10}




Definition at line 31 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER0\_\-PRESCALER\_\-DIV\_\-8@{TIMER0\_\-PRESCALER\_\-DIV\_\-8}}
\index{TIMER0\_\-PRESCALER\_\-DIV\_\-8@{TIMER0\_\-PRESCALER\_\-DIV\_\-8}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER0\_\-PRESCALER\_\-DIV\_\-8]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER0\_\-PRESCALER\_\-DIV\_\-8~2}\label{ATmega406_8h_83262dc8806bd35b95e39c7f4ad660dc}




Definition at line 30 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER0\_\-PRESCALER\_\-DIV\_\-FALL@{TIMER0\_\-PRESCALER\_\-DIV\_\-FALL}}
\index{TIMER0\_\-PRESCALER\_\-DIV\_\-FALL@{TIMER0\_\-PRESCALER\_\-DIV\_\-FALL}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER0\_\-PRESCALER\_\-DIV\_\-FALL]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER0\_\-PRESCALER\_\-DIV\_\-FALL~6}\label{ATmega406_8h_c67439191efe80613cbefa35399a776f}




Definition at line 34 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER0\_\-PRESCALER\_\-DIV\_\-RISE@{TIMER0\_\-PRESCALER\_\-DIV\_\-RISE}}
\index{TIMER0\_\-PRESCALER\_\-DIV\_\-RISE@{TIMER0\_\-PRESCALER\_\-DIV\_\-RISE}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER0\_\-PRESCALER\_\-DIV\_\-RISE]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER0\_\-PRESCALER\_\-DIV\_\-RISE~7}\label{ATmega406_8h_5deaad711ed0f159d7bf19beb594c577}




Definition at line 35 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER0\_\-PRESCALER\_\-REG\_\-0@{TIMER0\_\-PRESCALER\_\-REG\_\-0}}
\index{TIMER0\_\-PRESCALER\_\-REG\_\-0@{TIMER0\_\-PRESCALER\_\-REG\_\-0}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER0\_\-PRESCALER\_\-REG\_\-0]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER0\_\-PRESCALER\_\-REG\_\-0~0}\label{ATmega406_8h_8143ac91326ffcd96d2acd33924cc3aa}




Definition at line 37 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER0\_\-PRESCALER\_\-REG\_\-1@{TIMER0\_\-PRESCALER\_\-REG\_\-1}}
\index{TIMER0\_\-PRESCALER\_\-REG\_\-1@{TIMER0\_\-PRESCALER\_\-REG\_\-1}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER0\_\-PRESCALER\_\-REG\_\-1]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER0\_\-PRESCALER\_\-REG\_\-1~1}\label{ATmega406_8h_c88125b4d75100eb292b9a366c4bd5c6}




Definition at line 38 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER0\_\-PRESCALER\_\-REG\_\-2@{TIMER0\_\-PRESCALER\_\-REG\_\-2}}
\index{TIMER0\_\-PRESCALER\_\-REG\_\-2@{TIMER0\_\-PRESCALER\_\-REG\_\-2}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER0\_\-PRESCALER\_\-REG\_\-2]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER0\_\-PRESCALER\_\-REG\_\-2~8}\label{ATmega406_8h_655e86d55af2afe0033b3d8bf2aceb20}




Definition at line 39 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER0\_\-PRESCALER\_\-REG\_\-3@{TIMER0\_\-PRESCALER\_\-REG\_\-3}}
\index{TIMER0\_\-PRESCALER\_\-REG\_\-3@{TIMER0\_\-PRESCALER\_\-REG\_\-3}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER0\_\-PRESCALER\_\-REG\_\-3]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER0\_\-PRESCALER\_\-REG\_\-3~64}\label{ATmega406_8h_cae86407c26e1b79197011862a53b366}




Definition at line 40 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER0\_\-PRESCALER\_\-REG\_\-4@{TIMER0\_\-PRESCALER\_\-REG\_\-4}}
\index{TIMER0\_\-PRESCALER\_\-REG\_\-4@{TIMER0\_\-PRESCALER\_\-REG\_\-4}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER0\_\-PRESCALER\_\-REG\_\-4]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER0\_\-PRESCALER\_\-REG\_\-4~256}\label{ATmega406_8h_6c2a877eb19568271dd956d347d22372}




Definition at line 41 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER0\_\-PRESCALER\_\-REG\_\-5@{TIMER0\_\-PRESCALER\_\-REG\_\-5}}
\index{TIMER0\_\-PRESCALER\_\-REG\_\-5@{TIMER0\_\-PRESCALER\_\-REG\_\-5}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER0\_\-PRESCALER\_\-REG\_\-5]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER0\_\-PRESCALER\_\-REG\_\-5~1024}\label{ATmega406_8h_042c7933f29f1014ba3277b5103e6186}




Definition at line 42 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER0\_\-PRESCALER\_\-REG\_\-6@{TIMER0\_\-PRESCALER\_\-REG\_\-6}}
\index{TIMER0\_\-PRESCALER\_\-REG\_\-6@{TIMER0\_\-PRESCALER\_\-REG\_\-6}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER0\_\-PRESCALER\_\-REG\_\-6]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER0\_\-PRESCALER\_\-REG\_\-6~-1}\label{ATmega406_8h_95d957994107d6a2b5c7f6fa9453322d}




Definition at line 43 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER0\_\-PRESCALER\_\-REG\_\-7@{TIMER0\_\-PRESCALER\_\-REG\_\-7}}
\index{TIMER0\_\-PRESCALER\_\-REG\_\-7@{TIMER0\_\-PRESCALER\_\-REG\_\-7}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER0\_\-PRESCALER\_\-REG\_\-7]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER0\_\-PRESCALER\_\-REG\_\-7~-2}\label{ATmega406_8h_0b5413f6b78514d3aa97adbc8be48895}




Definition at line 44 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER1\_\-PRESCALER\_\-DIV\_\-0@{TIMER1\_\-PRESCALER\_\-DIV\_\-0}}
\index{TIMER1\_\-PRESCALER\_\-DIV\_\-0@{TIMER1\_\-PRESCALER\_\-DIV\_\-0}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER1\_\-PRESCALER\_\-DIV\_\-0]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER1\_\-PRESCALER\_\-DIV\_\-0~0}\label{ATmega406_8h_f1c1d4d979d1f563be962db8b145fbbf}




Definition at line 47 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER1\_\-PRESCALER\_\-DIV\_\-1@{TIMER1\_\-PRESCALER\_\-DIV\_\-1}}
\index{TIMER1\_\-PRESCALER\_\-DIV\_\-1@{TIMER1\_\-PRESCALER\_\-DIV\_\-1}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER1\_\-PRESCALER\_\-DIV\_\-1]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER1\_\-PRESCALER\_\-DIV\_\-1~1}\label{ATmega406_8h_00903327b93ba9aa8e5b61d970854436}




Definition at line 48 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER1\_\-PRESCALER\_\-DIV\_\-1024@{TIMER1\_\-PRESCALER\_\-DIV\_\-1024}}
\index{TIMER1\_\-PRESCALER\_\-DIV\_\-1024@{TIMER1\_\-PRESCALER\_\-DIV\_\-1024}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER1\_\-PRESCALER\_\-DIV\_\-1024]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER1\_\-PRESCALER\_\-DIV\_\-1024~7}\label{ATmega406_8h_0ad10baa71b1ca91c19048016f05017c}




Definition at line 54 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER1\_\-PRESCALER\_\-DIV\_\-128@{TIMER1\_\-PRESCALER\_\-DIV\_\-128}}
\index{TIMER1\_\-PRESCALER\_\-DIV\_\-128@{TIMER1\_\-PRESCALER\_\-DIV\_\-128}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER1\_\-PRESCALER\_\-DIV\_\-128]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER1\_\-PRESCALER\_\-DIV\_\-128~5}\label{ATmega406_8h_f666cc1840d7b4d6b8480dcc5109ed25}




Definition at line 52 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER1\_\-PRESCALER\_\-DIV\_\-256@{TIMER1\_\-PRESCALER\_\-DIV\_\-256}}
\index{TIMER1\_\-PRESCALER\_\-DIV\_\-256@{TIMER1\_\-PRESCALER\_\-DIV\_\-256}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER1\_\-PRESCALER\_\-DIV\_\-256]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER1\_\-PRESCALER\_\-DIV\_\-256~6}\label{ATmega406_8h_39b2b2e4d200fcfc3d3e37c639509709}




Definition at line 53 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER1\_\-PRESCALER\_\-DIV\_\-32@{TIMER1\_\-PRESCALER\_\-DIV\_\-32}}
\index{TIMER1\_\-PRESCALER\_\-DIV\_\-32@{TIMER1\_\-PRESCALER\_\-DIV\_\-32}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER1\_\-PRESCALER\_\-DIV\_\-32]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER1\_\-PRESCALER\_\-DIV\_\-32~3}\label{ATmega406_8h_350ffd98baea847a46cc9afc809a3e61}




Definition at line 50 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER1\_\-PRESCALER\_\-DIV\_\-64@{TIMER1\_\-PRESCALER\_\-DIV\_\-64}}
\index{TIMER1\_\-PRESCALER\_\-DIV\_\-64@{TIMER1\_\-PRESCALER\_\-DIV\_\-64}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER1\_\-PRESCALER\_\-DIV\_\-64]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER1\_\-PRESCALER\_\-DIV\_\-64~4}\label{ATmega406_8h_d45561073141104680888376d87c045c}




Definition at line 51 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER1\_\-PRESCALER\_\-DIV\_\-8@{TIMER1\_\-PRESCALER\_\-DIV\_\-8}}
\index{TIMER1\_\-PRESCALER\_\-DIV\_\-8@{TIMER1\_\-PRESCALER\_\-DIV\_\-8}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER1\_\-PRESCALER\_\-DIV\_\-8]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER1\_\-PRESCALER\_\-DIV\_\-8~2}\label{ATmega406_8h_8d2fa60e55354b71578efeebc62c2041}




Definition at line 49 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER1\_\-PRESCALER\_\-REG\_\-0@{TIMER1\_\-PRESCALER\_\-REG\_\-0}}
\index{TIMER1\_\-PRESCALER\_\-REG\_\-0@{TIMER1\_\-PRESCALER\_\-REG\_\-0}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER1\_\-PRESCALER\_\-REG\_\-0]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER1\_\-PRESCALER\_\-REG\_\-0~0}\label{ATmega406_8h_c09431aad889913350bf739bd1e551f8}




Definition at line 56 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER1\_\-PRESCALER\_\-REG\_\-1@{TIMER1\_\-PRESCALER\_\-REG\_\-1}}
\index{TIMER1\_\-PRESCALER\_\-REG\_\-1@{TIMER1\_\-PRESCALER\_\-REG\_\-1}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER1\_\-PRESCALER\_\-REG\_\-1]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER1\_\-PRESCALER\_\-REG\_\-1~1}\label{ATmega406_8h_3ca66f6a9cf2c7dd589bf1f839b8ca53}




Definition at line 57 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER1\_\-PRESCALER\_\-REG\_\-2@{TIMER1\_\-PRESCALER\_\-REG\_\-2}}
\index{TIMER1\_\-PRESCALER\_\-REG\_\-2@{TIMER1\_\-PRESCALER\_\-REG\_\-2}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER1\_\-PRESCALER\_\-REG\_\-2]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER1\_\-PRESCALER\_\-REG\_\-2~8}\label{ATmega406_8h_609a70f0a21cc0402185cb2bc3987c98}




Definition at line 58 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER1\_\-PRESCALER\_\-REG\_\-3@{TIMER1\_\-PRESCALER\_\-REG\_\-3}}
\index{TIMER1\_\-PRESCALER\_\-REG\_\-3@{TIMER1\_\-PRESCALER\_\-REG\_\-3}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER1\_\-PRESCALER\_\-REG\_\-3]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER1\_\-PRESCALER\_\-REG\_\-3~32}\label{ATmega406_8h_dc43c349d2e4c5bac8815c65cb54c547}




Definition at line 59 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER1\_\-PRESCALER\_\-REG\_\-4@{TIMER1\_\-PRESCALER\_\-REG\_\-4}}
\index{TIMER1\_\-PRESCALER\_\-REG\_\-4@{TIMER1\_\-PRESCALER\_\-REG\_\-4}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER1\_\-PRESCALER\_\-REG\_\-4]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER1\_\-PRESCALER\_\-REG\_\-4~64}\label{ATmega406_8h_b5bf5eadef1837eec749d1fc167e30a0}




Definition at line 60 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER1\_\-PRESCALER\_\-REG\_\-5@{TIMER1\_\-PRESCALER\_\-REG\_\-5}}
\index{TIMER1\_\-PRESCALER\_\-REG\_\-5@{TIMER1\_\-PRESCALER\_\-REG\_\-5}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER1\_\-PRESCALER\_\-REG\_\-5]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER1\_\-PRESCALER\_\-REG\_\-5~128}\label{ATmega406_8h_7b96ecfe303fdcc1c5bf136fe7a961ed}




Definition at line 61 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER1\_\-PRESCALER\_\-REG\_\-6@{TIMER1\_\-PRESCALER\_\-REG\_\-6}}
\index{TIMER1\_\-PRESCALER\_\-REG\_\-6@{TIMER1\_\-PRESCALER\_\-REG\_\-6}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER1\_\-PRESCALER\_\-REG\_\-6]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER1\_\-PRESCALER\_\-REG\_\-6~256}\label{ATmega406_8h_d600912867da52934f54803c6fbf8c6c}




Definition at line 62 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TIMER1\_\-PRESCALER\_\-REG\_\-7@{TIMER1\_\-PRESCALER\_\-REG\_\-7}}
\index{TIMER1\_\-PRESCALER\_\-REG\_\-7@{TIMER1\_\-PRESCALER\_\-REG\_\-7}!ATmega406.h@{ATmega406.h}}
\subsubsection[TIMER1\_\-PRESCALER\_\-REG\_\-7]{\setlength{\rightskip}{0pt plus 5cm}\#define TIMER1\_\-PRESCALER\_\-REG\_\-7~1024}\label{ATmega406_8h_b9b860fdea605509ceca7a558534f127}




Definition at line 63 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TMS\_\-BIT@{TMS\_\-BIT}}
\index{TMS\_\-BIT@{TMS\_\-BIT}!ATmega406.h@{ATmega406.h}}
\subsubsection[TMS\_\-BIT]{\setlength{\rightskip}{0pt plus 5cm}\#define TMS\_\-BIT~2}\label{ATmega406_8h_d7c86b074d6726ee0eeac30932996b9e}




Definition at line 816 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TMS\_\-PORT@{TMS\_\-PORT}}
\index{TMS\_\-PORT@{TMS\_\-PORT}!ATmega406.h@{ATmega406.h}}
\subsubsection[TMS\_\-PORT]{\setlength{\rightskip}{0pt plus 5cm}\#define TMS\_\-PORT~PORTB}\label{ATmega406_8h_018c2e96f97253298d2c1ca084c0421e}




Definition at line 815 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TOIE0\_\-REG@{TOIE0\_\-REG}}
\index{TOIE0\_\-REG@{TOIE0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TOIE0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TOIE0\_\-REG~TIMSK0}\label{ATmega406_8h_5a635571a56f1fb59e3b884aa073d512}




Definition at line 582 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TOIE1\_\-REG@{TOIE1\_\-REG}}
\index{TOIE1\_\-REG@{TOIE1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TOIE1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TOIE1\_\-REG~TIMSK1}\label{ATmega406_8h_72a162fa56af8033ce7ef5691d9c0800}




Definition at line 587 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TOV0\_\-REG@{TOV0\_\-REG}}
\index{TOV0\_\-REG@{TOV0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TOV0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TOV0\_\-REG~TIFR0}\label{ATmega406_8h_09d5f62889c143cea3fa808f861dfb42}




Definition at line 754 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TOV1\_\-REG@{TOV1\_\-REG}}
\index{TOV1\_\-REG@{TOV1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TOV1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TOV1\_\-REG~TIFR1}\label{ATmega406_8h_790eacbd141db2ee7206f580472434d0}




Definition at line 759 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TSM\_\-REG@{TSM\_\-REG}}
\index{TSM\_\-REG@{TSM\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TSM\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TSM\_\-REG~GTCCR}\label{ATmega406_8h_632ccca1330e774c17d0222764857134}




Definition at line 209 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWA0\_\-REG@{TWA0\_\-REG}}
\index{TWA0\_\-REG@{TWA0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWA0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWA0\_\-REG~TWAR}\label{ATmega406_8h_1a0e38420a034a62f6897287dcf56499}




Definition at line 553 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWA1\_\-REG@{TWA1\_\-REG}}
\index{TWA1\_\-REG@{TWA1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWA1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWA1\_\-REG~TWAR}\label{ATmega406_8h_fc29b9bcdba3841a69927f6dddc2fca6}




Definition at line 554 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWA2\_\-REG@{TWA2\_\-REG}}
\index{TWA2\_\-REG@{TWA2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWA2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWA2\_\-REG~TWAR}\label{ATmega406_8h_43b1d6907774b3461eed60572d049a62}




Definition at line 555 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWA3\_\-REG@{TWA3\_\-REG}}
\index{TWA3\_\-REG@{TWA3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWA3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWA3\_\-REG~TWAR}\label{ATmega406_8h_305511cde71c015669574514017e3c00}




Definition at line 556 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWA4\_\-REG@{TWA4\_\-REG}}
\index{TWA4\_\-REG@{TWA4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWA4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWA4\_\-REG~TWAR}\label{ATmega406_8h_1ac37d7ff58e663f09abef2e9eeea4dd}




Definition at line 557 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWA5\_\-REG@{TWA5\_\-REG}}
\index{TWA5\_\-REG@{TWA5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWA5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWA5\_\-REG~TWAR}\label{ATmega406_8h_c4fb46413e2af6f80f1d0c260a598008}




Definition at line 558 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWA6\_\-REG@{TWA6\_\-REG}}
\index{TWA6\_\-REG@{TWA6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWA6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWA6\_\-REG~TWAR}\label{ATmega406_8h_30fd6fd2e2fe3d796daa4c78a91cc771}




Definition at line 559 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWAM0\_\-REG@{TWAM0\_\-REG}}
\index{TWAM0\_\-REG@{TWAM0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWAM0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWAM0\_\-REG~TWAMR}\label{ATmega406_8h_95b32075ecfca5f4c50ae617eb259550}




Definition at line 488 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWAM1\_\-REG@{TWAM1\_\-REG}}
\index{TWAM1\_\-REG@{TWAM1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWAM1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWAM1\_\-REG~TWAMR}\label{ATmega406_8h_4cb85b48fb7dcde8b0f645a9294ce6a5}




Definition at line 489 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWAM2\_\-REG@{TWAM2\_\-REG}}
\index{TWAM2\_\-REG@{TWAM2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWAM2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWAM2\_\-REG~TWAMR}\label{ATmega406_8h_abd2e3224ab9d052923e53f4951d48ff}




Definition at line 490 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWAM3\_\-REG@{TWAM3\_\-REG}}
\index{TWAM3\_\-REG@{TWAM3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWAM3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWAM3\_\-REG~TWAMR}\label{ATmega406_8h_5ecbca4c463741a6214e1a03b6e303dc}




Definition at line 491 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWAM4\_\-REG@{TWAM4\_\-REG}}
\index{TWAM4\_\-REG@{TWAM4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWAM4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWAM4\_\-REG~TWAMR}\label{ATmega406_8h_e4c38ec53cdd5f3a6fcc4982af13ca8e}




Definition at line 492 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWAM5\_\-REG@{TWAM5\_\-REG}}
\index{TWAM5\_\-REG@{TWAM5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWAM5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWAM5\_\-REG~TWAMR}\label{ATmega406_8h_189157aafba758bbe678caa4c0607437}




Definition at line 493 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWAM6\_\-REG@{TWAM6\_\-REG}}
\index{TWAM6\_\-REG@{TWAM6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWAM6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWAM6\_\-REG~TWAMR}\label{ATmega406_8h_fe0b79b55406182671e246e8c2c8e8b5}




Definition at line 494 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWBCIE\_\-REG@{TWBCIE\_\-REG}}
\index{TWBCIE\_\-REG@{TWBCIE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWBCIE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWBCIE\_\-REG~TWBCSR}\label{ATmega406_8h_0893b1e87dda18a402b2b1fd4c732be8}




Definition at line 714 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWBCIF\_\-REG@{TWBCIF\_\-REG}}
\index{TWBCIF\_\-REG@{TWBCIF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWBCIF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWBCIF\_\-REG~TWBCSR}\label{ATmega406_8h_383cc818806dda857e9e0eae70061c25}




Definition at line 715 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWBCIP\_\-REG@{TWBCIP\_\-REG}}
\index{TWBCIP\_\-REG@{TWBCIP\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWBCIP\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWBCIP\_\-REG~TWBCSR}\label{ATmega406_8h_be906b2700318b79acc4e71b4f635c69}




Definition at line 711 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWBDT0\_\-REG@{TWBDT0\_\-REG}}
\index{TWBDT0\_\-REG@{TWBDT0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWBDT0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWBDT0\_\-REG~TWBCSR}\label{ATmega406_8h_b42ff7010acae4ed84ff8531735012a6}




Definition at line 712 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWBDT1\_\-REG@{TWBDT1\_\-REG}}
\index{TWBDT1\_\-REG@{TWBDT1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWBDT1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWBDT1\_\-REG~TWBCSR}\label{ATmega406_8h_805701f2119de9626d1ae61455c80d3e}




Definition at line 713 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWBR0\_\-REG@{TWBR0\_\-REG}}
\index{TWBR0\_\-REG@{TWBR0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWBR0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWBR0\_\-REG~TWBR}\label{ATmega406_8h_2c3248e632f67474e0cc8b75b9522d17}




Definition at line 212 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWBR1\_\-REG@{TWBR1\_\-REG}}
\index{TWBR1\_\-REG@{TWBR1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWBR1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWBR1\_\-REG~TWBR}\label{ATmega406_8h_6d881eb4e39ae66c50271b3af989230a}




Definition at line 213 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWBR2\_\-REG@{TWBR2\_\-REG}}
\index{TWBR2\_\-REG@{TWBR2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWBR2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWBR2\_\-REG~TWBR}\label{ATmega406_8h_b384ae85eac88a85bdcd192b41ff2f6a}




Definition at line 214 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWBR3\_\-REG@{TWBR3\_\-REG}}
\index{TWBR3\_\-REG@{TWBR3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWBR3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWBR3\_\-REG~TWBR}\label{ATmega406_8h_e50d13ed20901c9c72c4e63e3d7fad04}




Definition at line 215 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWBR4\_\-REG@{TWBR4\_\-REG}}
\index{TWBR4\_\-REG@{TWBR4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWBR4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWBR4\_\-REG~TWBR}\label{ATmega406_8h_df945bf290de24cfd55e8528a35a45f9}




Definition at line 216 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWBR5\_\-REG@{TWBR5\_\-REG}}
\index{TWBR5\_\-REG@{TWBR5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWBR5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWBR5\_\-REG~TWBR}\label{ATmega406_8h_538ccc3fd51667f02ea9fcf60671c766}




Definition at line 217 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWBR6\_\-REG@{TWBR6\_\-REG}}
\index{TWBR6\_\-REG@{TWBR6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWBR6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWBR6\_\-REG~TWBR}\label{ATmega406_8h_0958d2a95319b2a461ee7ca690ea0ce4}




Definition at line 218 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWBR7\_\-REG@{TWBR7\_\-REG}}
\index{TWBR7\_\-REG@{TWBR7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWBR7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWBR7\_\-REG~TWBR}\label{ATmega406_8h_38df7853beb30664f71fd7a6008cd746}




Definition at line 219 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWD0\_\-REG@{TWD0\_\-REG}}
\index{TWD0\_\-REG@{TWD0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWD0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWD0\_\-REG~TWDR}\label{ATmega406_8h_b0751fda327a1f870c3a4249bc9e5750}




Definition at line 194 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWD1\_\-REG@{TWD1\_\-REG}}
\index{TWD1\_\-REG@{TWD1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWD1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWD1\_\-REG~TWDR}\label{ATmega406_8h_033dfd7729a97c1fb98354a926dbb2df}




Definition at line 195 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWD2\_\-REG@{TWD2\_\-REG}}
\index{TWD2\_\-REG@{TWD2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWD2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWD2\_\-REG~TWDR}\label{ATmega406_8h_e5532ff1a52569720a9a44c1129772b0}




Definition at line 196 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWD3\_\-REG@{TWD3\_\-REG}}
\index{TWD3\_\-REG@{TWD3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWD3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWD3\_\-REG~TWDR}\label{ATmega406_8h_d77199f21ac4f230028e9a9ef46cd4d0}




Definition at line 197 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWD4\_\-REG@{TWD4\_\-REG}}
\index{TWD4\_\-REG@{TWD4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWD4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWD4\_\-REG~TWDR}\label{ATmega406_8h_1b9483e732fbd4df4e190ac5fe3dcc27}




Definition at line 198 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWD5\_\-REG@{TWD5\_\-REG}}
\index{TWD5\_\-REG@{TWD5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWD5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWD5\_\-REG~TWDR}\label{ATmega406_8h_338062c276f9cbd3169637b05af3194a}




Definition at line 199 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWD6\_\-REG@{TWD6\_\-REG}}
\index{TWD6\_\-REG@{TWD6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWD6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWD6\_\-REG~TWDR}\label{ATmega406_8h_d59dd12a1ce6f3c41ac0d42efc2fa9bd}




Definition at line 200 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWD7\_\-REG@{TWD7\_\-REG}}
\index{TWD7\_\-REG@{TWD7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWD7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWD7\_\-REG~TWDR}\label{ATmega406_8h_597822a314109606cf186c2c209cead7}




Definition at line 201 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWEA\_\-REG@{TWEA\_\-REG}}
\index{TWEA\_\-REG@{TWEA\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWEA\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWEA\_\-REG~TWCR}\label{ATmega406_8h_47bbd1562dc710e400f6821b92049c97}




Definition at line 512 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWEN\_\-REG@{TWEN\_\-REG}}
\index{TWEN\_\-REG@{TWEN\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWEN\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWEN\_\-REG~TWCR}\label{ATmega406_8h_32c9797ca7917c8a3ee36466c0fadb5e}




Definition at line 508 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWGCE\_\-REG@{TWGCE\_\-REG}}
\index{TWGCE\_\-REG@{TWGCE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWGCE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWGCE\_\-REG~TWAR}\label{ATmega406_8h_8aa44cc539b72201d371b113c7d071a6}




Definition at line 552 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWIE\_\-REG@{TWIE\_\-REG}}
\index{TWIE\_\-REG@{TWIE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWIE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWIE\_\-REG~TWCR}\label{ATmega406_8h_1f538b6acabd331860c94f40a1f04c35}




Definition at line 507 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWINT\_\-REG@{TWINT\_\-REG}}
\index{TWINT\_\-REG@{TWINT\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWINT\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWINT\_\-REG~TWCR}\label{ATmega406_8h_c735c510b13abfbcbf586ed0aff3d364}




Definition at line 513 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWPS0\_\-REG@{TWPS0\_\-REG}}
\index{TWPS0\_\-REG@{TWPS0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWPS0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWPS0\_\-REG~TWSR}\label{ATmega406_8h_31a045c22b12b87db286a6862d647d6c}




Definition at line 614 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWPS1\_\-REG@{TWPS1\_\-REG}}
\index{TWPS1\_\-REG@{TWPS1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWPS1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWPS1\_\-REG~TWSR}\label{ATmega406_8h_6bcc0a3bff4d75070d073b511c52a57d}




Definition at line 615 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWS3\_\-REG@{TWS3\_\-REG}}
\index{TWS3\_\-REG@{TWS3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWS3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWS3\_\-REG~TWSR}\label{ATmega406_8h_a80d04c0cfe488d895c325f69a02cc36}




Definition at line 616 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWS4\_\-REG@{TWS4\_\-REG}}
\index{TWS4\_\-REG@{TWS4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWS4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWS4\_\-REG~TWSR}\label{ATmega406_8h_99bd82dc5cc840f4824b7d2404162165}




Definition at line 617 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWS5\_\-REG@{TWS5\_\-REG}}
\index{TWS5\_\-REG@{TWS5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWS5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWS5\_\-REG~TWSR}\label{ATmega406_8h_704389eaf346061e30edcf4c1d47a159}




Definition at line 618 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWS6\_\-REG@{TWS6\_\-REG}}
\index{TWS6\_\-REG@{TWS6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWS6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWS6\_\-REG~TWSR}\label{ATmega406_8h_9bdbb9e6f024778a3aa11598452027ea}




Definition at line 619 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWS7\_\-REG@{TWS7\_\-REG}}
\index{TWS7\_\-REG@{TWS7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWS7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWS7\_\-REG~TWSR}\label{ATmega406_8h_8a099f9d306846be42e1327050fd0be9}




Definition at line 620 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWSTA\_\-REG@{TWSTA\_\-REG}}
\index{TWSTA\_\-REG@{TWSTA\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWSTA\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWSTA\_\-REG~TWCR}\label{ATmega406_8h_961fe987cb04a80696301d044f05b827}




Definition at line 511 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWSTO\_\-REG@{TWSTO\_\-REG}}
\index{TWSTO\_\-REG@{TWSTO\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWSTO\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWSTO\_\-REG~TWCR}\label{ATmega406_8h_38ebbdf5a0f71f8f236cc7eca67a24d7}




Definition at line 510 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!TWWC\_\-REG@{TWWC\_\-REG}}
\index{TWWC\_\-REG@{TWWC\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[TWWC\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define TWWC\_\-REG~TWCR}\label{ATmega406_8h_de51e6dabbe1024a0001775bfb3dd329}




Definition at line 509 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!V\_\-REG@{V\_\-REG}}
\index{V\_\-REG@{V\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[V\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define V\_\-REG~SREG}\label{ATmega406_8h_dc5c29a5cd7ad49dd65b3d5543d81264}




Definition at line 147 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADC0\_\-REG@{VADC0\_\-REG}}
\index{VADC0\_\-REG@{VADC0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADC0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADC0\_\-REG~VADCL}\label{ATmega406_8h_2eace9c669363857fbedd21b46739cad}




Definition at line 649 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADC0D\_\-REG@{VADC0D\_\-REG}}
\index{VADC0D\_\-REG@{VADC0D\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADC0D\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADC0D\_\-REG~DIDR0}\label{ATmega406_8h_49163349410f9dc4119c208e9bb8a813}




Definition at line 685 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADC10\_\-REG@{VADC10\_\-REG}}
\index{VADC10\_\-REG@{VADC10\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADC10\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADC10\_\-REG~VADCH}\label{ATmega406_8h_c58b1552151020f45bca9d45a23da6de}




Definition at line 625 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADC11\_\-REG@{VADC11\_\-REG}}
\index{VADC11\_\-REG@{VADC11\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADC11\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADC11\_\-REG~VADCH}\label{ATmega406_8h_3c724480635e7688a3301e15f4a91890}




Definition at line 626 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADC1\_\-REG@{VADC1\_\-REG}}
\index{VADC1\_\-REG@{VADC1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADC1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADC1\_\-REG~VADCL}\label{ATmega406_8h_b4a1f631bfcf4b906e4080d50bb5c2c0}




Definition at line 650 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADC1D\_\-REG@{VADC1D\_\-REG}}
\index{VADC1D\_\-REG@{VADC1D\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADC1D\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADC1D\_\-REG~DIDR0}\label{ATmega406_8h_278a74b7ccfddb82591da0eacf8893a7}




Definition at line 686 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADC2\_\-REG@{VADC2\_\-REG}}
\index{VADC2\_\-REG@{VADC2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADC2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADC2\_\-REG~VADCL}\label{ATmega406_8h_47517fa613676ecf7e4164e4aa8a9a3a}




Definition at line 651 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADC2D\_\-REG@{VADC2D\_\-REG}}
\index{VADC2D\_\-REG@{VADC2D\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADC2D\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADC2D\_\-REG~DIDR0}\label{ATmega406_8h_a7eda93ab8d0eea64ad641bca80f8821}




Definition at line 687 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADC3\_\-REG@{VADC3\_\-REG}}
\index{VADC3\_\-REG@{VADC3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADC3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADC3\_\-REG~VADCL}\label{ATmega406_8h_a1985c96dcae5adb8986949136463aa0}




Definition at line 652 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADC3D\_\-REG@{VADC3D\_\-REG}}
\index{VADC3D\_\-REG@{VADC3D\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADC3D\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADC3D\_\-REG~DIDR0}\label{ATmega406_8h_a60f10e807544a319d7023757b2bc7e4}




Definition at line 688 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADC4\_\-REG@{VADC4\_\-REG}}
\index{VADC4\_\-REG@{VADC4\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADC4\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADC4\_\-REG~VADCL}\label{ATmega406_8h_046932db035d88a84b98b85dae30da8b}




Definition at line 653 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADC5\_\-REG@{VADC5\_\-REG}}
\index{VADC5\_\-REG@{VADC5\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADC5\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADC5\_\-REG~VADCL}\label{ATmega406_8h_d8b92c8a71eb4af366433163895e5679}




Definition at line 654 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADC6\_\-REG@{VADC6\_\-REG}}
\index{VADC6\_\-REG@{VADC6\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADC6\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADC6\_\-REG~VADCL}\label{ATmega406_8h_4136851c0931791f78c2921eb0c7c2ae}




Definition at line 655 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADC7\_\-REG@{VADC7\_\-REG}}
\index{VADC7\_\-REG@{VADC7\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADC7\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADC7\_\-REG~VADCL}\label{ATmega406_8h_e7f3beccdc2eee2d9e19741a873f138e}




Definition at line 656 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADC8\_\-REG@{VADC8\_\-REG}}
\index{VADC8\_\-REG@{VADC8\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADC8\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADC8\_\-REG~VADCH}\label{ATmega406_8h_35619c2b988e0119f8fb27de9eb84a9f}




Definition at line 623 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADC9\_\-REG@{VADC9\_\-REG}}
\index{VADC9\_\-REG@{VADC9\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADC9\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADC9\_\-REG~VADCH}\label{ATmega406_8h_a3987514b86dc50786eb28ecc7917f81}




Definition at line 624 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADCCIE\_\-REG@{VADCCIE\_\-REG}}
\index{VADCCIE\_\-REG@{VADCCIE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADCCIE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADCCIE\_\-REG~VADCSR}\label{ATmega406_8h_3d615554bdfce49706ace5d209c2d9fd}




Definition at line 669 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADCCIF\_\-REG@{VADCCIF\_\-REG}}
\index{VADCCIF\_\-REG@{VADCCIF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADCCIF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADCCIF\_\-REG~VADCSR}\label{ATmega406_8h_369f3097aab9517f1bc3bc2fce0a2d4a}




Definition at line 670 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADEN\_\-REG@{VADEN\_\-REG}}
\index{VADEN\_\-REG@{VADEN\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADEN\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADEN\_\-REG~VADCSR}\label{ATmega406_8h_65a93fae37980e30e3fd5ae64af284b6}




Definition at line 672 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADMUX0\_\-REG@{VADMUX0\_\-REG}}
\index{VADMUX0\_\-REG@{VADMUX0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADMUX0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADMUX0\_\-REG~VADMUX}\label{ATmega406_8h_e5e0dd3c818bc3ff22fbf361c0070bb7}




Definition at line 608 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADMUX1\_\-REG@{VADMUX1\_\-REG}}
\index{VADMUX1\_\-REG@{VADMUX1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADMUX1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADMUX1\_\-REG~VADMUX}\label{ATmega406_8h_ff4f71a1520fa5bcb332e60a28f0b5c4}




Definition at line 609 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADMUX2\_\-REG@{VADMUX2\_\-REG}}
\index{VADMUX2\_\-REG@{VADMUX2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADMUX2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADMUX2\_\-REG~VADMUX}\label{ATmega406_8h_979ad0c6473a508042dc50a387d7cd35}




Definition at line 610 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADMUX3\_\-REG@{VADMUX3\_\-REG}}
\index{VADMUX3\_\-REG@{VADMUX3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADMUX3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADMUX3\_\-REG~VADMUX}\label{ATmega406_8h_f54da57328dd072b8014cd6f376adfb5}




Definition at line 611 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!VADSC\_\-REG@{VADSC\_\-REG}}
\index{VADSC\_\-REG@{VADSC\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[VADSC\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define VADSC\_\-REG~VADCSR}\label{ATmega406_8h_ef265fb5df35fc08a5c96fff56f5f7fc}




Definition at line 671 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WDCE\_\-REG@{WDCE\_\-REG}}
\index{WDCE\_\-REG@{WDCE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WDCE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WDCE\_\-REG~WDTCSR}\label{ATmega406_8h_09b8a372add8b4e03dd2d48af366873c}




Definition at line 178 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WDE\_\-REG@{WDE\_\-REG}}
\index{WDE\_\-REG@{WDE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WDE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WDE\_\-REG~WDTCSR}\label{ATmega406_8h_68a534a0c5a59a929e184874ac9ea541}




Definition at line 177 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WDIE\_\-REG@{WDIE\_\-REG}}
\index{WDIE\_\-REG@{WDIE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WDIE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WDIE\_\-REG~WDTCSR}\label{ATmega406_8h_5bb401bda2071e4416f81c2fa26a3d7d}




Definition at line 180 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WDIF\_\-REG@{WDIF\_\-REG}}
\index{WDIF\_\-REG@{WDIF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WDIF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WDIF\_\-REG~WDTCSR}\label{ATmega406_8h_ce95db9638b9dd95b4332e5a9eee338b}




Definition at line 181 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WDP0\_\-REG@{WDP0\_\-REG}}
\index{WDP0\_\-REG@{WDP0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WDP0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WDP0\_\-REG~WDTCSR}\label{ATmega406_8h_fccf8ccff2dddf330d1f5f8875fad1f6}




Definition at line 174 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WDP1\_\-REG@{WDP1\_\-REG}}
\index{WDP1\_\-REG@{WDP1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WDP1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WDP1\_\-REG~WDTCSR}\label{ATmega406_8h_79c1ffde21945ce60b0afaf033c9980a}




Definition at line 175 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WDP2\_\-REG@{WDP2\_\-REG}}
\index{WDP2\_\-REG@{WDP2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WDP2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WDP2\_\-REG~WDTCSR}\label{ATmega406_8h_b8152b6da120a011179dc54061670ac5}




Definition at line 176 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WDP3\_\-REG@{WDP3\_\-REG}}
\index{WDP3\_\-REG@{WDP3\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WDP3\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WDP3\_\-REG~WDTCSR}\label{ATmega406_8h_fd294c509a61d6df051e540ab7be192e}




Definition at line 179 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WDRF\_\-REG@{WDRF\_\-REG}}
\index{WDRF\_\-REG@{WDRF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WDRF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WDRF\_\-REG~MCUSR}\label{ATmega406_8h_8733752726a2bd869e92714e64e0714b}




Definition at line 391 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WGM00\_\-REG@{WGM00\_\-REG}}
\index{WGM00\_\-REG@{WGM00\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WGM00\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WGM00\_\-REG~TCCR0A}\label{ATmega406_8h_7d46975ec4154199bf50380121ce600e}




Definition at line 691 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WGM01\_\-REG@{WGM01\_\-REG}}
\index{WGM01\_\-REG@{WGM01\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WGM01\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WGM01\_\-REG~TCCR0A}\label{ATmega406_8h_67cab651d9a52a906ef4c4394b7599bf}




Definition at line 692 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WGM02\_\-REG@{WGM02\_\-REG}}
\index{WGM02\_\-REG@{WGM02\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WGM02\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WGM02\_\-REG~TCCR0B}\label{ATmega406_8h_14aec6e45f5112cedf2524c61386e08f}




Definition at line 594 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WUTCF\_\-REG@{WUTCF\_\-REG}}
\index{WUTCF\_\-REG@{WUTCF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WUTCF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WUTCF\_\-REG~WUTCSR}\label{ATmega406_8h_928be98ee9a1b55525f0f69fcd954a72}




Definition at line 139 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WUTE\_\-REG@{WUTE\_\-REG}}
\index{WUTE\_\-REG@{WUTE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WUTE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WUTE\_\-REG~WUTCSR}\label{ATmega406_8h_c422baacf32065cfb9882307a5d303f6}




Definition at line 137 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WUTIE\_\-REG@{WUTIE\_\-REG}}
\index{WUTIE\_\-REG@{WUTIE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WUTIE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WUTIE\_\-REG~WUTCSR}\label{ATmega406_8h_0a92a7affc80b01c307e403cb2080d96}




Definition at line 140 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WUTIF\_\-REG@{WUTIF\_\-REG}}
\index{WUTIF\_\-REG@{WUTIF\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WUTIF\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WUTIF\_\-REG~WUTCSR}\label{ATmega406_8h_56a2870a56dfd798705c3e0a89caff7b}




Definition at line 141 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WUTP0\_\-REG@{WUTP0\_\-REG}}
\index{WUTP0\_\-REG@{WUTP0\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WUTP0\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WUTP0\_\-REG~WUTCSR}\label{ATmega406_8h_850807a1697f3a8205cbbd4d8540a399}




Definition at line 134 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WUTP1\_\-REG@{WUTP1\_\-REG}}
\index{WUTP1\_\-REG@{WUTP1\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WUTP1\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WUTP1\_\-REG~WUTCSR}\label{ATmega406_8h_f1d5e82dae14e77783ccd4a66d033169}




Definition at line 135 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WUTP2\_\-REG@{WUTP2\_\-REG}}
\index{WUTP2\_\-REG@{WUTP2\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WUTP2\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WUTP2\_\-REG~WUTCSR}\label{ATmega406_8h_29179877138ad82f9afad795bd1cfb43}




Definition at line 136 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!WUTR\_\-REG@{WUTR\_\-REG}}
\index{WUTR\_\-REG@{WUTR\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[WUTR\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define WUTR\_\-REG~WUTCSR}\label{ATmega406_8h_e7ad3b4b9fcd24c9b515c688f8baae88}




Definition at line 138 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!XOE\_\-REG@{XOE\_\-REG}}
\index{XOE\_\-REG@{XOE\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[XOE\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define XOE\_\-REG~CCSR}\label{ATmega406_8h_d6ba715221a9ca0bd6cc04d589332d18}




Definition at line 309 of file ATmega406.h.\index{ATmega406.h@{ATmega406.h}!Z\_\-REG@{Z\_\-REG}}
\index{Z\_\-REG@{Z\_\-REG}!ATmega406.h@{ATmega406.h}}
\subsubsection[Z\_\-REG]{\setlength{\rightskip}{0pt plus 5cm}\#define Z\_\-REG~SREG}\label{ATmega406_8h_c14906b36c9bea67d3374e5015a1d0a2}




Definition at line 145 of file ATmega406.h.