\section{aversive\_\-10-03-12/modules/comm/uart/uart\_\-recv9.c File Reference}
\label{uart__recv9_8c}\index{aversive\_\-10-03-12/modules/comm/uart/uart\_\-recv9.c@{aversive\_\-10-03-12/modules/comm/uart/uart\_\-recv9.c}}
{\tt \#include $<$uart.h$>$}\par
{\tt \#include $<$uart\_\-defs.h$>$}\par
{\tt \#include $<$uart\_\-private.h$>$}\par
\subsection*{Functions}
\begin{CompactItemize}
\item 
int {\bf uart\_\-9bits\_\-recv} (uint8\_\-t num)
\end{CompactItemize}


\subsection{Function Documentation}
\index{uart\_\-recv9.c@{uart\_\-recv9.c}!uart\_\-9bits\_\-recv@{uart\_\-9bits\_\-recv}}
\index{uart\_\-9bits\_\-recv@{uart\_\-9bits\_\-recv}!uart_recv9.c@{uart\_\-recv9.c}}
\subsubsection[uart\_\-9bits\_\-recv]{\setlength{\rightskip}{0pt plus 5cm}int uart\_\-9bits\_\-recv (uint8\_\-t {\em num})}\label{uart__recv9_8c_e843402902d2797c2b107b22cb971730}


same than uart\_\-recv with 9 bits. 

Definition at line 29 of file uart\_\-recv9.c.

References parse\_\-doc::elt, and uart\_\-9bits\_\-recv\_\-nowait().